For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove instrument panel compartment. Refer to Instrument Panel Compartment Replacement.
2. Remove the instrument panel molding - passenger side. Refer to Instrument Panel Molding Replacement - Passenger Side.

1 | Instrument Panel Lower Extension Side Trim Panel Fastener (Qty: 3)
2 | Instrument Panel Lower Extension Side Trim Panel

#### Procedure

Grasp the trim panel assembly and pull rearward disengaging the retainer securing it to the instrument panel.