Compact Disc Inoperative. Opel Sintra 1999

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Is the CD player mute or skipping? | -- | Go to Step 3 | Go to Step 2
2 | Does the letter E followed by 2 numbers (E##) appear in the radio display? | -- | Go to Step 3 | Go to Step 5

3

1. Inspect the CD player for the following conditions:

• | The disc is inserted upside down.

• | The disc is scratched or dirty.

• | The disc is moist or wet.

• | The disc may be moist if a cold disc was inserted into a hot player, or vice versa.

• | The internal temperature of the IP is high.

• | A very high internal temperature may cause the disc to eject.

2. Wait for 1 hour in order to allow the moisture to evaporate.
3. Use a known good disc in order to test the operation of the CD player.

Is the CD player operating correctly?

--

System OK

Go to Step 4

4

• | Verify that the disc is inserted correctly.

• | Clean any dirt or fingerprints from the disc.

| Allow one hour for condensation to evaporate.

• | Duplicate the road operating conditions with a known good disc (skipping may be normal on rough or dirt roads).

• | Attempt to duplicate other conditions with a known good disc. Some discs may contain marks that are not visible.

Is the CD player operating correctly?

--

System OK

Go to Step 5

5 | Service the CD player. Refer to Compact Disc Care and Cleaning . Is the symptom still present? | -- | -- | System OK