Entertainment Connector End Views. Opel Sintra 1999

For 1990-2009 cars

#### Auxiliary Video Module (AVM) C1

Connector Part Information

• | 12064769

• | 10-Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10-Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 40 | Power Input | A | ORN | 40 | Power Input
B | DK GRN | 145 | Radio On Signal Input | B | DK GRN | 145 | Radio On Signal Input
C | WHT | 199 | Video Audio Input, LH (+) | C | WHT | 199 | Video Audio Input, LH (+)
D | YEL | 116 | Video Audio Input, LH (-) | D | YEL | 116 | Video Audio Input, LH (-)
E | -- | -- | Not Used | E | -- | -- | Not Used
F | LT BLU | 115 | Video Audio Input, RH (-) | F | LT BLU | 115 | Video Audio Input, RH (-)
G | BLU | 46 | Video Audio Input, RH (+) | G | BLU | 46 | Video Audio Input, RH (+)
H | BRN | -- | Video Signal Input (-) | H | BRN | -- | Video Signal Input (-)
J | GRY | -- | Video Signal Input (+) | J | GRY | -- | Video Signal Input (+)
K | BLK | 150 | Ground | K | BLK | 150 | Ground

#### Auxiliary Video Module (AVM) C1 (second design)

Connector Part Information

• | 12064769

• | 10-Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10-Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GRY | -- | Video Signal Input (+) | A | GRY | -- | Video Signal Input (+)
B | BRN | -- | Video Signal Input (-) | B | BRN | -- | Video Signal Input (-)
C | BLK | -- | Ground | C | BLK | -- | Ground
D | ORN | -- | Power Input | D | ORN | -- | Power Input
E | DK GRN | -- | Not Used | E | DK GRN | -- | Not Used
F | RED/BLK | -- | Video Screen Power Ground | F | RED/BLK | -- | Video Screen Power Ground
G | RED/WHT | -- | Video Screen Backlight Power | G | RED/WHT | -- | Video Screen Backlight Power
H | PNK | -- | Ignition Power | H | PNK | -- | Ignition Power
J | DK BLU | -- | Video Audio Input, RH | J | DK BLU | -- | Video Audio Input, RH
K | WHT | -- | Video Audio Input, LH | K | WHT | -- | Video Audio Input, LH

#### Auxiliary Video Module (AVM) C2

Connector Part Information

• | 12064762

• | 6-Way F Metri-Pack 150 Series (GRY)

Connector Part Information

• | 12064763

• | 6-Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | -- | Video Signal Output (-) | A | WHT | -- | Video Signal Output (-)
B | BLK | 150 | Ground | B | BLK | 150 | Ground
C | ORN | 40 | Screen Position Input | C | ORN | 40 | Screen Position Input
D | RED | 40 | Ignition Power | D | RED | 40 | Ignition Power
E | PPL | 40 | Screen Power Feed (Output) | E | PPL | 40 | Screen Power Feed (Output)
F | YEL | -- | Video Signal Output (+) | F | YEL | 150 | Video Signal Output (+)

#### Auxiliary Video Module (AVM) C2 (second design)

Connector Part Information

• | 12064871

• | 10-Way F Metri-Pack 150 Series (BLU)

Connector Part Information

• | 12064872

• | 10-Way M Metri-Pack 150 Series (BLU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | -- | Video Signal Output (+) | A | YEL | -- | Video Signal Output (+)
B | WHT | -- | Video Signal Output (-) | B | WHT | -- | Video Signal Output (-)
C | WHT/BLK | -- | Video Signal Shield | C | WHT/BLK | -- | Video Signal Child
D | BLK | -- | Video Screen Power Ground | D | BLK | -- | Video Screen Power Ground
E | PPL | -- | Video Screen Power Feed | E | PPL | -- | Video Screen Power Feed
F | RED/WHT | -- | Video Screen Backlight Power | F | RED/WHT | -- | Video Screen Backlight Power
G | RED/BLK | -- | Video Screen Backlight Ground | G | RED/BLK | -- | Video Screen Backlight Ground
H | RED | -- | Ignition Power | H | RED c | -- | Ignition Power
J | ORN | -- | Screen Position Output | J | ORN | -- | Screen Position Output
K | -- | -- | Not Used | K | -- | -- | Not Used

#### Auxiliary Video Module (AVM) C3

Connector Part Information

• | 12064760

• | 4-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12064761

• | 4-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 40 | Power Output | A | ORN | 40 | Power Output
B | BLK | 150 | Ground | B | BLK | 150 | Ground
C | GRY | 8 | Interior Lights Dimming Input | C | GRY | 8 | Interior Lights Dimming Input
D | LT GRN | 145 | Radio On Signal Output | D | DK GRN | 145 | Radio On Signal Output

#### Auxiliary Video Module (AVM) C4

Connector Part Information

• | 12064766

• | 8-Way F Metri-Pack 150 Series (BLU)

Connector Part Information

• | 12064767

• | 8-Way M Metri-Pack 150 Series (BLU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT BLU | 115 | Speaker Output (Video), RH (-) | A | LT BLU | 115 | Speaker Output (Video), RH (-)
B | DK BLU | 46 | Speaker Output (Video), RH (+) | B | DK BLU | 46 | Speaker Output (Video), RH (+)
C | YEL | 116 | Speaker Output (Video), LH (-) | C | YEL | 116 | Speaker Output (Video), LH (-)
D | BRN | 199 | Speaker Output (Video), LH (+) | D | BRN | 199 | Speaker Output (Video), LH (+)
E | PPL | 46 | Video Audio Channel Output, LH (+) | E | PPL | 46 | Video Audio Channel Output, LH (+)
F | GRN | 115/116 | Video Audio Channel Output (-) | F | GRN | 115/116 | Video Audio Channel Output (-)
G | WHT | 199 | Video Audio Channel Output, RH (+) | G | WHT | 199 | Video Audio Channel Output, RH (+)
H | BLK | 150 | Interior Lights Dimming Ground | H | WHT/BLK | 150 | Interior Lights Dimming Ground

#### Interface Module (IM)

Connector Part Information

• | 12110259

• | 16-Way F Micro-Pack 100 Series (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | LT BLU | 115 | Radio Audio Input (RH -)
A2 | DK BLU | 46 | Radio Audio Input (RH +)
A3 | YEL | 116 | Radio Audio Input (LH -)
A4 | BRN | 199 | Radio Audio Input (LH +)
A5 | LT GRN | 1011 | Rear Seat Audio System On Signal
A6 | GRY | 8 | Interior Lights Dimming Feed (Input)
A7 | -- | -- | Not Used
A8 | YEL | 43 | Ignition Power Input
B1 | LT BLU | 115 | RH Radio Rear Speaker Return (-)
B2 | DK BLU | 46 | RH Radio Rear Speaker Feed (+)
B3 | YEL | 116 | LH Radio Rear Speaker Return (-)
B4 | BRN | 199 | LH Radio Rear Speaker Feed (+)
B5 | BLK | 906 | Rear Seat Audio (RSA) Enabled Signal
B6 | BLK/WHT | 351 | Ground
B7 | -- | -- | Not Used
B8 | GRY/BLK | 308 | Pulsed Width Modulation (PWM) Input

#### Radio Rear Seat Audio Control

Connector Part Information

• | 12110259

• | 16-Way F Micro-Pack 100 Series (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | LT BLU | 115 | Speaker return-right rear
A2 | DK BLU | 46 | Speaker feed-right rear
A3 | YEL | 116 | Speaker return-left rear
A4 | BRN | 199 | Speaker feed-left rear
A5 | LT GRN | 1011 | RSA enable out
A6 | GRY | 8 | Interior lamp dim signal
A7 | -- | -- | Not Used
A8 | YEL | 43 | Fused accessory feed
B1 | LT BLU | 115 | Speaker return-right rear
B2 | DK BLU | 46 | Speaker feed-right rear
B3 | YEL | 116 | Speaker return-left rear
B4 | BRN | 199 | Speaker feed-left rear
B5 | BLK | 906 | RSA enable in
B6 | BLK/WHT | 351 | Ground-clean
B7 | -- | -- | Not Used
B8 | GRY/BLK | 308 | Park lamp switch output-park lamps ON

#### Second Seat Audio (SSA) Control

Connector Part Information

• | 12064799

• | 12-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Interior Lights Dimming Feed (Input)
B | LT BLU | 115 | Radio Audio Input, RH (-)
C | DK BLU | 46 | Radio Audio Input, RH (+)
D | YEL | 116 | Radio Audio Input, LH (+)
E | BRN | 199 | Radio Audio Input, LH (-)
F | PPL | 115 | Video Audio Input, RH (-)
G | ORN | 46 | Video Audio Input, RH (+)
H | GRN | 116 | Video Audio Input, LH (-)
J | WHT | 199 | Video Audio Input, LH (+)
K | BLK | 150 | Ground
L | BLK/WHT | 906 | Rear Seat Audio (RSA) Enabled Input
M | WHT/RED | 150 | Interior Lights Dimming Ground

#### Tape Retract Module (TRM)

Connector Part Information

• | 12047785

• | 4-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 40 | B+ Feed
B | BLK | 150 | Ground
C | ORN | 40 | Ignition Feed
D | ORN | 40 | B+ Output (Switched)

#### Tape Retract Module (TRM) (second design)

Connector Part Information

• | 12084944

• | 16-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | ORN | -- | Battery (+)
A2 | PNK | -- | Ignition Feed
A3 | -- | -- | Not Used
A4 | -- | -- | Not Used
A5 | ORN | -- | VCP Power Feed
A6 | ORN | -- | AVM Power Input
A7 | GRY | -- | Video Signal (+)
A8 | BRN | -- | Video Signal (-)
B1 | BLK | -- | Ground
B2 | PNK | -- | Ignition Feed
B3 | -- | -- | Not Used
B4 | -- | -- | Not Used
B5 | RED/WHT | -- | Video Screen Backlight Power
B6 | BLK | -- | Power Ground
B7 | GRY | -- | Video Shield
B8 |  | -- | Video Shield

#### Third Seat Audio (TSA) Control

Connector Part Information

• | 12064799

• | 12-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 8 | Interior Lights Dimming Feed (Input)
B | LT BLU | 115 | Radio Audio Input, RH (-)
C | BLU | 46 | Radio Audio Input, RH (+)
D | YEL | 116 | Radio Audio Input, LH (+)
E | BRN | 199 | Radio Audio Input, LH (-)
F | PPL | 115 | Video Audio Input, RH (-)
G | ORN | 46 | Video Audio Input, RH (+)
H | GRN | 116 | Video Audio Input, LH (-)
J | WHT | 199 | Video Audio Input, LH (+)
K | BLK | 150 | Ground
L | BLK/WHT | 906 | Rear Seat Audio (RSA) Enabled Input
M | GRY | 150 | Interior Lights Dimming Ground

#### Video Entertainment System (VES) Relay (if equipped)

Connector Part Information

• | 12129715

• | 6-Way F Metri-Pack 280 Series Flexlock (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | BLK | 150 | Ground
A2 | ORN | 40 | B+ Feed
B1-B2 | -- | -- | Not Used
C1 | ORN | 40 | B+ Feed (Relay Switched)
C2 | PNK/BLK | 39 | Ignition Feed

#### In-line Connector C326

Connector Part Information

• | 12047785

• | 4-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047786

• | 4-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 8 | Interior Lights Dimming Feed | A | ORN | 8 | Interior Lights Dimming Feed
B | BLK | 150 | Ground | B | BLK | 150 | Ground
C | GRY | 150 | Interior Lights Dimming Ground | C | GRY | 150 | Interior Lights Dimming Ground
D | BLK/WHT | 906 | Rear Seat Audio (RSA) Enabled Signal | D | BLK/WHT | 906 | Rear Seat Audio (RSA) Enabled Signal

#### In-line Connector C328

Connector Part Information

• | 12047886

• | 8-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12045688

• | 8-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT BLU | 115 | Video Audio Feed, RH (-) | A | LT BLU | 115 | Video Audio Feed, RH (-)
B | BLU | 46 | Radio Audio Feed, RH (+) | B | BLU | 46 | Radio Audio Feed, RH (+)
C | YEL | 116 | Radio Audio Feed, LH (+) | C | YEL | 116 | Radio Audio Feed, LH (+)
D | BRN | 199 | Radio Audio Feed, LH (-) | D | BRN | 199 | Radio Audio Feed, LH (-)
E | PPL | 115 | Video Audio Feed, RH (-) | E | PPL | 115 | Video Audio Feed, RH (-)
F | ORN | 46 | Radio Audio Feed, RH (+) | F | ORN | 46 | Radio Audio Feed, RH (+)
G | GRN | 116 | Radio Audio Feed, LH (+) | G | GRN | 116 | Radio Audio Feed, LH (+)
H | WHT | 199 | Radio Audio Feed, LH (-) | H | WHT | 199 | Radio Audio Feed, LH (-)

#### LH Radio Speaker

Connector Part Information

• | 12052832

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 118 | Speaker feed-LF
B | TAN | 201 | Speaker return-LF

#### LH Radio Liftgate Speaker

Connector Part Information

• | 12052832

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---

A

YEL

116

• | LR liftgate speaker feed

• | (UK6) LR liftgate feed to radio rear speaker amplifier

B

BRN

199

• | LR liftgate speaker return

• | (UK6) LR liftgate return to radio rear speaker amplifier

#### Remote CD Changer

Connector Part Information

• | 12064980

• | 9-Way F Mircro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
7 | PNK | 314 | R14 In
8 | BRN/WHT | 230 | Interior lamp dim signal
9 | Bare | 2011 | Dim
10 | DK GRN/WHT | 368 | RH output
11 | BRN/WHT | 367 | LH output
12 | BLK/WHT | 372 | Audio signal return
13 | BLK/WHT | 351 | Power ground
14 | DK GRN | 835 | Entertainment and Comfort (E&C) serial data communication
15 | ORN | 640 | Fused battery feed

#### Radio C1

Connector Part Information

• | 12047531

• | 10-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY | 118 | Speaker return-LF
2 | TAN | 201 | Speaker feed-LF
3 | DK GRN | 117 | Speaker return-RF
4 | LT GRN | 200 | Speaker feed-RF
5 | BLK/WHT | 351 | Ground
6 | GRY/BLK | 308 | Park lamp switch signal-park lamps ON
7 | BRN/WHT | 230 | Radio dimmer feed
8 | DK GRN | 145 | Radio ON Signal
9 | YEL | 43 | Fused power feed
10 | ORN | 640 | Fused battery feed

#### Radio C2

Connector Part Information

• | 12065785

• | 10-Way F Micro-Pack 100 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
11 | -- | -- | Not Used
12 | BLK | 906 | RSA enable out
13 | LT GRN | 1011 | RSA In
14 | DK BLU | 1796 | Steering wheel controls input (Pontiac/Oldsmobile)
15 | DK GRN | 835 | Data link
16 | DK GRN | 389 | Vehicle speed sensor (VSS) (Chevrolet/Oldsmobile)

17

LT BLU

115

• | RR liftgate speaker return

• | (UK6) RR liftgate return to radio rear speaker amplifier

18

DK BLU

46

• | RR liftgate speaker feed

• | (UK6) RR liftgate feed to radio rear speaker amplifier

19

YEL

116

• | LR liftgate speaker return

• | (UK6) LR liftgate return to radio rear speaker amplifier

20

BRN

199

• | LR liftgate speaker feed

• | (UK6) LR liftgate feed to radio rear speaker amplifier

#### Radio C3

Connector Part Information

• | 12064980

• | 9-Way F Mirco-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
7 | PNK | 314 | R14 out
8 | BRN/WHT | 230 | Interior lamp dim signal
9 | -- | -- | Not Used
10 | DK GRN/WHT | 368 | RH input
11 | BRN/WHT | 367 | LH input
12 | BLK/WHT | 372 | Audio signal return
13 | BLK/WHT | 351 | Power ground
14 | DK GRN | 835 | Entertainment and Comfort (E&C) serial data communication
15 | ORN | 640 | Fused battery feed out

#### RH Radio Liftgate Speaker

Connector Part Information

• | 12052832

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---

A

LT BLU

115

• | RR liftgate speaker feed

• | (UK6) RR liftgate feed to radio rear speaker amplifier

B

DK BLU

46

• | RR liftgate speaker return

• | (UK6) RR liftgate return to radio rear speaker amplifier

#### RH Radio Speaker

Connector Part Information

• | 12052832

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK GRN | 117 | Speaker feed-RF
B | LT GRN | 200 | Speaker return-RF