Knock Sensor Module. Opel Sintra 1997

For 1990-2009 cars

### Removal Procedure

1. Remove the PCM. Refer to Powertrain Control Module and Sensors for procedure.
2. Remove the KS Module cover.
3. Carefully squeeze the latches on KS Module.

Carefully remove KS Module.

### Installation Procedure

1. Carefully insert KS module into socket. Carefully press down on KS Module until latches catch.
2. Install the KS Module cover.
3. Install the PCM. Refer to Powertrain Control Module and Sensors for procedure.