Cruise Control Does Not Disengage with Brake Pedal. Opel Sintra 1999

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire cruise control system check performed? | -- | Go to Step 2 | Go to Cruise Control System Check

2

1. Disconnect the cruise control module connector.
2. Connect a test light from cruise control module connector terminal G to ground.
3. Depress the brake pedal.

Does the test light illuminate?

--

Go to Step 3

Go to Step 4

3

1. Check for a poor connection at the cruise control module terminal C.
2. If the connection is OK, replace the cruise control module. Refer to Multifunction, Turn Signal, and Hazard Switch Replacement - On Vehicle in Steering Wheel and Column - Tilt.

Is the repair complete?

--

Go to Step 5

--

4 | Repair the open in circuit 17 between S205 and the cruise control module connector terminal G. Is the repair complete? | -- | Go to Step 5 | --

5

1. Turn the ignition switch to the OFF position.
2. Reconnect all connectors components removed.

Have all the repairs been made?

--

Go to Cruise Control System Check

--