Fog Lights System Check. Opel Sintra 1999

For 1990-2009 cars

## Fog Lights System Check Front

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---

1

1. Turn the headlamp switch to the HEAD position on the headlamp/instrument panel (IP) dimmer switch.
2. Turn the headlamp dimmer switch to the LOW position.
3. Turn the fog lamp switch to the ON position.

• | Both lamps are on.

• | The fog lamp switch indicator is on.

• | Refer to Fog Lamps Inoperative - All

• | Refer to Fog Lamps Inoperative - One

• | Refer to Fog Lamp Indicator Inoperative

2 | Turn the headlamp dimmer switch to the HIGH position. | The fog lamps are off. | Refer to Fog Lamps Always On
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.

## Fog Lights System Check Rear -(Export)

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---

1

1. Turn the headlamp switch to the HEAD position on the headlamp and IP lamp dimmer switch.
2. Press the rear fog lamp switch.

• | The rear fog lamps are on.

• | The rear fog lamp switch indicator is on.

Refer to Rear Fog Lamps Inoperative

2 | Press the rear fog lamp switch. | The rear fog lamps are off. | Refer to Rear Fog Lamps Always On
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.