SERVICE MANUAL UPDATE SEC. 125C TRANS. DIAGNOSIS. Pontiac 6000 1989

For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 125C TRANS. DIAGNOSIS

#### Models Affected: 1989 6000, SUNBIRD AND GRAND AM MODELS

The 3rd clutch switch is incorrectly identified as normally open in Figure 39 in Section THM 125C Transaxle Diagnosis of the 1989 6000, Sunbird and Grand Am Service Manuals. The switch is identified correctly in the following illustration.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.