WEATHER PAK WIRE CONNECTOR SERVICE INFORMATION. Pontiac 6000 1983

For 1990-2009 cars

# WEATHER PAK WIRE CONNECTOR SERVICE INFORMATION

THERE HAVE BEEN SOME INQUIRIES CONCERNING THE WEATHER-PAK CONNECTOR REPAIRS AND REPLACEMENT PARTS. THE 1981 CHASSIS SERVICE MANUAL PROVIDES DETAILED REPAIR PROCEDURES IN SECTION 8A1 PAGE 12 AND 13. REPLACEMENT PARTS ARE LISTED SEPARATELY IN THE GMWDD STANDARD PARTS CATALOG IN GROUP 8.965 PAGE 134-135-153. PART NUMBERS OF HOUSINGS AND WIRE TERMINALS ARE AS FOLLOWS. HOUSINGS AND TERMINAL CONNECTORS ARE NOT SUPPLIED IN KIT FORM AND MUST BE PURCHASED SEPARATELY. THE WIRE CRIMPING TOOLS TO SERVICE THESE CONNECTORS ARE DIFFERENT FROM PAST MODEL TOOLS. HOUSING 1 WIRE FEMALE CONNECTOR 12014849 MALE CONNECTOR 12014848 HOUSING 2 WIRE FEMALE CONNECTOR 12014838 MALE CONNECTOR 12014839 HOUSING 3 WIRE FEMALE CONNECTOR 12019653 MALE CONNECTOR 12019656 HOUSING 6 WIRE FEMALE CONNECTOR 12014840 MALE CONNECTOR 12014841 HOUSING WIRE TERMINAL HOUSING SINGLE CONNECTOR FEMALE CONNECTOR 12014837 MALE CONNECTOR 12014836

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.