ELECT. CLU. BEZEL & RET.SQUEAK DEFECTIVE BEZEL & RET. UNIT. Pontiac 6000 1984

For 1990-2009 cars

# ELECT. CLU. BEZEL & RET.SQUEAK DEFECTIVE BEZEL & RET. UNIT

A condition of bezel squeak may be encountered on some 1984 STE vehicles. To correct this condition, a new bezel and retainer unit is available.

Part Number Retainer Unit ----------- ------------- 10036912 Bezel Unit 10036913 Retainer Unit

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.