AM BAND RADIO NOISE MISSING GROUND WIRE. Pontiac Fiero 1985

For 1990-2009 cars

# AM BAND RADIO NOISE MISSING GROUND WIRE

#### VEHICLES AFFECTED: 1985 Fiero

#### CONDITION:

---------- Some early built 1985 Fiero vehicles may experience an AM Band Radio ignition noise.

#### CAUSE:

----- The noise condition may be the result of a missing radio noise suppression ground wire.

#### CORRECTION:

---------- To repair the noise condition, install a noise suppression ground wire, using no. 16 gauge wire with 3/8 inch ring terminals (See Attached Illustration For Installation).

#### NOTICE: All Fiero vehicles built after V.I.N. 202644 have the correct parts.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.