REAR COMPARTMENT TORQUE ROD- REPLACEMENT/ MANUAL REVISION. Pontiac Fiero 1986

For 1990-2009 cars

# REAR COMPARTMENT TORQUE ROD- REPLACEMENT/ MANUAL REVISION

SERVICE MANUAL REVISION

#### VEHICLES AFFECTED 1984-88 FIEROS ----------------- The service procedure for removing and replacing rear compartment torque rods on 1984-88 Fieros has been revised from what is shown in section 7 (Body Portion) of the Service Manual.

The following service procedure is the revised version and should be used as reference when torque rod removal is necessary.

#### Procedure

Remove or disconnect (Figure 1, 2, 3, 4, 5)

1. Deck lid (6)

2. Motor compartment side quarter grille panel (not shown)

3. Screw (2), use tool J-35808 or equivalent

4. Hinge (4)

5. Loosen heat shield, air conditioning hose and bracket, if present.

6. Pin (9) with end of torque rod resting against plywood, grasp U end of rod (8) and pull rearward to release pin.

7. Torque rod from hook (8)

8. Torque rod (3)

#### Install or Connect

1. Torque rod (3)

2. Torque rod to hook

3. Pin (9) o With torque rod resting against plywood, grasp U end of rod (8) and pull rearward to insert pin. o Release U end (8) of rod making sure that end of rod hooks are over pin.

4. Air conditioning hose and bracket, heat shield

5. Hinge (4)

6. Screw (2)

7. Motor compartment side quarter grille panel

8. Deck lid (6)

Use applicable labor operation and time as shown in the Labor Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.