DISTRIBUTOR 'O' RING INCLUDED WITH ALL CAMPAIGN ENGINE. Pontiac Fiero 1984

For 1990-2009 cars

# DISTRIBUTOR 'O' RING INCLUDED WITH ALL CAMPAIGN ENGINE

BEGINNING APRIL 21, 1988 REPLACEMENT CAMPAIGN ENGINE KITS SHIPPED FROM THE PLANT WILL INCLUDE A NEW RUBBER O-RING, P/N 1979784, FOR THE DISTRIBUTOR.

REMOVE AND DISCARD THE OLD O-RING AND INSTALL THE NEW O-RING ONTO THE DISTRIBUTOR. COAT THE NEW O-RING WITH CLEAN ENGINE OIL PRIOR TO INSTALLING THE DISTRIBUTOR INTO THE ENGINE.

FIGURES: 1

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.

COPYRIGHT 1988 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.