For 1990-2009 cars

# Info - 4L60-E Valve Body, Spacer Plate and Gasket Kit (Ordering Reference Table)

Subject: | 4L60-E Valve Body, Spacer Plate and Gasket Kit (Ordering Reference Table)

Models: | 1998-2001 Chevrolet Camaro, Corvette

| 1998-2001 Pontiac Firebird

| 1999-2001 Chevrolet and GMC C/K Trucks

| with 4L60-E Automatic Transmission (RPOs M30, M32)

To assist in ordering the new Valve Body, Spacer Plate, and Gasket Kit, the following table can be used for reference:

Model Year** | Vehicle Platform | Engine (RPO) | Transmission Family (RPO) | Transmission Broadcast Code | Reman Valve Body-Spacer Plate-Gaskets Service Package
--- | --- | --- | --- | --- | ---
1999-2001i | C/K Truck | 4.8 L (LR4) | 4L60-E (M30) | CCD, CFD, CHD, CJD, KBD, KCD | 24221162
1999-2001i | C/K Truck | 5.3 L (LM7) | 4L60-E (M30) | CCD, CFD, CHD, CJD, KBD, KCD | 24221162
1998-2001i | F Car | 5.7 L (LS1) | 4L60-E (M30) | FFD | 24221158
1998-2001i | Y Car | 5.7 L (LS1) | 4L60-E (M30) | YDD | 24221158
NOTE: ** = Reman Valve Body-Spacer Plate-Gaskets Service Package Releases To Service Only 1998, 1999, 2000, and 2001i (Through Julian Date 01-031/1-31-01) 4L60-E Transmissions. All transmissions built after Julian Date 01-031 (January 31, 2001) can be serviced with individual components. Refer to the GMSPO catalog for the correct part numbers.

Parts are currently available from GMSPO.