For 1990-2009 cars

Table 1: | Fuse Block Application Table
Table 2: | Underhood Electrical Center 1 MaxiFuse® Application
Table 3: | Underhood Electrical Center 1 MiniFuse® Application
Table 4: | Underhood Electrical Center 2 MaxiFuse® Application Table
Table 5: | Underhood Electrical Center 2 MiniFuse® Application Table

### IP Fuse Block

#### Fuse Block Application Table

Fuse | Rating | Description
--- | --- | ---
1 - STOP HAZARD | 20A |

• | Hazard lamp flasher

• | Stop lamp switch

2 - TURN B/U | 20A |

• | Backup lamp switch

• | Daytime running lamps (DRL) module

• | Park/neutral position switch

• | Second gear start switch

• | Traction control switch

• | Turn signal lamp flasher

3 - RADIO | 1A | Steering wheel controls
4 - RADIO ACCY | 25A |

• | Amplifier

• | Radio power antenna

• | Remote compact disc player

5 - TAIL LPS | 20A |

• | Daytime running lamps (DRL) module

• | Headlamp switch

6 - HVAC | 20A | HVAC control
7 - PWR ACCY | 15A |

• | Instrument cluster

• | Outside rearview mirror switch

• | Radio

• | Rear compartment lid release relay

• | Theft deterrent relay

• | Theft deterrent shock sensor

8 - COURTESY | 20A | Body control module (BCM)
9 - GAUGES | 10A |

• | Body control module (BCM),

• | Daytime running lamps (DRL) module

• | Instrument cluster

• | Stop lamp switch

10 - AIR BAG | 15A | Inflatable restraint sensing and diagnostic module (SDM)
11 - CIG ACCY | 25A |

• | Auxiliary power outlet

• | Cigar lighter

• | Data link connector (DLC)

12 - DEFOG/SEATS | 30A |

• | Driver seat assembly

• | HVAC control

• | Passenger seat assembly

13 - RADIO | 1A | Steering wheel control
14 - WIPER/WASH | 25A |

• | Windshield wiper motor

• | Wiper/washer switch

15 - WINDOWS | 30A |

• | Folding top relay (with ETA)

• | Folding top switch

• | Power window control module

• | Rear Fog Lamp Relay (Export)

• | Side window switches

16 - IP DIMMER | 5A |

• | Ashtray lamp

• | Door illumination lamps

• | Electronic traction control switch

• | Fog lamp switch

• | Folding top switch

• | Headlamp switch

• | HVAC control

• | Instrument cluster

• | PRNDL illumination lamp

• | Radio

• | Rear fog lamp switch (Export)

• | Second gear start switch

17 - RADIO | 15A |

• | Body control module (BCM)

• | Radio

• | STG WHL CNTRL Fuse 3

### Underhood Electrical Center 1

#### Underhood Electrical Center 1 MaxiFuse® Application

Fuse | Rating | Description
--- | --- | ---
ABS BAT 1 | 40A | Electronic brake control module (EBCM)
ABS BAT 2 | 50A |

• | ABS BAT MiniFuse®

• | TCS BAT MiniFuse®

COOL FAN | 40A |

• | COOL FAN relay 1

• | COOL FAN relay 2

• | COOL FAN relay 3

• | COOL FAN MiniFuse®

H/L DOOR HORN | 50A |

• | HORN MiniFuse®

• | LH HDLP DR MiniFuse®

• | RH HDLP DR MiniFuse®

#### Underhood Electrical Center 1 MiniFuse® Application

Fuse | Rating | Description
--- | --- | ---
ABS BAT SOL | 25A | Electronic brake control module (EBCM)
AIR PUMP | 25A |

• | AIR pump relay

• | AIR pump solenoid

COOL FAN | 10A |

• | COOL FAN relay 1

• | COOL FAN relay 2

• | COOL FAN relay 3

FUEL PUMP | 20A | Fuel pump relay
HORN | 20A | Horn relay
LH HDLP DR | 15A | Headlamp opening door actuator control module
PCM BAT | 10A | Powertrain control module (PCM)
RH HDLP DR | 15A | Headlamp opening door actuator control module
TCS BAT | 20A |

• | Accelerator and servo control module

• | Throttle actuator control (TAC) module

### Underhood Electrical Center 2

#### Underhood Electrical Center 2 MaxiFuse® Application Table

Fuse/Circuit Breaker | Rating | Description
--- | --- | ---
ENG CTRL | 50A |

• | AIR PUMP MiniFuse®

• | FUEL PUMP MiniFuse®

• | PCM BAT MiniFuse®

IGN | 50A |

• | Ignition relay

• | Ignition switch

• | Starter relay

IP-1 | 40A | Blower motor relay
IP-2 | 40A |

• | STOP/HAZARD MiniFuse®

• | TAIL LPS MiniFuse®

#### Underhood Electrical Center 2 MiniFuse® Application Table

Fuse/Circuit Breaker | Rating | Description
--- | --- | ---
ABS IGN | 10A |

• | Electronic brake control module (EBCM)

• | Accelerator and servo control module

A/C CRUISE | 15A |

• | A/C compressor relay

• | Cruise control clutch switch

• | Cruise control module

• | Cruise control release (brake) switch

• | Cruise control switches (multi-function lever)

ENG CTRL | 15A |

• | Automatic transmission

• | (V6 VIN K) Electronic ignition control module

• | Evaporative emission (EVAP) canister purge solenoid valve

• | Evaporative emission (EVAP) canister vent solenoid valve

ENG SEN | 20A |

• | Heated oxygen sensors

• | Manual transmission

• | Mass air flow (MAF) sensor

• | Stop lamp switch

INJ 1 | 15A |

• | (V6 VIN K) Fuel injectors

• | (V8 VIN G) Bank 1 fuel injectors

• | (V8 VIN G) Ignition control module, LH

INJ 2 | 15A |

• | (V8 VIN G) Bank 2 Fuel injectors

• | (V8 VIN G) Ignition control module, RH

PCM IGN | 15A | Powertrain control module (PCM)
STRTR | 15A |

• | Clutch pedal position (CPP) switch

• | Park/neutral position switch

• | Instrument cluster

• | Powertrain control module (PCM)