For 1990-2009 cars

# QUIET TURN SIGNAL FLASHERS HIGHER NOISE LEVEL FLASHER P/N

#### VEHICLES AFFECTED: All Models

If comments are received regarding quiet turn signal flashers, the following check can be made:

Make sure the flasher is securely mounted in the correct location. This will ensure that the sound generated by the flasher will resonate into the passenger compartment. If the above procedure does not produce desired results, a higher noise level flasher, part number 10041073 available through GM Parts Department, can be installed.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.