For 1990-2009 cars

#### Engine Component View (Left Side)

(1) | Ignition Control Module (ICM) and Coils Assembly
(2) | Bank 1 Heated Oxygen Sensor 1
(3) | Crankshaft Position (CKP) Sensor
(4) | Exhaust Gas Recirculation (EGR) Valve
(5) | Mass Air Flow (MAF) Sensor
(6) | Manifold Absolute Pressure (MAP) Sensor

#### Engine Component View (Right Side)

(1) | Idle Air Control (IAC) Valve
(2) | Mass Air Flow (MAF) Sensor
(3) | Engine Coolant Temperature (ECT) Sensor
(4) | Throttle Position (TP) Sensor
(5) | Camshaft Position (CMP) Sensor
(6) | Fuel Injectors
(7) | Bank 2 Heated Oxygen Sensor 1
(8) | Manifold Absolute Pressure (MAP) Sensor
(9) | Fuel Pressure Regulator

Name | Location | Locator View (8A Cell 201 Page #) | Figure | Connector Eng View
--- | --- | --- | --- | ---
A/C Compressor Relay | Underhood Electrical Center, left hand side of engine compartment | 19 | 36 | --
A/C Refrigerant Pressure Sensor | Above right hand Shock Tower, in high side refrigerant line between compressor and evaporator | 19 | 35 | --
Camshaft Position (CMP) Sensor | Mounted to engine front cover | 29 | 56 | --
Crankshaft Position (CKP) Sensor | Lower front of engine behind Harmonic Balancer | 29 | 57 | 202-12
Data Link Connector (DLC) | On bottom of Instrument Panel, right of steering column | -- | -- | 50-2
Engine Coolant Temperature (ECT) Sensor | Front of lower Intake Manifold, under Thorottle Body | 8 | 14 | --
Evaporative Canister Purge Solenoid Valve | Right center of Engine mounted to Manifold | 26 | 30 | --
Evaporative Purge Vacuum Switch | Rear right hand top of engine | 6 | 10 | --
Exhaust Gas Recirculation (EGR) Valve | Upper left hand side of engine | 27 | 53 | 202-14
Fuel Injectors | Top of engine, mounted to fuel rail, at each cylinder intake port | 26, 27 | 50, 53 | --
Fuel Pump Prime Connector | Top of right hand Shock Tower, 1-way connector out of harness. | 15 | 28 | --
Fuel Pump/Fuel Level Sender | Mounted inside fuel tank | -- | -- | --
Fuel Pump Relay | Forward of left hand kick panel, mounted to foot-rest bracket under carpet. | 7 | 13 | 202-14
Fuse Block | LH side of Instrument Panel | 8 | 15 | --
Generator | Top center right hand side of engine | -- | -- | --
Heated Oxygen Sensor, Bank 1 HO2S 1 | Mounted in rear of right hand exhaust manifold | 6 | 10 | 202-15
Heated Oxygen Sensor, Bank 1 HO2S 2 | In exhaust system, front of Catalytic Converter. | 29 | 58 | 202-15
Heated Oxygen Sensor, Bank 1 HO2S 3 | In exhaust system, rear of Catalytic Converter. | 29 | 58 | 202-15
Heated Oxygen Sensor, Bank 2 HO2S 1 | Mounted in rear of left hand exhaust manifold | 12 | 22 | 202-15
Idle Air Control Valve (IAC) | Right front on Intake Manifold | 13 | 25 | 202-15
Ignition Control Module (ICM) | Above Left hand Valve Cover | 27 | 53 | 202-13
Intake Air Temperature (IAT) Sensor | Front of engine compartment, on front intake air duct | 28 | 55 | --
Bank 1 Knock Sensor, left hand (KS) | Left hand of engine block | 27 | 52 | --
Bank 2 Knock Sensor, right hand (KS) | Right hand of engine block | 11 | 20 | --
Malfunction Indicator Lamp (MIL) | Upper right hand side of Instrument Panel | -- | Refer to Instrument Cluster in Electrical Diagnosis | --
Manifold Absolute Pressure (MAP) Sensor | Mounted to intake vacuum source on rear right hand side of intake manifold | 6 | 10 | 202-16
Mass Air Flow (MAF) Sensor | Mounted to top of Throttle body | 13 | 25 | 202-17
Powertrain Control Module (PCM) | In Engine compartment, rearward of right hand Shock Tower | 19 | 35 | 22-8
Positive Crankcase Ventilation Valve | Top right hand front of engine | -- | -- | --
Primary Cooling Fan | Left hand side behind radiator | -- | -- | --
Primary Cooling Fan Relay | Underhood Electrical Center, left hand side of engine compartment. | 7 | 15 | 202-35
Secondary Cooling Fan | Right hand side, behind radiator | -- | -- | --
Secondary Cooling Fan Relay | Underhood Electrical Center, left hand side of engine compartment. | 3 | 8 | 11-5
SMCC II Cruise Control Module | Left hand of vehicle, mounted to frame rail forward of front wheelhouse. | 19 | 36 | 34-2 50-2
Body Control Module | Mounted to HAVC Module, above right hand I/P insulator panel | 22 | 41 | 202-16
Throttle Body | Mounted to the Upper Intake Manifold, top, in center front of engine | -- | -- | --
Throttle Position (TP) Sensor | Right hand side of Throttle Body Assembly | 13 | 25 | --
TCC Brake Switch (Automatic Transmission) | Mounted in Brake pedal bracket, Lower left hand side of I/P | 0 | 1 | --
Clutch Anticipate/Cruise Release Switch (Manual Transmission) | Mounted in Brake/Clutch pedal bracket, Lower left hand side of I/P | 0 | 1 | --
Underhood Electrical Center | Left hand side of engine compartment. | 3 | 8 | 10-0
Vehicle Speed Sensor (M30 Automatic Transmission) (VSS) | Rear right hand side of Transmission | 10 | 20 | --
Vehicle Speed Sensor (MM6 Manual Transmission) (VSS) | Rear left hand side of Transmission | 16, 26 | 30, 51 | --