For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
1st - 2nd Shift Solenoid Valve | Inside the automatic transmission | Automatic Transmission Electronic Component Views in Automatic Transmission | Automatic Transmission Internal Connector End Views in Automatic Transmission
2nd - 3rd Shift Solenoid Valve | Inside the automatic transmission | Automatic Transmission Electronic Component Views in Automatic Transmission | Automatic Transmission Internal Connector End Views in Automatic Transmission
3rd - 2nd Shift Solenoid Valve | Inside the automatic transmission | Automatic Transmission Electronic Component Views in Automatic Transmission | Automatic Transmission Internal Connector End Views in Automatic Transmission
A/C Compressor Clutch | Front of engine , lower right side | HVAC Component Views in HVAC Systems with A/C - Manual | Engine Controls Connector End Views
A/C Clutch Diode (V6 VIN K) | Sealed in harness, approximately 3 cm from injector 2 breakout | -- | --
A/C Refrigerant Pressure Sensor | Above the right front wheelhouse, attached to refrigerant line | HVAC Component Views in HVAC Systems with A/C - Manual | Engine Controls Connector End Views
Automatic Transmission | Behind engine | -- | Automatic Transmission Inline Harness Connector End View in Automatic Transmission
Body Control Module (BCM) | Under the right side of I/P, near the blower motor | Body Control System Component Views in Body Control Module | Body Control System Connector End Views in Body Control Module
Camshaft Position (CMP) Sensor | Mounted in engine front cover | Engine Controls Component Views | Engine Controls Connector End Views
Crankshaft Position (CKP) Sensor | Lower front of engine | Engine Controls Component Views | Engine Controls Connector End Views
Cruise Control Module | Mounted to the left front frame rail, forward of wheelhouse | Cruise Control Components in Cruise Control | Cruise Control Connector End Views in Cruise Control
Data Link Connector (DLC) | Under the I/P, right of the steering column | -- | Engine Controls Connector End Views
Electronic Brake Control Module (EBCM) | Mounted with brake pressure modulator valve on top of left front frame rail top front left side of engine | -- | Antilock Brake System Connector End Views in Antilock Brake System
Electronic Ignition Control Module (ICM) (V6 VIN K) | Top front left side of engine | Engine Controls Component Views | Engine Controls Connector End Views
Engine Coolant Temperature (ECT) Sensor | Under throttle body, front side of engine | Engine Controls Component Views | Engine Controls Connector End Views
Engine Cooling Fan | Behind radiator | -- | Cooling System Connector End Views in Engine Cooling
Engine Oil Level Switch (V6 VIN K) | Lower left side of engine, in oil pan | Engine Controls Component Views | Engine Controls Connector End Views
Exhaust Gas Recirculation (EGR) Valve (V6 VIN K) | Front left side of engine, in front of ignition control module | Engine Controls Component Views | Engine Controls Connector End Views
Evaporative Emission (EVAP) Canister Purge Solenoid Valve (V6 VIN K) | Front of engine, RH side next to injector #2 | Engine Controls Component Views | Engine Controls Connector End Views
Evaporative Emission (EVAP) Canister Vent Solenoid Valve (V6 VIN K) | Top, right side engine, part of EVAP canister | Engine Controls Component Views | Engine Controls Connector End Views
Fuel Injectors (V6 VIN K) | Mounted on intake manifold, part of fuel rail | Engine Controls Component Views | Engine Controls Connector End Views
Fuel Tank Unit | Under rear of vehicle | -- | --
Heated Oxygen Sensor Bank 1, Sensor 1 (V6 VIN K) | Mounted in left exhaust manifold | Engine Controls Component Views | Engine Controls Connector End Views
Heated Oxygen Sensor Bank 2, Sensor 1 (V6 VIN K) | Mounted in right exhaust manifold | Engine Controls Component Views | Engine Controls Connector End Views
Heated Oxygen Sensor Bank 1, Sensor 3 (V6 VIN K) | At rear of catalytic converter | Engine Controls Component Views | Engine Controls Connector End Views
HVAC Control | Center of I/P, above radio | HVAC Component Views in HVAC Systems with A/C - Manual | HVAC Connector End Views in HVAC Systems with A/C - Manual
Idle Air Control (IAC) Valve (V6 VIN K) | Right front of intake manifold | Engine Controls Component Views | Engine Controls Connector End Views
Instrument Cluster | Left side of I/P | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges, and Console | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges, and Console
I/P Fuse Block | Left end of the I/P carrier | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Intake Air Temperature (IAT) Sensor | Mounted on air duct, in front of intake manifold | Engine Controls Component Views | Engine Controls Connector End Views
Knock Sensor, LH (V6 VIN K) | In bottom left side of engine block | Engine Controls Component Views | Engine Controls Connector End Views
Knock Sensor, RH (V6 VIN K) | In bottom right side of engine block | Engine Controls Component Views | Engine Controls Connector End Views
Manifold Absolute Pressure (MAP) Sensor (V6 VIN K) | Mounted to right side of intake manifold | Engine Controls Component Views | Engine Controls Connector End Views
Mass Air Flow (MAF) Sensor (V6 VIN K) | Mounted on air duct, in front of intake manifold | Engine Controls Component Views | Engine Controls Connector End Views
Park Neutral Position Switch | Under console, on base of the shift control lever | -- | Engine Controls Connector End Views in Engine Controls 5.7L
Powertrain Control Module (PCM) (V6 VIN K) | Right side of engine compartment, rear of wheelhouse |

#### PCM Location

Powertrain Control Module Connector End Views

Radio | Center of I/P, below HVAC control | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
Stoplamp Switch | Mounted on the brake pedal bracket | Hydraulic Brake Component Views in Hydraulic Brakes | Antilock Brake System Connector End Views in Antilock Brake Systems
Throttle Actuator Control (TAC) Module | Mounted on the Accelerator pedal | -- | --
Throttle Position (TP) Sensor | Mounted to front of throttle body | Engine Controls Component Views | Engine Controls Connector End Views
Undercoat Electrical Center 1 | Left front corner of the engine compartment | Power and Grounding Component Views in Wiring Systems | Electrical Center Identification Views in Wiring Systems
Undercoat Electrical Center 2 | Left front corner of the engine compartment | Power and Grounding Component Views in Wiring Systems | Electrical Center Identification Views in Wiring Systems
Vehicle Speed Sensor (Manual) | Rear left side of transmission | -- | Engine Controls Connector End Views
C100 (10 cavities) | Engine to forward lamp harness, in the engine compartment, above right wheelhouse | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C101 (10 cavities) | Engine to forward lamp harness, in the engine compartment, above right wheelhouse | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C102 (1 cavities) | Engine to forward lamp harness, in the engine compartment, above right wheelhouse | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C105 (8 cavities) | Engine to forward lamp harness, in engine compartment, above right wheelhouse | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C106 (7 cavities) | Engine to engine jumper harness | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C107 (7 cavities) | Engine to engine jumper harness | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C108 (3 cavities) | Engine to camshaft position sensor jumper harness | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200A (17 cavities) | Forward lamp to I/P harness, between left kick panel and steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200B (18 cavities) | Forward lamp to I/P harness, between left kick panel and steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200D (48 cavities) | Part of the I/P harness, between the left kick panel and the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C210 (8 cavities) | I/P to engine harness, under right side of I/P, behind knee bolster | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C220 (10 cavities) | I/P to engine harness, under right side of I/P, behind knee bolster | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C230 (10 cavities) | I/P to engine harness, under right side of I/P, behind knee bolster | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C405A (7 cavities) | Fuel tank harness to I/P harness pass through connector, forward of rear axle | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C405B (16 cavities) | I/P harness pass through connector, forward of rear axle | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C405D (4 cavities) | Fuel tank harness to I/P harness pass through connector, forward of rear axle | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G106 | Attached to top left side of radiator support | Power and Grounding Components in Wiring Systems | --
G110 (V6 VIN K) | Front of engine, bolted to pulley above A/C clutch connector | Power and Grounding Components in Wiring Systems | --
G112 | Attached to rear of left cylinder head | Power and Grounding Components in Wiring Systems | --
G200 | Near left "A" pillar, bolted to I/P mounting stud behind kick panel | Power and Grounding Components in Wiring Systems | --
G305 | Bolted to left rocker panel at floor pan bar 3 | Power and Grounding Components in Wiring Systems | --
P100 | Left side in dash panel, engine to passenger compartment | Harness Routing Views in Wiring Systems | --
P110 | Right side in dash panel, engine to passenger compartment | Harness Routing Views in Wiring Systems | --
S104 (V6 VIN K) | Engine harness, main branch approximately 15 cm from vehicle speed sensor breakout | -- | --
S107 (V6 VIN K) | Engine harness, main branch, approximately 21 cm from powertrain control module (PCM) breakout | -- | --
S108 (V6 VIN K) | Engine harness, main branch, approximately 7 cm from vehicle speed sensor breakout | -- | --
S110 (V6 VIN K) | Engine harness, approximately 4 cm from powertrain control module (PCM) breakout | -- | --
S113 | Forward lamp harness, approximately 7 cm from engine coolant fans/cruise control module breakout | -- | --
S114 (V6 VIN K) | Engine harness, approximately 3 cm from generator breakout | -- | --
S115 (V6 VIN K) | Engine harness at generator breakout | -- | --
S117 (V6 VIN K) | Engine harness, approximately 2.5 cm from engine fuel injector 5 breakout | -- | --
S121 (V6 VIN K) | Engine harness, main branch, approximately 8 cm from powertrain control module (PCM) breakout | -- | --
S144 (V6 VIN K) | Engine harness, approximately 2 cm from engine fuel injector 3 breakout | -- | --
S145 (V6 VIN K) | Engine harness, approximately 3.5 cm from engine fuel injector 3 breakout | -- | --
S148 (V6 VIN K) | I/P harness, approximately 2 cm from radio connectors breakout | -- | --
S159 | Forward lamp harness, approximately 8 cm into secondary air injection bleed valve solenoid breakout (CKT 429) | -- | --
S165 | Forward lamp harness, approximately 7 cm from main branch into underhood electrical center 2 breakout (CKT 139) | -- | --
S166 | Forward lamp harness, approximately 14 cm from G105 breakout | -- | --
S167 | Forward lamp harness, approximately 7 cm from underhood electrical center 1 breakout | -- | --
S169 | Forward lamp harness, approximately 6 cm from main branch into underhood electrical center 1 breakout | -- | --
S177 | Forward lamp harness, approximately 4 cm from main branch into underhood electrical center 1 breakout | -- | --
S179 | Forward lamp harness, approximately 25 cm from underhood electrical center 1 breakout | -- | --
S182 | Forward lamp harness, approximately 15 cm from underhood electrical center 1 breakout | -- | --
S184 | Forward lamp harness, approximately 5 cm from underhood electrical center 1 breakout | -- | --
S206 | I/P harness, at rear compartment lid release relay breakout | -- | --
S215 | I/P harness, approximately 11 cm from antenna cable breakout | -- | --
S217 | I/P harness, approximately 18 cm from body control module (BCM) breakout | -- | --
S225 | I/P harness, approximately 6 cm from the blower motor breakout | -- | --
S234 (Automatic) | I/P harness, approximately 5 cm from the body control module (BCM) breakout | -- | --
S240 | I/P harness, approximately 17 cm from the antenna cable breakout | -- | --
S242 | I/P harness, approximately 4 cm from the data link connector (DLC) breakout | -- | --
S244 (Coupe) | I/P harness, approximately 40 cm back from C405 | -- | --
S244 (Convertible) | I/P harness, approximately 46 cm back from C405 | -- | --