For 1990-2009 cars

Application | Millimeters | Inches
--- | --- | ---
Aluminum Wheel

- Lateral Runout

0.762

0.030

- Radial Runout

0.762

0.030

Tire and Wheel Assembly (Radial and Lateral Runout)

- Off-Vehicle

1.27

0.05

- On-Vehicle

1.52

0.06

- Wheel Stud

0.25

0.01

- Wheel Hub

0.132

0.0052

One-Piece Propeller Shaft Runout Specifications
Front | 1.016 mm | 0.040 in
Center | 1.27 mm | 0.050 in
Rear | 1.40 mm | 0.055 in
Two-Piece Propeller Shaft Runout Specifications
Front | 0.762 mm | 0.030 in
Center | 0.762 mm | 0.030 in
Rear | 0.889 mm | 0.035 in
Pinion Runout Specifications
Flange | 0.076 mm | 0.003 in