For 1990-2009 cars

# FRONT DOOR GLASS RETAINER ASSY (NEW PARTS USAGE)

#### Subject: FRONT DOOR GLASS RETAINER ASSEMBLIES (COMMONLY CALLED "DOOR GLASS PATCH") NEW PARTS USAGE

#### Models Affected: 1992 FIREBIRD MODELS

1991 Firebird vehicles built after VIN breakpoint NL202399 will use a new type front door glass retainer assembly.

The new part combines the vertical weatherstrip and plastic panel (used on earlier styles) into a single component.

If service of these parts is required, it is recommended that the part be replaced with the type part it was built with.

#### Example:

- Past models prior to 1992 VIN breakpoints, use the early type multi piece retainer. - Models built after VIN breakpoints, use new components.

Part Numbers: 10198202 - Right 10198203 - Left

Parts are currently available from GMSPO.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.