For 1990-2009 cars

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
A/C Refrigerant Pressure Sensor | 6 | -- | 53
Camshaft Position (CMP) Sensor Retaining Bolt | 10 | -- | 89
Crankshaft Balancer Bolt | 150 +114° | 111 +114° | --
Crankshaft Position (CKP) Sensor Bolts | 20 | 15 | --
Engine Coolant Temperature (ECT) Sensor | 25 | 18 | --
Engine Oil Level Switch | 20 | 15 | --
Exhaust Gas Recirculation Valve Adapter Bolt to Exhaust Manifold | 25 | 18 | --
Exhaust Gas Recirculation Valve Adapter Nuts to Cylinder Head | 50 | 37 | --
Exhaust Gas Recirculation Valve Nuts to EGR Valve Adapter | 29 | 21 | --
Exhaust Gas Recirculation Valve Outlet Pipe Bolt to Upper Intake Manifold | 25 | 18 | --
Exhaust Gas Recirculation Valve Outlet Pipe Nut to EGR Valve Adapter | 29 | 21 | --
Fuel Filter Fitting | 30 | 22 | --
Fuel Pipe Front Clip Bolts | 4.5 | -- | 40
Fuel Pipe Rear Clip Bolt | 5.5 | -- | 49
Fuel Pipe Shield Bolt | 5 | -- | 44
Fuel Pipe Shield Nuts | 5 | -- | 44
Fuel Pipe Shield Studs | 5 | -- | 44
Fuel Rail Attaching Nuts or Bolts | 10 | -- | 89
Fuel Sender Assembly Attaching Nuts | 6.5 | -- | 58
Fuel Tank Fill Pipe Shield Bolt | 2.5 | -- | 22
Fuel Tank Retaining Strap Bolts | 33 | 25 | --
Heated Oxygen Sensor(s) | 42 | 31 | --
Idle Air Control Valve Attaching Screws | 3 | -- | 27
Ignition Coil to Ignition Control Module Screws | 4-5 | -- | 40
Ignition Control Module Assembly to Bracket Nuts | 30 | 22 | --
In-Pipe Fuel Filter Nut | 30 | 22 | --
Knock Sensor(s) | 19 | 14 | --
Spark Plug(s) | 27 | 20 | --
Throttle Body Retaining Nuts or Bolts | 10 | -- | 89
Throttle Position Sensor Attaching Screws | 2 | -- | 18