For 1990-2009 cars

Table 1: | Outside Remote Control Rearview Mirror Select Switch (Pontiac)
Table 2: | Outside Rearview Mirror Motor RH and LH

#### Outside Remote Control Rearview Mirror Select Switch (Pontiac)

Connector Part Information |

• | 1206-4862

• | 8 Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 750 | Ground
B | LT BLU | 82 | Power mirror motor feed--left horizontal motor--left direction
C | YEL | 88 | Power mirror motor feed--left vertical motor--up direction
D | WHT | 81 | Power mirror motor feed--left horizontal motor--right direction
E | LT GRN | 89 | Power mirror motor feed--left vertical motor--down direction
F | BRN/WHT | 149 | Courtesy lamp feed
G | RED/WHT | 881 | Power mirror motor feed--right horizontal motor--right direction
H | ORN | 640 | Fuse output--battery--type III fuse

#### Outside Rearview Mirror Motor RH and LH

Connector Part Information |

• | 1206-6498

• | 4 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED/WHT | 881 | Power Mirror motor feed--right horizontal motor--right direction (RH Mirror)
A | WHT | 81 | Power Mirror motor feed--left horizontal motor--right direction (LH Mirror)
B | GRY | 90 | Power Mirror motor feed--right horizontal motor--left direction (RH Mirror)
B | LT BLU | 82 | Power Mirror motor feed--left horizontal motor--left direction (LH Mirror)
C | GRY | 90 | Power Mirror motor feed--right horizontal motor--left direction (RH Mirror)
C | LT BLU | 82 | Power Mirror motor feed--left horizontal motor--left direction (LH Mirror)
D | DK BLU/WHT | 149 | Power Mirror motor feed--right vertical motor--up direction (RH Mirror)
D | YEL | 88 | Power Mirror motor feed--left vertical motor--up direction (LH Mirror)