For 1990-2009 cars

# INOP. POWER DOOR LOCKS/ POWER WINDOWS

#### SUBJECT: INOPERATIVE POWER DOOR LOCKS/POWER WINDOWS (INSTALL NEW SWITCHES)

#### MODELS: 1993-97 CHEVROLET CAMARO 1994-97 PONTIAC FIREBIRD

#### CONDITION:

SOME OWNERS MAY COMMENT THAT THE POWER DOOR LOCKS/POWER WINDOWS ARE INOPERATIVE.

#### CAUSE:

THE PLASTIC USED IN THE ROCKER KNOB PORTION OF THE ORIGINAL POWER DOOR LOCK/POWER WINDOW SWITCHES MAY BE ATTACKED BY THE GREASE IN THE SWITCH, CAUSING THE MOUNTING TABS TO BREAK. A NEW MATERIAL WAS USED IN PRODUCTION STARTING IN JANUARY, 1997.

#### CORRECTION:

REPLACE THE SWITCHES WITH THE NEW PART NUMBERS LISTED BELOW. FOLLOW THE INSTRUCTIONS IN SECTION 10-6 OF THE SERVICE MANUAL. ANY OF THE OLD SWITCHES IN DEALER STOCK SHOULD NOT BE USED AND SHOULD BE RETURNED TO GMSPO FOR CREDIT.

#### PARTS INFORMATION:

NEW P/N OLD P/N APPLICATION ======= ======= ===========

10402835 10290123 PDL - RH 94-96 CHEVROLET 10402836 10290122 PDL - LH 94-96 CHEVROLET 10402837 10290120 PW - RH 94-96 CHEVROLET 10402838 10290119 PW - LH 94-96 CHEVROLET 10402839 10273827 PDL - RH 97 CHEVROLET 10402840 10273826 PDL - LH 97 CHEVROLET 10402841 10273840 PW - RH 97 CHEVROLET 10402842 10273839 PW - LH 97 CHEVROLET 10402843 10290121 PDL - RH/LH 93-97 PONTIAC 10402844 10290117 PW - RH 93-97 PONTIAC 10402845 10290118 PW - LH 93-97 PONTIAC

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### IMPORTANT: NEW SWITCHES FOR THE 1993 CHEVROLET HAVE NOT YET BEEN RELEASED. THIS BULLETIN WILL BE UPDATED WHEN THEY ARE AVAILABLE.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER DESCRIPTION LABOR TIME =============== =========== ==========

N2114 DOOR LOCK - RF USE PUBLISHED LABOR OPERATION TIME

N2115 DOOR LOCK - LF USE PUBLISHED LABOR OPERATION TIME

N2144 DOOR WINDOW - RF USE PUBLISHED LABOR OPERATION TIME

N2145 DOOR WINDOW - LF USE PUBLISHED LABOR OPERATION TIME

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.