For 1990-2009 cars

# SQUEAKS FROM REAR AREA OF FRT. DOORS - REPLACE WEDGE PLATE

#### Subject: SQUEAKS FROM REAR OF DOORS (NEW BODY SIDE WEDGE PLATE)

#### Models Affected: 1982-1991 FIREBIRD MODELS WITH T-TOPS OR CONVERTIBLES

#### Condition:

---------- Some customers may comment about squeaks coming from the rear areas of front doors.

#### Cause:

------- May be due to metal portion of wedge plate system becoming dry and generating squeak noise.

#### Correction:

----------- Replace the body side portion of the wedge plate system with new plastic type available from GMSPO, P/N 10198229.

Parts are expected to be available on March 18, 1991. Until then normal part orders will not be accepted by GMSPO. Only verifiable emergency VIP orders will be accepted. SPO will make every effort to obtain parts. All parts will be placed on 400 control to waive VIP surcharges. However, the part will be shipped premium transportation at dealer's expense. All other order types will be cancelled as incorrectly ordered while the 400 control is in place.

#### Procedure:

1. Remove original metal type body side wedge plate and gasket from the door opening and discard.

2. Install the new plastic type wedge plate to the body with the original screws and torque to 2.0 N.m (18 lbs. in.).

3. Check for proper contact by placing a piece of masking tape on the wedge plate and slowly closing the door. Open the door and check the tape for contact marks.

#### Important: Properly adjusted wedge plates should have approximately 1.0 mm of interference with the door in the full closed position.

Shims that locate behind the door portion wedge plate are available from GMSPO and come in the following thickness.

1.0mm - P/N 20452860

2.Omm - P/N 20452861

Parts are currently available from GMSPO.

Labor Operation Number: T1548

Labor Time : .2 Hours Per Side

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.