For 1990-2009 cars

Application | N·m | Lbs Ft | Lbs In
--- | --- | --- | ---
Catalytic Converter Hanger Bolt | 41 | 30 | --
Catalytic Converter Heat Shield Bolt | 2.0 | -- | 18
Catalytic Converter Bolt | 25 | 18 | --
Crossover Pipe Nut | 35 | 26 | --
Exhaust Heat Shield Bolt | 2.0 | -- | 18
Exhaust Manifold Pipe Bolt | 35 | 26 | --
Exhaust Muffler Clamp Bolt | 68 | 50 | --
Exhaust Muffler Hanger Bolt | 9.5 | -- | 84
Exhaust Muffler Heat Shield Bolt | 2.0 | -- | 18
Exhaust Pipe Hanger Nut | 20 | 15 | --
Exhaust Pipe Hanger Bracket Bolt | 9.5 | -- | 84
Exhaust Pipe Heat Shield Bolt | 2.0 | -- | 18
Heated Oxygen Sensor | 42 | 31 | --