For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. On vehicles with manual transmission, apply the park brake.
2. On vehicles with automatic transmission, place the shift lever in the park position.
3. Depress the rear compartment lid release switch.

The rear compartment lid opens.

The rear compartment lid does not open. Refer to Rear Compartment Lid Release Inoperative .

2 |

1. Close the rear compartment lid.
2. Press the rear compartment lid release button on the remote control door lock transmitter.

The rear compartment lid opens.

The rear compartment lid does not open. Refer to Remote Keyless Entry System Check .

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.