For 1990-2009 cars

Table 1: | A/C Compressor Clutch
Table 2: | A/C Refrigerant Pressure Sensor
Table 3: | Camshaft Position (CMP) Sensor
Table 4: | Crankshaft Position (CKP) Sensor
Table 5: | Engine Coolant Temperature Sensor
Table 6: | Engine Oil Level Switch
Table 7: | Evaporative Emission (EVAP) Canister Purge Valve
Table 8: | Evaporative Emission (EVAP) Canister Vent Valve
Table 9: | Exhaust Gas Recirculation (EGR) Valve
Table 10: | Fuel Injector #1
Table 11: | Fuel Injector #3
Table 12: | Fuel Injector #5
Table 13: | Fuel Injector #7
Table 14: | Fuel Injector #2
Table 15: | Fuel Injector #4
Table 16: | Fuel Injector #6
Table 17: | Fuel Injector #8
Table 18: | Fuel Tank Pressure Sensor
Table 19: | Heated Oxygen Sensor (HO2S), Left Rear
Table 20: | Heated Oxygen Sensor (HO2S), Right Front
Table 21: | Heated Oxygen Sensor (HO2S), Right Rear
Table 22: | Idle Air Control (IAC) Valve
Table 23: | Intake Air Temperature (IAT) Sensor
Table 24: | Knock Sensors (KS)
Table 25: | Manifold Absolute Pressure (MAP) Sensor
Table 26: | Mass Air Flow (MAF) Sensor
Table 27: | Reverse Inhibit Solenoid
Table 28: | Secondary Air Injection (AIR) Bleed Valve Solenoid
Table 29: | Secondary Air Injection (AIR) Pump
Table 30: | Skip Shift Solenoid
Table 31: | Throttle Position (TP) Sensor
Table 32: | Vehicle Speed Sensor (VSS)

#### A/C Compressor Clutch

Connector Part Information |

• | 1216-2017

• | 2 Way F Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK GRN | 59 | A/C Compressor Clutch Control
B | BLK | 450 | A/C Compressor Clutch Ground

#### A/C Refrigerant Pressure Sensor

Connector Part Information |

• | 1211-0192

• | 3 Way M Metri-Pack 150 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 407 | A/C Refrigerant Pressure Sensor Ground
B | GRY | 474 | A/C Refrigerant Pressure Sensor 5.0V Reference
C | RED/BLK | 380 | A/C Refrigerant Pressure Sensor Signal

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | 1205-9595

• | 3 Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN/WHT | 633 | Camshaft Position (CMP) Sensor Signal - Input
B | PNK/BLK | 632 | Reference Low
C | RED | 631 | Ignition Feed

#### Crankshaft Position (CKP) Sensor

Connector Part Information |

• | 1205-9595

• | 3 Way Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 573 | Crankshaft Position (CKP) Sensor Signal - Input
B | YEL/BLK | 1868 | Reference Low
C | LT GRN | 1867 | Ignition Feed

#### Engine Coolant Temperature Sensor

Connector Part Information |

• | 1211-0192

• | 3 Way F Metri-Pack 150 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 718 | Engine Coolant Tenperature (ECT) Sensor Ground
B | YEL | 410 | Engine Coolant Temperature (ECT) Sensor Signal
C | DK GRN | 135 | Engine Coolant Temperature (ECT) Sensor Output

#### Engine Oil Level Switch

Connector Part Information |

• | 1205-2641

• | 2 Way F Metri-Pack 150 Series Sealed

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 1174 | Oil Level Switch Signal
B | BLK | 450 | Ground

#### Evaporative Emission (EVAP) Canister Purge Valve

Connector Part Information |

• | 1205-2643

• | 2 Way Metri-Pack 150 Series Sealed (RED)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 239 | Ignition Feed
B | DK GRN/WHT | 428 | EVAP Canister Purge Valve Control

#### Evaporative Emission (EVAP) Canister Vent Valve

Connector Part Information |

• | 1205-2643

• | 2 Way F Metri-Pack 150 Series Sealed (RED)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 239 | Ignition Feed
B | WHT | 1310 | EVAP Canister Vent Valve Control

#### Exhaust Gas Recirculation (EGR) Valve

Connector Part Information |

• | 1218-6056

• | 5 Way F Metri-Pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 435 | Exhaust Gas Recirculation (EGR) Valve Ground
B | BLK | 552 | Exhaust Gas Recirculation (EGR) Sensor Ground
C | BRN | 1456 | Exhaust Gas Recirculation (EGR) Pintle Position
D | GRY | 705 | Exhaust Gas Recirculation (EGR) 5V Reference
E | LT BLU | 697 | Exhaust Gas Recirculation (EGR) Valve Control

#### Fuel Injector #1

Connector Part Information |

• | 1212-9140

• | 2 Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition Feed
B | BLK | 1744 | Fuel Injector #1 Control

#### Fuel Injector #3

Connector Part Information |

• | 1212-9140

• | 2 Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition Feed
B | PNK/BLK | 1746 | Fuel Injector #3 Control

#### Fuel Injector #5

Connector Part Information |

• | 1212-9140

• | 2 Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition Feed
B | BLK/WHT | 845 | Fuel Injector #5 Control

#### Fuel Injector #7

Connector Part Information |

• | 1212-9140

• | 2 Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition Feed
B | RED/BLK | 877 | Fuel Injector #7 Control

#### Fuel Injector #2

Connector Part Information |

• | 1212-9140

• | 2 Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 839 | Ignition Feed
B | LT GRN/BLK | 1745 | Fuel Injector #2 Control

#### Fuel Injector #4

Connector Part Information |

• | 1212-9140

• | 2 Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 839 | Ignition Feed
B | LT BLU/BLK | 844 | Fuel Injector #4 Control

#### Fuel Injector #6

Connector Part Information |

• | 1212-9140

• | 2 Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 839 | Ignition Feed
B | YEL/BLK | 846 | Fuel Injector #6 Control

#### Fuel Injector #8

Connector Part Information |

• | 1212-9140

• | 2 Way F Metri-Pack 280.1 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 839 | Ignition Feed
B | DK BLU/WHT | 878 | Fuel Injector #8 Control

#### Fuel Tank Pressure Sensor

Connector Part Information |

• | 1205-9595

• | 3 Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | Fuel Sensor Ground
B | DK GRN | 890 | Fuel Tank Pressure Signal
C | GRY/BLK | 416 | 5V Sensor Feed

#### Heated Oxygen Sensor (HO2S), Left Rear

Connector Part Information |

• | 1216-0825

• | 4 Way Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/WHT | 1669 | LR Heated Oxygen Sensor (HO2S) - Low
B | PPL/WHT | 1668 | LR Heated Oxygen Sensor (HO2S) - High
C | BLK | 450 | Ground
D | PNK | 539 | Ignition Feed

#### Heated Oxygen Sensor (HO2S), Right Front

Connector Part Information |

• | 121-60825

• | 4 Way M Metri-Pack 150 Series Sealed(BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 1667 | Heated Oxygen Sensor (HO2S) - Low
B | PPL | 1666 | Heated Oxygen Sensor (HO2S) - High
C | BLK | 450 | Ground
D | PNK | 539 | Ignition Feed

#### Heated Oxygen Sensor (HO2S), Right Rear

Connector Part Information |

• | 1216-0825

• | 4 Way M Metri-Pack 150 Series Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 1671 | RR Heated Oxygen Sensor (HO2S) - Low
B | PPL | 1670 | RR Heated Oxygen Sensor (HO2S) - High
C | BLK | 450 | Ground
D | PNK | 539 | Ignition Feed

#### Idle Air Control (IAC) Valve

Connector Part Information |

• | 1216-2190

• | 4 Way F Metri-Pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/BLK | 444 | Idle Air Control (IAC) Valve Coil B Signal - Low
B | LT GRN WHT | 1749 | Idle Air Control (IAC) Valve Coil B Signal - High
C | LT BLU/BLK | 1748 | Idle Air Control (IAC) Valve Coil A Signal - Low
D | LT BLU/WHT | 1747 | Idle Air Control (IAC) Valve Coil A Signal - High

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | 1216-2199

• | 2 Way F Metri Pack 150.2 Series Pull to Seat (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 719 | Intake Air Temperature (IAT) Sensor Ground
B | TAN | 472 | Intake Air Temperature (IAT) Sensor Signal

#### Knock Sensors (KS)

Connector Part Information |

• | 1205-2641

• | 2 Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 496 | Knock Sensor (KS) Signal - Front
B | LT BLU | 1876 | Knock Sensor (KS) Signal - Rear

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | 1212-9946

• | 3 Way F Metri Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | Manifold Absolute Pressure (MAP) Sensor Ground
B | LT GRN | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
C | GRY | 416 | Manifold Absolute Pressure (MAP) Sensor 5.0V Reference

#### Mass Air Flow (MAF) Sensor

Connector Part Information |

• | 1205-9595

• | 3 Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 492 | Mass Air Flow (MAF) Sensor Signal
B | BLK/WHT | 451 | Ground
C | PNK | 539 | Ignition Feed

#### Reverse Inhibit Solenoid

Connector Part Information |

• | 1205-2646

• | 2 Way F Metri-Pack 150 Series Sealed (WHT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 1652 | Reverse Inhibit Solenoid Control
B | PNK | 539 | Ignition Feed

#### Secondary Air Injection (AIR) Bleed Valve Solenoid

Connector Part Information |

• | 1205-2643

• | 2 Way F Metri-Pack 150 Series Sealed (RED)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK/BLK | 429 | Secondary Air Injection Bleed Valve Solenoid - Feed
B | BLK | 150 | Ground

#### Secondary Air Injection (AIR) Pump

Connector Part Information |

• | 1211-0293

• | 3 Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 78 | Secondary Air Injection Pump Motor - Feed
B | PNK/BLK | 429 | Secondary Air Injection Solenoid - Feed
C | BLK | 150 | Ground

#### Skip Shift Solenoid

Connector Part Information |

• | 1205-2643

• | 2 Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 587 | Skip Shift Solenoid Control
B | PNK | 539 | Ignition Feed

#### Throttle Position (TP) Sensor

Connector Part Information |

• | 1211-0192

• | 3 Way F Metri-Pack 150 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 596 | Throttle Position (TP) Sensor 5V Reference
B | BLK | 452 | Sensor Ground
C | DK BLU | 417 | Throttle Position Sensor Signal

#### Vehicle Speed Sensor (VSS)

Connector Part Information |

• | 1216-2195

• | 2 Way F Metri-Pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 401 | Vehicle Speed Sensor (VSS) Signal - Low
B | YEL | 400 | Vehicle Speed Sensor (VSS) Signal - High