For 1990-2009 cars

# EARLY/SOFT UPSHIFTS CONTROL VALVE ASSEMBLY

1985 THM 700-R4 "YT" MODEL TRANSMISSIONS - PARISIENNE MODELS WITH 4.3L V-6 ENGINES

On March 18, 1985, or Julian Date 077 (figure 1), all 1985 THM 700-R4 "YT" Model transmissions are being built using a newly calibrated control valve assembly. This new assembly, part #8654229, will eliminate a condition of early and soft upshifts.

#### IMPORTANT: Prior to replacing the control valve assembly for the condition described above, verify that the T.V. cable is adjusted properly. A T.V. cable that is adjusted too long may also cause early and soft upshifts.

Refer to the appropriate service information manual for proper installation procedures.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.