For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Dome Lamp Bolt/Screw | 1.7 N·m | 15 lb in
Fog Lamp to Headlamp Bolt | 10 N·m | 89 lb in
Fog Lamp Bolt (Pontiac) | 15 N·m | 11 lb ft
Fog Lamp Nut (Pontiac) | 8 N·m | 71 lb in
Fog Lamp to Bracket Bolt (Chevrolet) | 10 N·m | 89 lb in
Front Fascia Reinforcement Nut | 10 N·m | 89 lb in
Headlamp Bezel Screw (Pontiac) | 1.7 N·m | 15 lb in
Headlamp Housing Bracket Bolt | 7 N·m | 62 lb in
Headlamp Opening Door Bolt/Screw (Pontiac) | 2.0 N·m | 18 lb in
Headlamp Switch Bolt | 1.9 N·m | 17 lb in
High-Mount Stoplamp Screw | 1.7 N·m | 15 lb in
Inside Handle Bezel Bolt/Screw | 1.4 N·m | 12 lb in
Parking and Turn Signal Lamp Bolt | 2.5 N·m | 22 lb in
Park and Turn Signal Lamp Nut | 4.0 N·m | 35 lb in
Park and Turn Signal Lamp Bolt (Trans Am) | 2.5 N·m | 22 lb in
Rear Fog Lamp Nut (Export) | 1.4 N·m | 12 lb in
Rear License Lamp Screw | 1.9 N·m | 17 lb in
Rear Sidemarker Lamp Screw | 1.4 N·m | 12 lb in
Side Marker Lamp Screw | 1.4 N·m | 12 lb in
Taillamp Nut | 3 N·m | 27 lb in