For 1990-2009 cars

# Service VME - Convertible Top Hydraulic Fluid

Subject: | Service VME -- Convertible Top Hydraulic Fluid

Models: | .

When servicing the vehicle with the VIN you entered, the following diagnosis might be helpful if the vehicle exhibits the described symptoms.

### SERVICE VME

This is a service VME to all Chevrolet and Pontiac dealerships regarding 1994 through 2002 Camaro and Firebird convertible top hydraulic fluid. This is Art Spong, Brand Quality Manager for the F-cars. The service manual and ESI incorrectly advise to use DEXRON® III automatic transmission fluid for the hydraulic fluid in the convertible top system. The proper fluid is a ten-weight SAE oil. A bulletin will be issued and ESI will also be corrected. Thanks. If there are any questions, I can be reached at 586-947-8890.

Please follow this diagnosis process thoroughly and complete each step. If the condition exhibited is resolved without completing every step, the remaining steps do not need to be performed. If these steps do not resolve the condition, please contact GM TAC for further diagnostic assistance. This diagnostic approach was developed for the vehicle with the VIN you entered and should not be automatically be used for other vehicles with similar symptoms.