For 1990-2009 cars

# FIRM ACCELERATOR PEDAL EFFORT CABLE CONSTRUCTION/ROUTING

1984 2.5 LITER FIREBIRD

#### Condition

Customer comment of firm accelerator pedal effort.

#### Cause

Cable construction as well as designated routing may contribute to firm accelerator pedal effort.

#### Correction

Replace the accelerator cable, with a new cable identified by a silver I.D. tag. Part numbers remain unchanged.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.