For 1990-2009 cars

# SCRATCH/DAMAGED VINYL WINDOWS REPAIR KITS AND PROCEDURES

#### VEHICLES AFFECTED: ALL CONVERTIBLE TOPS WITH CLEAR PLASTIC BACK WINDOWS

Customer comments of scratches or damage to clear plastic rear windows on convertible tops can be repaired with a special compound and buffing operation to remove the damage.

The repair kit, Part Number, BPR, contains an instruction sheet, an abrasive compound, anti-static cream and two buffing cloths for the anti-static material. Each kit contains enough material for 10 to 15 repairs.

The recommended repair kit is available from.

DOMINION SURE SEAL 5496 Gurvan Drive Mississauga, On

Phone: 416-625-7900 Telex: 06961303

DISCLAIMER

"We believe this source and their material to be reliable. There may be additional manufacturers of such material. General Motors does not endorse, indicate any preference for or assume any responsibility for the products or equipment from these firms or for any such items which may be available from other sources."

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.