For 1990-2009 cars

Application | N·m | Lb Ft | Lb In.
--- | --- | --- | ---
A/C Refrigerant Pressure Sensor | 5 | -- | 44
Camshaft Position (CMP) Sensor retaining bolt | 10 | -- | 90
Crankshaft Balancer bolt | 150 +76° | 110 +76° | --
Crankshaft Position (CKP) Sensor bolts | 20-40 | 14-28 | --
Engine Coolant Temperature (ECT) Sensor | 30 | 22 | --
Engine Oil Level Switch | 20 | 15 | --
Exhaust Gas Recirculation Valve adapter bolt to Exhaust Manifold | 25 | 18 | --
Exhaust Gas Recirculation Valve adapter nuts to Cylinder Head | 50 | 37 | --
Exhaust Gas Recirculation Valve nuts to EGR Valve Adapter | 29 | 21 | --
Exhaust Gas Recirculation Valve outlet pipe bolt to Upper Intake Manifold | 25 | 18 | --
Exhaust Gas Recirculation Valve outlet pipe nut to EGR Valve Adapter | 29 | 21 | --
Fuel Rail Attaching Nuts or Bolts | 10 | 7 | --
Fuel Tank Retaining Strap Bolts | 33 | 24 | --
Heated Oxygen Sensor(s) | 42 | 31 | --
Idle Air Control Valve Attaching Screws | 3 | -- | 27
Ignition Coil to Ignition Control Module screws | 4-5 | -- | 40
In-Pipe Fuel Filter Nut | 30 | 22 | --
Knock Sensor(s) | 19 | -- | 14
Spark Plug(s) | 27 | 20 | --
Throttle Body Retaining Nuts or Bolts | 10 | 7 | --