For 1990-2009 cars

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Accelerator and Cruise Control Servo Cable Adjuster Bolt | 7.5 | -- | 66
Air Cleaner Bolt | 12 | -- | 106
Air Conditioning Condenser Tube Bolt | 16 | 12 | --
Air Conditioning Condenser Tube Nut | 16 | 12 | --
Coolant Heater Bolt (3.8L) | 1.9 | -- | 17
Coolant Heater (5.7L) | 40 | 30 | --
Coolant Pump Bolt (5.7L) | 25 | 18 | --
Coolant Pump Pulley Bolt (5.7L) - First Pass | 10 | -- | 89
Coolant Pump Pulley Bolt (5.7L) - Last Pass | 25 | 18 | --
Coolant Recovery Reservoir Bolt | 12 | -- | 106
Cooling Fan Motor Bolts | 6 | -- | 53
Drive Belt Tensioner Bolt | 50 | 37 | --
EGR Valve Outlet Pipe Bolt | 29 | 21 | --
EGR Valve Outlet Pipe Nut | 29 | 21 | --
Engine Coolant Temperature Sensor (3.8L) | 25 | 18 | --
Engine Coolant Temperature Sensor (5.7L) | 29 | 21 | --
Engine Block Coolant Drain Hole Plug (5.7L) | 60 | 44 | --
Knock Sensor (3.8L) | 19 | 14 | --
Air Lower Deflector Screw | 10 | -- | 89
Radiator Drain Cock | 1.5 | -- | 13
Transmission Oil Cooler Pipe Fittings at Radiator | 27 | 20 | --
Water Outlet Bolt (3.8L) | 27 | 20 | --
Water Outlet Bolt (5.7L) | 15 | 11 | --
Water Pump Bolt (3.8L) | 15 | 11 + 80° | --
Water Pump Pulley Bolt (3.8L) | 13 | -- | 115