For 1990-2009 cars

Table 1: | Inflatable Restraint Instrument Panel Module
Table 2: | Inflatable Restraint Sensing and Diagnostic Module
Table 3: | Seat Belt Switch

#### Inflatable Restraint Instrument Panel Module

Connector Part Information |

• | 1211-0288

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT/BLK | 1403 | SIR Inflator Feed - Passenger Side High
B | DK GRN/WHT | 1404 | SIR Inflator Output - Passenger Side Low

#### Inflatable Restraint Sensing and Diagnostic Module

Connector Part Information |

• | 1211-0192

• | 12 Way F Micro-Pack 100 Series (YEL)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WHT/BLK | 1403 | Passenger Side - High
2 | WHT | 347 | Driver Side - High
3 | DK GRN | 348 | Driver Side - Low
4 | DK GRN/WHT | 1404 | Passenger Side - Low
5 | TAN | 800 | Serial Data - UART
6 | BLK/WHT | 1751 | Ground
7 | BRN | 358 | Inflatable Restraint Indicator
8 | BLK/WHT | 238 | Seat Belt Switch Signal
10 | YEL | 1139 | Ignition Feed

#### Seat Belt Switch

Connector Part Information |

• | 1204-7663

• | 2 Way Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 238 | Seat Belt Switch Signal
B | BLK | 650 | Ground