For 1990-2009 cars

#### Trim Height Specifications (Front Fascia)

Suspension | Tire | Camaro Frt. Fascia | Trans Am Frt. Fascia | Firebird Frt. Fascia
--- | --- | --- | --- | ---
Metric | English | Metric | English | Metric | English
F41(Base) | 235/55 | 443 mm | 17.4 in | -- | -- | 342 mm | 13.4 in
FE2(Z28, Trans Am Base) | 235/55 | 443 mm | 17.4 in | 416 mm | 16.3 in | -- | --
245/50 | 443 mm | 17.4 in | 416 mm | 16.3 in | -- | --
FE4 (Z28, Trans Am Special) | 245/50 | 443 mm | 17.4 in | 342 mm | 13.4 in | -- | --
FE7(Z-28 SS, B4C, WS6, Firm, HD) | 275/40 | 443 mm | 17.4 in | 342 mm | 13.4 in | -- | --

#### Trim Height Specifications (Rear Fascia)

Suspension | Tire | Camaro Rear Fascia | Fire/TA Rear Fascia | Side Rocker (All)
--- | --- | --- | --- | ---
Metric | English | Metric | English | Metric | English
F41(Base) | 235/55 | 367 mm | 14.4 in | 375 mm | 14.7 in | 204 mm (Front) 208 mm (Rear) | 8.0 (Front) 8.2 (Rear)
FE2(Z38, Trans Am Base) | 235/55 | 367 mm | 14.4 in | 375 mm | 14.7 in | 204 mm (Front) 208 mm (Rear) | 8.0 in (Front) 8.2 in (Rear)
245/50 | 367 mm | 14.4 in | 375 mm | 14.7 in | 204 mm (Front) 208 mm (Rear) | 8.0 in (Front) 8.2 in (Rear)
FE4(Z28, Trans Am Special | 245/50 | 367 mm | 14.4 in | 375 mm | 14.7 in | 204 mm (Front) 208 mm (Rear) | 8.0 in (Front) 8.2 in (Rear)
FE7 (Z-28 SS, B4C, WS6, Firm, HD) | 275/40 | 367 mm | 14.4 in | 375 mm | 14.7 in | 204 mm (Front,) 208 mm (Rear) | 8.0 in (Front) 8.2 in (Rear)