For 1990-2009 cars

# COLD ENGINE SPEED SAG W/ A/T ENGAGEMENT-PROM P/N PROVIDED

6000, Firebird, Grand Am, Fiero

Some 1985 vehicles with 2.5L-TBI engines with automatic transmissions may exhibit a deep sag in engine speed upon gear engagement after a cold start. Should such a condition be encountered that cannot be corrected by published service procedures, a new PROM may be installed (parts listed below).

#### Model Part Number ----- ----------- 6000 16051305 6000 LE 16051314 Firebird 16051323 Grand Am 16051333 Fiero 16051388

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.