For 1990-2009 cars

# No Oil Indicated On Dipstick (Replace Dipstick Tube and Dipstick)

Subject: | No Oil Indicated On Dipstick (Replace Dipstick Tube And Dipstick)

Models: | 1996-99 Chevrolet Camaro

| 1996-99 Pontiac Firebird

| with 3.8 L V6 engine (VIN K -- RPO L36)

### Condition

Some customers may comment on a no oil reading when checking the oil with the dipstick, even though the engine has oil in it.

### Cause

In certain cases, the dipstick may come in contact with the windage tray and deflect away from the oil in the crankcase. This may cause a no oil reading on the dipstick.

### Correction

Replace the dipstick and dipstick tube with new parts listed below. See figure for identification of prior dipstick tube and new dipstick tube.

### Parts Information

Part Number | Description
--- | ---
12564961 | Dipstick Tube - Replaces 24505124
24505407 | Indicator (Dipstick)

Parts are currently available from GMSPO.

### Warranty Information

For vehicles repaired under warranty, use:

Labor Operation | Description | Labor Time
--- | --- | ---
J0930 | Tube, Oil level indicator - replace | Use published labor operation time