For 1990-2009 cars

# PRE-DELIVERY INSPECTION OF FLOOR SHIFT DETENT ROD

Some 1982 Firebird models with automatic transmission may have been built with a broken shift lever detent rod. Please have your dealer personnel check for this condition during pre-delivery inspection and, if necessary, install a new detent rod (part number 10023591) as outlined in bulletin 82-T-48.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.