For 1990-2009 cars

## Ignition Coil and Ignition Coil Module Disassemble L36

### Disassembly Procedure

1. Remove the ignition coil bolts.
2. Remove the ignition coils and the seals from the ignition control module.
3. Remove the ignition control module from the ignition control module bracket.

## Ignition Coil and Ignition Coil Module Disassemble LT1

### Disassembly Procedure

1. Drill out the ignition coil bracket rivets.
2. Remove the ignition coil.
3. Remove the ignition coil module bolts.
4. Remove the ignition coil module.