For 1990-2009 cars

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Adapter Plate Plug | 27 | 20 | --
Adapter Plate to Transmission Case Bolts | 35 | 26 | --
Backup Lamp Switch | 27 | 20 | --
Clutch Fork Bolt | 25 | 18 | --
Clutch Housing to Adapter Plate Bolt | 35 | 26 | --
Computer Aided Gear Select Solenoid | 40 | 30 | --
Cover Plate Bolts | 20 | 15 | --
Extension Housing Plug | 27 | 20 | --
Extension Housing to Transmission Case Bolts | 35 | 26 | --
Reverse Idler Shaft Bracket Bolts | 25 | 18 | --
Reverse Lockout Assembly Bolt | 18 | 13 | --
Reverse Lockout Solenoid | 40 | 30 | --
Shifter Bolts | 20 | 15 | --
Shift Detent Assembly | 40 | 30 | --
Shift Lever Guide Bolts | 27 | 20 | --
Shift Guide Plate Bolts | 22 | 16 | --
Transmission Case Drain Plug | 18 | 13 | --
Transmission Case Fill Plug | 18 | 13 | --
Vehicle Speed Sensor Bolt | 10 | -- | 89

## Fastener Tightening Specifications F Car

Application | Specification
--- | ---
Metric | English
Adapter Plate Plug | 27 N·m | 20 lb ft
Adapter Plate to Transmission Case Bolts | 35 N·m | 26 lb ft
Backup Lamp Switch | 27 N·m | 20 lb ft
Computer Aided Gear Select Solenoid | 40 N·m | 30 lb ft
Cover Plate Bolts | 20 N·m | 15 lb ft
Extension Housing Plug | 27 N·m | 20 lb ft
Extension Housing to Transmission Case Bolts | 35 N·m | 26 lb ft
Neutral Return Cam Spring Retaining Bolt | 25 N·m | 18 lb ft
Reverse Idler Shaft Bracket Bolts | 25 N·m | 18 lb ft
Reverse Lockout Assembly Bolt | 18 N·m | 13 lb ft
Reverse Lockout Solenoid | 40 N·m | 30 lb ft
Shift Detent Assembly | 40 N·m | 30 lb ft
Shift Guide Plate Bolts | 22 N·m | 16 lb ft
Shift Lever Guide Bolts | 27 N·m | 20 lb ft
Transmission Case Drain Plug | 18 N·m | 13 lb ft
Transmission Case Fill Plug | 18 N·m | 13 lb ft

## Fastener Tightening Specifications Y Car

Application | Specification
--- | ---
Metric | English
Adapter Plate Plug | 27 N·m | 20 lb ft
Adapter Plate to Transmission Case Bolts | 48 N·m | 36 lb ft
Backup Lamp Switch | 27 N·m | 20 lb ft
Computer Aided Gear Select Solenoid | 40 N·m | 30 lb ft
Cover Plate Bolts | 20 N·m | 15 lb ft
Extension Housing Plug | 27 N·m | 20 lb ft
Extension Housing to Transmission Case Bolts | 48 N·m | 36 lb ft
Neutral Return Cam Spring Retaining Bolt | 25 N·m | 18 lb ft
Reverse Idler Shaft Bracket Bolts | 25 N·m | 18 lb ft
Reverse Lockout Assembly Bolt | 18 N·m | 13 lb ft
Reverse Lockout Solenoid | 40 N·m | 30 lb ft
Shift Detent Assembly | 40 N·m | 30 lb ft
Shift Guide Plate Bolts | 22 N·m | 16 lb ft
Shift Lever Guide Bolts | 27 N·m | 20 lb ft
Transmission Case Drain Plug | 18 N·m | 13 lb ft
Transmission Case Fill Plug | 18 N·m | 13 lb ft