For 1990-2009 cars

## Right Side View Engine Wiring Harness LT1

(1) | Canister Purge Solenoid Valve Electrical Connector
(2) | Injector Electrical Connector
(3) | Manifold Absolute Pressure Sensor Electrical Connector
(4) | Generator Electrical Connector
(5) | A/C Compressor Clutch Electrical Connector
(6) | Vacuum Tube
(7) | Engine Ground Terminal
(8) | Engine Wiring Harness Ground Nut
(9) | Knock Sensor Electrical Connector
(10) | Engine Wiring Harness Clamp Bolt
(11) | Engine Wiring Harness
(12) | Ignition Distributor Electrical Connector
(13) | Engine Wiring Harness Start Lead Nut
(14) | Engine Wiring Harness Start Lead
(15) | Engine Wiring Harness Start Lead Washer
(16) | Oxygen Sensor Electrical Connector
(17) | Manifold Absolute Pressure Sensor
(18) | Manifold Absolute Pressure Connector
(19) | Engine Wiring Harness
(20) | Throttle Position Sensor Electrical Connector
(21) | Idle Air Control Stepper Motor Electrical Connector

## Right Side View Engine Wiring Harness L36

Figure 1: |

(1) | Fuel Injector Connector
(2) | Charcoal Canister Connector
(3) | Canister Purge Solenoid Connector
(4) | Manifold Absolute Pressure Connector
(5) | Oxygen Sensor Connector
(6) | Transmission Bolts/Screws
(7) | Engine Wiring Harness Clips
(8) | Right Side Knock Sensor Connector
(9) | Right Side Engine Mount Bracket
(10) | Engine Wiring Harness Clips
(11) | Vacuum Tube
(12) | Vacuum Port

Figure 2: |

(1) | Engine Bracket
(2) | A/C Compressor Connector
(3) | Mass Air Flow Connector
(4) | Engine Temperature Sensor Connector
(5) | Engine Wiring Harness Clip
(6) | Engine Wiring Harness Clip Bolt
(7) | Throttle Position Sensor Connector
(8) | Idle Air Control Connector
(9) | Generator Connector