For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Battery | In the right front of the engine compartment | Harness Routing Views in Wiring Systems | --
Body Control Module (BCM) | Under the right side of the IP near the blower motor | Body Control System Component Views in Body Control Systems | Body Control System Connector End Views in Body Control Systems
Clutch Pedal Position (CPP) Switch | Mounted to the clutch pedal bracket | Cruise Control Component Views in Criuse Control | --
Generator (V6 VIN K) | On the front right side of the engine | Engine Electrical Component Views | Engine Electrical Connector End Views
Generator (V8 VIN G) | On the front left side of the engine | Instrument Panel, Gages, and Console Component Views in Instrument Cluster, Gauges and Console | Engine Electrical Connector End Views
Ignition Switch | Mounted near the base of the steering column | Engine Electrical Component Views | Engine Electrical Connector End Views
Instrument Cluster | On the left side of the IP | Instrument Panel, Gages, and Console Component Views in Instrument Cluster, Gauges and Console | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges, and Console
Park Neutral Position Switch | Under the center console, on the base of the shift control lever | Tilt Wheel/Column Component Views in Steering-Tilt | Engine Electrical Connector End Views
Powertrain Control Module (PCM) (V6 VIN K) | On the right side of the engine compartment, rear of the wheelhouse | Harness Routing Views in Wiring Systems | Powertrain Control Module Connector End Views in 3.8L Engine Controls
Powertrain Control Module (PCM) (V8 VIN G) | On the right side of the engine compartment, rear of the wheelhouse | Engine Controls Component Views in 5.7L Engine Controls | Powertrain Control Module Connector End Views in 5.7L Engine Controls
Starter Motor (V8 VIN G) | On the bottom right side of the engine | Engine Electrical Component Views | --
Starter Motor (V6 VIN K) | On the bottom left side of the engine | Engine Electrical Component Views | --
Starter Relay | In underhood electrical center 2 | -- | --
Starter Solenoid (V6 VIN K) | On the bottom left side of the engine, above the starter motor | Engine Electrical Component Views | --
Starter Solenoid (V8 VIN G) | On the bottom right side of the engine, above the starter motor | Engine Electrical Component Views | --
Underhood Electrical Center 2 | In the left front corner of the engine compartment | Harness Routing Views in Wiring Systems | --
C101 (10 cavities) | Engine to forward lamp harness, in the engine compartment, above the right wheelhouse | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C102 (1 cavity) | Engine to forward lamp harness, in the engine compartment, above the right wheelhouse | Harness Routing Views in Wiring Systems | --
C200A (17 cavities) | Forward lamp to IP harness, between the left kick panel and the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200B (18 cavities) | Forward lamp to IP harness, between the left kick panel and the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200D (48 cavities) | Part of the IP harness, between the left kick panel and the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C220 (10 cavities) | IP to engine harness, under the right side of the IP, behind the knee bolster | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G100 (V6 VIN K) | On the lower right side of the engine, above the A/C compressor | Harness Routing Views in Wiring Systems | --
G100 (V8 VIN G) | On the lower right side of the engine, above the starter solenoid | Harness Routing Views in Wiring Systems | --
G101 | In the engine compartment, attached to the front of the left wheelhouse | Harness Routing Views in Wiring Systems | --
P100 | Left side in the dash panel, engine to the passenger compartment | Harness Routing Views in Wiring Systems | --
P110 | Right side in the dash panel, engine to the passenger compartment | Harness Routing Views in Wiring Systems | --
S170 | In the forward lamp harness, approximately 13 cm (5.1 in) from G106 breakout | -- | --
S183 | In the forward lamp harness, approximately 10 cm (4 in) from the UH electrical center 1 breakout | -- | --