For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Remove all items that may obstruct the convertible top switch.
2. Lower both of the sun visors.
3. Release the 2 latches. One latch is located above each sun visor.
4. Turn the ignition switch to the RUN position.
5. Lower all of the side windows.
6. Move the folding top switch to the DOWN position.

The convertible top lowers quietly and smoothly with no binding.

Power Folding Top Does Not Open

2 | Move the folding top switch to the UP position. | The convertible top raises quietly and smoothly with no binding. | Power Folding Top Does Not Close