For 1990-2009 cars

Figure 1: |

#### Engine Component Locator View (Left Side)

(1) | Manifold Vacuum Source
(2) | Ignition Control Module (ICM) and Coils Assembly
(3) | HO2S Bank 1 Sensor 1 (Behind Exhaust Downtube)
(4) | Engine Oil Level Switch
(5) | Crankshaft Position Sensor
(6) | Exhaust Gas Recirculation (EGR) Valve
(7) | Mass Air Flow (MAF) Sensor

Figure 2: |

#### Engine Component Locator View (Right Side)

(1) | Fuel Pressure Regulator
(2) | Idle Air Control (IAC) Valve
(3) | Throttle Position (TP) Sensor
(4) | Engine Coolant Temperature (ECT) Sensor
(5) | Camshaft Position (CMP) Sensor
(6) | EVAP Canister Purge Solenoid Valve
(7) | Heated Oxygen Sensor (HO2S) Bank2 Sensor1
(8) | Fuel Injectors
(9) | Manifold Absolute Pressure (MAP) Sensor
(10) | Positive Crankcase Ventilation (PCV) Valve

Figure 3: |

#### Lower Left Side of Engine (V6 VIN K)

(1) | Starter solenoid
(2) | Starter motor
(3) | Oil level switch
(4) | Lower control arm
(5) | Steering gear
(6) | Left engine mount

Figure 4: |

#### Front Left Side of Engine (V6 VIN K)

(1) | Generator