For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Disconnect the electrical connector (1) from the vehicle speed sensor (2).
3. Remove the attaching bolt and the vehicle speed sensor.
4. Remove the vehicle speed sensor.

### Installation Procedure

1. Install the vehicle speed sensor.
2. Install the vehicle speed sensor bolt.

Tighten
Tighten the vehicle speed sensor bolt to 10 N·m (89 lb in).

3. Install the electrical connector (1) on the vehicle speed sensor (2).
4. Lower the vehicle.