For 1990-2009 cars

Figure 1: |

#### Component Locator View

(1) | Case Assembly
(2) | Reverse Input Clutch
(3) | Input Clutch Housing
(4) | Overrun Clutch
(5) | Forward Clutch
(6) | Forward Sprag Clutch Assembly
(7) | 3-4 Clutch
(8) | Input Planetary Gear Set
(9) | Lo and Reverse Clutch
(10) | Lo Roller Clutch Assembly
(11) | Reaction Planetary Gear Set
(12) | Output Shaft
(13) | Speed Sensor
(14) | Parking Pawl
(15) | Parking Lock Actuator Assembly
(16) | Control Valve Assembly
(17) | Manual Shaft
(18) | Inside Detent Lever
(19) | 2-4 Band Assembly
(20) | Pump Assembly
(21) | Stator Roller Clutch
(22) | Torque Converter Assembly
(23) | Turbine Shaft

Figure 2: |

#### Case and Associated Parts 1 of 2

(1) | Torque Converter Assembly
(2) | Bolt, Pump to Case
(3) | O-Ring, Pump to Case Bolt
(4) | Pump Assembly, Oil
(5) | Seal, Oil (Pump to Case)
(6) | Gasket, Pump Cover to Case
(7) | Bushing, Case
(8) | Case, Transmission
(9) | Vent Assembly, Transmission
(10) | Connector, Oil Cooler Pipe
(11) | Plug, Case Servo
(12) | Spring, Servo Return
(13) | Pin, 2nd Apply Piston
(14) | Ring, Retainer (2nd Apply Piston)
(15) | Retainer, Servo Cushion Spring
(16) | Spring, Servo Cushion (Outer)
(17) | Piston, 2nd Apply
(18) | Ring, Oil Seal (2nd Apply Piston - Outer)
(19) | Ring, Oil Seal (2nd Apply Piston - Inner)
(20) | Housing, Servo Piston (Inner)
(21) | Seal, O-Ring
(22) | Spring, Servo Apply Pin
(23) | Washer, Servo Apply Pin
(24) | Ring, Retainer (Apply Pin)
(25) | Piston, 4th Apply
(26) | Ring, Oil Seal (4th Apply Piston - Outer)
(27) | Seal, O-Ring (2-4 Servo Cover)
(28) | Cover, 2-4 Servo
(29) | Ring, Servo Cover Retaining
(30) | Seal, Case Extension to Case
(31) | Extension, Case
(31) | Extension, Case
(32) | Bolt, Case Extension to Case
(33) | Bushing, Case Extension
(34) | Seal Assembly, Case Extension Oil
(35) | Bolt, Speed Sensor Retaining
(36) | Speed Sensor, Internal Transmission
(37) | Seal, O-Ring (ITSS to Case Extension)
(71) | Seal, Filter
(72) | Filter Assembly, Transmission Oil
(73) | Gasket, Transmission Oil Pan
(73) | Gasket, Transmission Oil Pan
(74) | Magnet, Chip Collector
(75) | Pan, Transmission Oil
(75) | Pan, Transmission Oil
(76) | Screw, Transmission Oil Pan
(76) | Screw, Transmission Oil Pan
(94) | Bolt, Converter Housing to Case
(95) | Connector, Oil Cooler Quick
(96) | Clip, Oil Cooler Quick Connect
(97) | Plug, Converter Housing Access Hole
(98) | Plate, Converter Bolt Inspection
(99) | Plug, Cup D4 Orifice
(100) | Stud, A/Trans. Case
(101) | Plug Asm., A/Trans. Oil Pan
(102) | Housing, Converter
(102) | Housing, Converter
(103) | Case, Main Section
(103) | Case, Main Section
(105) | Spring, Servo Cushion (Inner)
(106) | Seal Assembly, Case Oil (Y-Car Only)

Figure 3: |

#### Case and Associated Parts 2 of 2

(38) | Plug, Transmission Case (Accumulator Bleed)
(39) | Plug, Pressure
(40) | Retainer and Ball Assembly, Third Accumulator
(41) | Pin, Band Anchor
(42) | Retainer and Ball Assembly (Double Orifice)
(43) | Pin, Accumulator Piston
(44) | Piston, 3-4 Accumulator
(45) | Ring, Oil Seal (3-4 Accumulator Piston)
(46) | Spring, 3-4 Accumulator
(47) | Gasket, Spacer Plate to Case
(48) | Plate, Valve Body Spacer
(49) | Screen, Shift Solenoids
(50) | Screen, Pressure Control Solenoid
(52) | Gasket, Spacer Plate to Valve Body
(53) | Plate, Spacer Plate Support
(54) | Spring, 1-2 Accumulator
(55) | Ring, Oil Seal (1-2 Accumulator)
(56) | Piston, 1-2 Accumulator
(57) | Cover and Pin Assembly, 1-2 Accumulator
(58) | Bolt, Accumulator Cover
(59) | Bolt, Accumulator Cover
(60) | Valve Assembly, Control Body
(61) | Checkball
(62) | Bolt, Valve Body
(63) | Spring Assembly, Manual Detent
(64) | Bolt, Manual Detent Spring
(65) | Seal, Wiring Harness Pass-through Connector O-Ring
(66) | Solenoid Assembly, Wiring Harness
(67) | Seal, O-Ring (Solenoid)
(68) | Bolt, Hex Washer Head (Solenoid)
(69) | Switch Assembly, Transmission Pressure
(70) | Bolt, Pressure Switch Assembly
(77) | Bolt, Spacer Plate Support
(91) | Number 10 Checkball
(93) | Bracket, Dipstick Stop
(104) | Spring, 1-2 Accumulator (Inner)

Figure 4: |

#### Oil Pump Assembly

(200) | Body, Pump
(201) | Ring, Oil Seal (Slide to Wear Plate)
(202) | Seal, O-Ring (Slide Seal Back-Up)
(203) | Slide, Pump
(204) | Spring, Pivot Pin
(205) | Pin, Pivot Slide
(206) | Spring, Pump Slide (Outer)
(207) | Spring, Pump Slide (Inner)
(208) | Support, Pump Slide Seal
(209) | Seal, Pump Slide
(210) | Ring, Pump Vane
(210) | Ring, Pump Vane
(211) | Guide, Rotor
(212) | Rotor, Oil Pump
(213) | Vane, Pump
(214) | Shaft, Stator
(215) | Cover, Pump
(216) | Valve, Pressure Regulator
(217) | Spring, Pressure Regulator Valve
(218) | Spring, Pressure Regulator Isolator
(219) | Valve, Reverse Boost
(220) | Sleeve, Reverse Boost Valve
(221) | Ring, Oil Pump Reverse Boost Valve Retaining
(222) | Ring, Oil Pump Converter Clutch Valve Retaining
(223) | Valve, Stop
(224) | Valve, Converter Clutch
(225) | Spring, Converter Clutch Valve (Inner)
(226) | Spring, Converter Clutch Valve (Outer)
(227) | Rivet, Pressure Relief Bolt
(228) | Ball, Pressure Relief
(229) | Spring Pressure Relief
(230) | Ring, Oil Seal (Stator Shaft)
(231) | Seal, Oil Pump Cover Screen
(232) | Screen, Oil Pump Cover
(233) | Bolt, M8 X 1.25 X 40 (Cover to Body)
(234) | Bushing, Stator Shaft (Front)
(235) | Plug, Oil Pump Cover (FWD Clutch Feed)
(236) | Plug, Oil Pump Cover
(236) | Plug, Oil Pump Cover
(236) | Plug, Oil Pump Cover
(236) | Plug, Oil Pump Cover
(236) | Plug, Oil Pump Cover
(236) | Plug, Oil Pump Cover
(237) | Retainer and Ball Assembly, Check Valve
(237) | Retainer and Ball Assembly, Check Valve
(238) | Orifice, Converter Clutch Signal (Cup Plug)
(240) | Plug, Cup Orifice
(241) | Bushing, Stator Shaft (Rear)
(242) | Bushing, Pump Body
(243) | Seal Assembly, Oil
(244) | Retainer, Front Helix

Figure 5: |

#### Control Valve Body Assembly (1 of 2)

(350) | Control Valve Body Assembly
(353) | Seal, Forward Accumulator Oil
(354) | Piston, Forward Accumulator
(355) | Pin, Forward Accumulator
(356) | Spring, Forward Accumulator
(357) | Valve, Forward Abuse
(358) | Spring, Forward Abuse Valve
(359) | Plug, Bore
(360) | Pin, Coiled Spring
(360) | Pin, Coiled Spring
(361) | Valve, Low Overrun
(362) | Spring, Low Overrun Valve
(363) | Cover, Forward Accumulator
(364) | Bolt, Forward Accumulator Cover
(364) | Bolt, Forward Accumulator Cover
(365) | Spring, 1-2 Shift Valve
(366) | Valve, 1-2 Shift
(367a) | 1-2 Shift Solenoid Valve
(367b) | 2-3 Shift Solenoid Valve
(368) | Valve, 2-3 Shift
(369) | Valve, 2-3 Shuttle
(370) | Spring, 1-2 Accumulator Valve
(371) | Valve, 1-2 Accumulator
(372) | Sleeve, 1-2 Accumulator Valve
(374) | Valve, Actuator Feed Limit
(375) | Spring, Actuator Feed Limit Valve
(376) | Plug, Bore
(377) | Pressure Control Solenoid Valve
(378) | Retainer, Pressure Control Solenoid
(379) | Retainer, Solenoid
(379) | Retainer, Solenoid
(395) | Retainer, Bore Plug

Figure 6: |

#### Control Valve Body Assembly (2 of 2)

(340) | Manual Valve
(350) | Control Valve Body Assembly
(359) | Bore Plug
(360) | Pin, Coiled Spring
(379) | Retainer, Solenoid
(379) | Retainer, Solenoid
(380) | Valve, Regulator Apply
(381) | Bore Plug
(381) | Bore Plug
(381) | Bore Plug
(381) | Bore Plug
(382) | Spring, 4-3 Sequence Valve
(383) | Valve, 4-3 Sequence
(384) | Valve, 3-4 Relay
(385) | Valve, 3-4 Shift
(386) | Spring, 3-4 Shift Valve
(387) | Valve, Reverse Abuse
(388) | Spring, Reverse Abuse Valve
(389) | Valve, 3-2 Downshift
(390) | Spring, 3-2 Downshift Valve
(391) | Valve, 3-2 Control
(392) | Spring, 3-2 Control Valve
(394) | 3-2 Control Solenoid
(395) | Retainer, Bore Plug
(395) | Retainer, Bore Plug
(395) | Retainer, Bore Plug
(395) | Retainer, Bore Plug
(396) | TCC PWM Solenoid Valve
(397) | Spring, Regulator Apply
(398) | Valve, Isolator

Figure 7: |

#### Internal Parts 1 of 2

(600) | Spring Asm., 3-4 Clutch Boost (5)
(601) | Washer, Thrust (Pump to Drum)
(602) | Band Assembly, 2-4
(603) | Bushing, Reverse Input Clutch (Front)
(605) | Housing and Drum Assembly, Reverse Input Clutch
(606) | Bushing, Reverse Input Clutch (Rear)
(607) | Piston Asm., Reverse Input Clutch
(608) | Seals, Reverse Input Clutch (Inner and Outer)
(609) | Spring Asm., Reverse Input Clutch
(610) | Ring, Reverse Input Clutch Spring Retainer
(611) | Plate, Reverse Input Clutch (Belleville)
(612a) | Plate, Reverse Input Clutch Turbulator (Steel)
(612b) | Plate Asm., Reverse Input Clutch (Fiber)
(613) | Plate, Reverse Input Clutch Backing (Selective)
(614) | Ring, Reverse Input Clutch Retaining
(615) | Bearing Assembly, Stator Shaft/Selective Washer
(616) | Washer, Thrust (Selective)
(617) | Retainer and Ball Asm., Check Valve
(618) | Seal, O-Ring (Turbine Shaft/Selective Washer)
(619) | Ring, Oil Seal (Solid)
(620) | Retainer and Checkball Assembly
(620) | Retainer and Checkball Assembly
(621) | Housing and Shaft Assembly, Input
(622) | Seal, O-Ring Input to Forward Clutch Housing
(623) | Piston, 3rd and 4th Clutch
(625) | Ring, 3rd and 4th Clutch (Apply)
(626) | Spring Assembly, 3rd and 4th Clutch
(627) | Retainer and Ball Assembly, Forward Clutch Housing
(628) | Housing, Forward Clutch
(630) | Piston, Forward Clutch
(632) | Piston, Overrun Clutch
(633) | Ball, Overrun Clutch
(634) | Spring Assembly, Overrun Clutch
(635) | Snap Ring, Overrun Clutch Spring Retainer
(636) | Seal, Input Housing to Output Shaft
(637) | Bearing Assembly, Input Sun Gear
(638) | Snap Ring, Overrun Clutch Hub Retaining
(639) | Hub, Overrun Clutch
(641) | Retainer and Race Assembly, Sprag
(641) | Retainer and Race Assembly, Sprag
(642) | Forward Sprag Assembly
(643) | Retainer Rings, Sprag Assembly
(643) | Retainer Rings, Sprag Assembly
(644) | Race, Forward Clutch (Outer)
(645a) | Plate Assembly, Overrun Clutch (Steel)
(645b) | Plate, Overrun Clutch (Fiber)
(646) | Plate, Forward Clutch (Apply)
(648) | Plate, Forward Clutch (Waved)
(649a) | Plate Assembly, Forward Clutch (Steel)
(649b) | Plate, Forward Clutch (Fiber)
(650) | Plate, Forward Clutch Backing (Selective)
(651) | Ring, Forward Clutch Backing Plate Retainer
(653) | Plate, 3rd and 4th Clutch Apply (Stepped)
(654a) | Plate Assembly, 3rd and 4th Clutch (Fiber)
(654b) | Plate, 3rd and 4th Clutch (Steel)
(655) | Plate, 3rd and 4th Clutch Backing (Selective)
(656) | Ring, 3rd and 4th Clutch Backing Plate Retainer
(698) | Plug, Orificed Cup

Figure 8: |

#### Internal Parts 2 of 2

(7) | Bushing, Case
(657) | Bushing, Input Sun Gear Front
(658) | Gear, Input Sun
(659) | Bushing, Input Sun Gear Rear
(661) | Retainer, Output Shaft to Input Carrier
(662) | Carrier Assembly, Input
(663) | Bearing Assembly, Thrust (Input Carrier to Reaction Shaft)
(664) | Gear, Input Internal
(665) | Bushing, Reaction Carrier Shaft Front
(666) | Shaft, Reaction Carrier
(667) | Bushing, Reaction Carrier Shaft Rear
(668) | Retainer Ring, Reaction Shaft/Internal Gear
(669) | Washer, Thrust (Reaction Shaft Shell)
(670) | Shell, Reaction Sun
(671) | Retainer Ring, Reaction Sun Gear
(672) | Bushing, Reaction Sun
(673) | Gear, Reaction Sun
(674) | Washer, Thrust (Race/Reaction Shell)
(675) | Race, Lo and Reverse Roller Clutch
(676) | Retainer Ring, Lo and Reverse Support to Case
(677) | Retainer Ring, Lo and Reverse Roller Assembly (Cam)
(677) | Retainer Ring, Lo and Reverse Roller Assembly (Cam)
(678) | Clutch Assembly, Lo and Reverse Roller
(679) | Support Assembly, Lo and Reverse Clutch
(680) | Spring, Lo and Reverse Clutch Support Retainer
(681) | Carrier Assembly, Reaction
(682a) | Plate, Lo and Reverse Clutch (Waved)
(682b) | Plate, Spacer Lo and Reverse Clutch (Selective)
(682c) | Plate Assembly, Lo and Reverse Clutch (Fiber)
(682d) | Plate, Lo and Reverse Clutch Turbulator (Steel)
(683) | Bearing Assembly, Thrust (Reaction Carrier/Support)
(684) | Gear, Internal Reaction
(685) | Support, Internal Reaction Gear
(686) | Retainer Ring, Reaction Gear/Support
(687) | Shaft, Output
(690) | Sleeve, Output Shaft
(691) | Seal, Output Shaft
(692) | Bearing, Reaction Gear Support to Case
(693) | Retainer Ring, Lo and Reverse Clutch
(694) | Spring Assembly, Lo and Reverse Clutch
(695) | Piston, Lo and Reverse Clutch
(696) | Seal, Lo and Reverse Clutch (Outer, Center and Inner)
(697) | Deflector, Oil (High Output Models Only)
(699) | Rotor, Internal Transmission Speed Sensor

Figure 9: |

#### Parking Lock and Manual Shift Shaft Assembly

(78) | Steel Cup Plug
(79) | Parking Brake Pawl Shaft
(80) | Parking Pawl Return Spring
(81) | Parking Brake Pawl
(82) | Manual Shaft Seal
(83) | Manual Shaft Retainer
(84) | Manual Shaft (Model Dependent)
(85) | Parking Lock Actuator Assembly
(86) | Parking Lock Bracket
(87) | Parking Lock Bracket (2) Bolt
(88) | Inside Detent Lever
(89) | Manual Valve Link
(90) | Hex Head Nut

Figure 10: |

#### Seal Locations

(3) | O-Ring, Pump to Case Bolt
(5) | Seal, Oil (Pump to Case)
(18) | Ring, Oil Seal (2nd Apply Piston-Outer)
(19) | Ring, Oil Seal (2nd Apply Piston-Inner)
(21) | Seal, O-Ring
(26) | Ring, Oil Seal (4th Apply Piston-Outer)
(27) | Seal, O-Ring (2-4 Servo Cover)
(30) | Seal, Case Extension to Case
(34) | Seal Assembly, Case Extension Oil
(37) | Seal, O-Ring (ITSS to Case Extension)
(106) | Seal Assembly, Case Oil (Y-Car Only)
(230) | Ring, Oil Seal (Stator Shaft)
(243) | Seal Assembly, Oil
(608) | Seals, Reverse Input Clutch (inner and outer)
(608) | Seals, Reverse Input Clutch (inner and outer)
(618) | Seal, O-Ring (Turbine Shaft/Selective Washer)
(619) | Ring, Oil Seal (Solid)
(622) | Seal, O-Ring Input to Forward Housing
(623) | Piston, 3rd and 4th Clutch
(630) | Piston, Forward Clutch
(632) | Piston, Overrun Clutch
(636) | Seal, Input Housing to Output Shaft
(691) | Seal, Output Shaft (Model Dependent)
(696) | Seal, Transmission (Low and Reverse Clutch-Outer, Center, Inner
(696) | Seal, Transmission (Lo and Reverse Clutch-Outer, Center, Inner
(696) | Seal, Transmission (Lo and Reverse Clutch-Outer, Center, Inner

Figure 11: |

#### Bearings and Bushings

(7) | Case Bushing
(33) | Case Extension Bushing
(234) | Stator Shaft Bushing (Front)
(241) | Stator Shaft Bushing (Rear)
(242) | Oil Pump Body Bushing
(601) | Thrust Washer (Pump to Drum)
(603) | Reverse Input Cl. Bushing (Front)
(606) | Reverse Input Clutch Bushing (Rear)
(615) | Stator Shaft/Selective Washer Bearing Assembly
(616) | Thrust Washer (Selective)
(637) | Input Sun Gear Bearing Assembly
(657) | Input Sun Gear Bushing (Front)
(659) | Input Sun Gear Bushing (Rear)
(663) | Thrust Bearing Assembly (Input Carrier to Reaction Shaft)
(665) | Reaction Carrier Shaft Bushing (Front)
(667) | Reaction Carrier Shaft Bushing (Rear)
(669) | Thrust Washer (Reaction Shaft/Shell)
(672) | Reaction Gear Bushing
(674) | Thrust Washer (Race/Reaction Shell)
(683) | Thrust Bearing Assembly (Reaction Carrier/Support)
(692) | Reaction Gear Support to Case Bearing

Figure 12: |

#### Valve Trains

(340) | Valve, Manual
(353) | Seal, Forward Accumulator Oil
(354) | Piston, Forward Accumulator
(355) | Pin, Forward Accumulator
(356) | Spring, Forward Accumulator
(357) | Valve, Forward Abuse
(358) | Spring, Forward Abuse Valve
(359) | Plug, Bore
(359) | Plug, Bore
(360) | Pin, Coiled Spring
(360) | Pin, Coiled Spring
(360) | Pin, Coiled Spring
(361) | Valve, Low Overrun
(362) | Spring, Low Overrun Valve
(363) | Cover, Forward Accumulator
(364) | Bolt, Forward Accumulator Cover
(364) | Bolt, Forward Accumulator Cover
(365) | Spring, 1-2 Shift Valve
(366) | Valve, 1-2 Shift
(367) | Shift Solenoid Valve
(367) | Shift Solenoid Valve
(368) | Valve, 2-3 Shift
(369) | Valve, 2-3 Shuttle
(370) | Spring, 1-2 Accumulator Valve
(371) | Valve, 1-2 Accumulator
(372) | Sleeve, 1-2 Accumulator Valve
(374) | Valve, Actuator Feed Limit
(375) | Spring, Actuator Feed Limit Valve
(376) | Plug, Bore
(377) | Pressure Control Solenoid
(378) | Retainer, Pressure Control Solenoid
(379) | Retainer, Solenoid
(379) | Retainer, Solenoid
(379) | Retainer, Solenoid
(379) | Retainer, Solenoid
(380) | Valve, Converter Clutch Signal
(381) | Plug, Bore
(381) | Plug, Bore
(381) | Plug, Bore
(381) | Plug, Bore
(382) | Spring, 4-3 Sequence Valve
(383) | Valve, 4-3 Sequence
(384) | Valve, 3-4 Relay
(385) | Valve, 3-4 Shift
(386) | Spring, 3-4 Shift Valve
(387) | Valve, Reverse Abuse
(388) | Spring, Reverse Abuse Valve
(389) | Valve, 3-2 Downshift
(390) | Spring, 3-2 Downshift Valve
(391) | Valve, 3-2 Control
(392) | Spring, 3-2 Control Valve
(394) | 3-2 Control Solenoid
(395) | Retainer, Bore Plug
(395) | Retainer, Bore Plug
(395) | Retainer, Bore Plug
(395) | Retainer, Bore Plug
(395) | Retainer, Bore Plug
(396) | TCC PWM Solenoid Valve
(397) | Spring, Regulator Apply
(398) | Valve, Isolator

Figure 13: |

#### Control Valve Body Passages (Case Side)

(#2) | Checkball (61)
(#3) | Checkball (61)
(#4) | Checkball (61)
(#5) | Checkball (61)
(#6) | Checkball (61)
(#8) | Checkball (61)
(#12) | Checkball (61)
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(12) | PR
(12) | PR
(12) | PR
(13) | D4-3-2
(13) | D4-3-2
(14) | Lo/Reverse
(14) | Lo/Reverse
(15) | Reverse
(15) | Reverse
(15) | Reverse
(16) | Reverse Input (Rev. Cl.)
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(20) | Accumulator
(20) | Accumulator
(22) | Signal A
(22) | Signal A
(23) | Signal B
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(26) | C.C. Signal
(26) | C.C. Signal
(27) | 3-4 Signal
(27) | 3-4 Signal
(28) | 3rd Accumulator
(28) | 3rd Accumulator
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(30) | 4th Signal
(30) | 4th Signal
(31) | Servo Feed
(31) | Servo Feed
(31) | Servo Feed
(32) | 4th
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(35) | Overrun
(35) | Overrun
(36) | Overrun Clutch Feed
(37) | Overrun Clutch
(38) | D2
(38) | D2
(38) | D2
(40) | 3-2 Signal
(40) | 3-2 Signal
(41) | Lo
(41) | Lo
(41) | Lo
(42) | Lo/1st
(42) | Lo/1st
(42) | Lo/1st
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void

Figure 14: |

#### Spacer Plate to Control Valve Body Gasket

(3) | Line
(3) | Line
(3) | Line
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(13) | D4-3-2
(13) | D4-3-2
(14) | Lo/Reverse
(14) | Lo/Reverse
(14) | Lo/Reverse
(15) | Reverse
(15) | Reverse
(15) | Reverse
(16) | Reverse Input (Rev. Cl.)
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(20) | Accumulator
(20) | Accumulator
(20) | Accumulator
(21) | Orificed Accumulator
(22) | Signal A
(22) | Signal A
(22) | Signal A
(23) | Signal B
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(26) | C.C. Signal
(26) | C.C. Signal
(27) | 3-4 Signal
(27) | 3-4 Signal
(28) | 3rd Accumulator
(28) | 3rd Accumulator
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(30) | 4th Signal
(30) | 4th Signal
(31) | Servo Feed
(31) | Servo Feed
(31) | Servo Feed
(32) | 4th
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(35) | Overrun
(35) | Overrun
(35/39) | Overrun/Orificed D2
(36) | Overrun Clutch Feed
(37) | Overrun Clutch
(38) | D2
(38) | D2
(38) | D2
(38) | D2
(38) | D2
(40) | 3-2 Signal
(40) | 3-2 Signal
(41) | Lo
(41) | Lo
(41) | Lo
(41) | Lo
(42) | Lo/1st
(42) | Lo/1st
(43) | Exhaust
(43) | Exhaust
(44) | Orificed Exhaust
(44) | Orificed Exhaust
(47) | Void

Figure 15: |

#### Spacer Plate Passages

(49) | Shift Solenoids Screen
(50) | Pressure Control Solenoid Screen
(3) | Line
(3) | Line
(3) | Line
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9/10) | Actuator Feed Limit/Filtered Actuator Feed
(9/10) | Actuator Feed Limit/Filtered Actuator Feed
(9/10) | Actuator Feed Limit/Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10/22) | Filtered Actuator Feed/Signal A
(10/23) | Filtered Actuator Feed/Signal B
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(13) | D4-3-2
(13) | D4-3-2
(14) | Lo/Reverse
(14) | Lo/Reverse
(14) | Lo/Reverse
(15) | Reverse
(15) | Reverse
(15/16) | Reverse/Reverse Input (Rev. Cl.)
(15/16) | Reverse/Reverse Input (Rev. Cl.)
(16) | Reverse Input (Rev. Cl.)
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(17/18) | D4
(17/18) | D4
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(20) | Accumulator
(20) | Accumulator
(20) | Accumulator
(20/21) | Accumulator/Orificed Accumulator
(20/21) | Accumulator/Orificed Accumulator
(21) | Orificed Accumulator
(22) | Signal A
(22) | Signal A
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24/25) | 2nd/2nd Clutch
(24/25) | 2nd/2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(26) | C.C. Signal
(26) | C.C. Signal
(27) | 3-4 Signal
(27) | 3-4 Signal
(27/29) | 3-4 Signal
(27/29) | 3-4 Signal
(28) | 3rd Accumulator
(29/28) | 3-4 Clutch/3rd Accumulator
(29/28) | 3-4 Clutch/3rd Accumulator
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(30) | 4th Signal
(30) | 4th Signal
(30) | 4th Signal
(31) | Servo Feed
(31) | Servo Feed
(31) | Servo Feed
(32) | 4th
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(35a) | Overrun
(35) | Overrun
(35/36) | Overrun/Overrun Clutch Feed
(35/36) | Overrun/Overrun Clutch Feed
(35/39) | Overrun/Orificed D2
(36) | Overrun Clutch Feed
(37) | Overrun Clutch
(38) | D2
(38) | D2
(38) | D2
(38) | D2
(38/39) | D2/Orificed D2
(40) | 3-2 Signal
(40) | 3-2 Signal
(41) | Lo
(41) | Lo
(41) | Lo
(41) | Lo
(42) | Lo/1st
(42) | Lo/1st
(43) | Exhaust
(43/44) | Exhaust/Orificed Exhaust
(43/44) | Exhaust/Orificed Exhaust
(44) | Orificed Exhaust
(47) | Void

Figure 16: |

#### Spacer Plate to Case Gasket

(3) | Line
(3) | Line
(3) | Line
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(13) | D4-3-2
(13) | D4-3-2
(14) | Lo/Reverse
(14) | Lo/Reverse
(14) | Lo/Reverse
(15) | Reverse
(15) | Reverse
(16) | Reverse Input (Rev. Cl.)
(16) | Reverse Input (Rev. Cl.)
(16) | Reverse Input (Rev. Cl.)
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(20) | Accumulator
(20) | Accumulator
(20) | Accumulator
(20) | Accumulator
(21) | Orificed Accumulator
(21) | Orificed Accumulator
(22) | Signal A
(22) | Signal A
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(26) | C.C. Signal
(26) | C.C. Signal
(27) | 3-4 Signal
(27) | 3-4 Signal
(27) | 3-4 Signal
(28) | 3rd Accumulator
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(30) | 4th Signal
(30) | 4th Signal
(31) | Servo Feed
(31) | Servo Feed
(31) | Servo Feed
(32) | 4th
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(35) | Overrun
(35) | Overrun
(36) | Overrun Clutch Feed
(36) | Overrun Clutch Feed
(37) | Overrun Clutch
(38) | D2
(38) | D2
(38) | D2
(38) | D2
(39) | Orificed D2
(39) | Orificed D2
(40) | 3-2 Signal
(40) | 3-2 Signal
(41) | Lo
(41) | Lo
(41) | Lo
(41) | Lo
(42) | Lo/1st
(42) | Lo/1st
(43) | Exhaust
(43) | Exhaust
(44) | Orificed Exhaust
(44) | Orificed Exhaust

Figure 17: |

#### Case Passages (Control Valve Body Side)

(#1) | Checkball (91)
(#7) | 3rd Accum. Retainer and Ball Assembly (40)
(#10) | Checkball (42)
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(13) | D4-3-2
(13) | D4-3-2
(14) | Lo/Reverse
(14) | Lo/Reverse
(14) | Lo/Reverse
(15) | Reverse
(16) | Reverse Input (Rev. Cl.)
(16) | Reverse Input (Rev. Cl.)
(16) | Reverse Input (Rev. Cl.)
(16) | Reverse Input (Rev. Cl.)
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(19) | Rear Lube
(20) | Accumulator
(21) | Orificed Accumulator
(22) | Signal A
(22) | Signal A
(22) | Signal A
(24) | 2nd
(24) | 2nd
(24) | 2nd
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(26) | C.C. Signal
(26) | C.C. Signal
(27) | 3-4 Signal
(27) | 3-4 Signal
(28) | 3rd Accumulator
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(30) | 4th Signal
(31) | Servo Feed
(32) | 4th
(32) | 4th
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(35) | Overrun
(35) | Overrun
(36) | Overrun Clutch Feed
(36) | Overrun Clutch Feed
(37) | Overrun Clutch
(37) | Overrun Clutch
(37) | Overrun Clutch
(38) | D2
(38) | D2
(38) | D2
(38) | D2
(39) | Orificed D2
(40) | 3-2 Signal
(41) | Lo
(41) | Lo
(41) | Lo
(42) | Lo/1st
(42) | Lo/1st
(43) | Exhaust
(43) | Exhaust
(44) | Orificed Exhaust
(44) | Orificed Exhaust
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void

Figure 18: |

#### 2-4 Servo Fluid Passages

(#7) | 3rd Accumulator Retainer and Ball Assembly (40)
(#7) | 3rd Accumulator Retainer and Ball Assembly (40)
(11) | Case Servo Orificed Plug
(11) | Case Servo Orificed Plug
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(28) | 3rd Accumulator
(28) | 3rd Accumulator
(28) | 3rd Accumulator
(32) | 4th
(32) | 4th
(32) | 4th
(32) | 4th
(43) | Exhaust
(43) | Exhaust
(44) | Orificed Exhaust
(44) | Orificed Exhaust

Figure 19: |

#### Pump Cover Passages: Case Side

(232) | Oil Pump Cover Screen
(237) | Check Valve Retainer and Ball Assembly
(237) | Check Valve Retainer and Ball Assembly
(240) | Orificed Cup Plug
(240) | Orificed Cup Plug
(1) | Suction (Intake)
(2) | Decrease
(2) | Decrease
(3) | Line
(3) | Line
(3) | Line
(5) | Release
(7) | To Cooler
(8) | Lube from Cooler
(8) | Lube from Cooler
(11) | Torque Signal
(16) | Reverse Input (Rev. Cl.)
(16) | Reverse Input (Rev. Cl.)
(16) | Reverse Input (Rev. Cl.)
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(26) | C.C. Signal
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(37) | Overrun Clutch
(37) | Overrun Clutch
(37) | Overrun Clutch
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(45) | Vent
(46) | Seal Drain
(47) | Void
(47) | Void

Figure 20: |

#### Pump Cover Passages

(1) | Suction (intake)
(1) | Suction (intake)
(2) | Decrease
(2) | Decrease
(2) | Decrease
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(4) | Converter Feed
(4) | Converter Feed
(4) | Converter Feed
(4) | Converter Feed
(5) | Release
(5) | Release
(7) | To Cooler
(8) | Lube from Cooler
(8) | Lube from Cooler
(11) | Torque Signal
(16) | Reverse Input
(16) | Reverse Input
(16) | Reverse Input
(18) | Forward Clutch Feed
(26) | C.C. Signal
(26) | C.C. Signal
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(37) | Overrun Clutch
(37) | Overrun Clutch
(37) | Overrun Clutch
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(45) | Vent
(46) | Seal Drain
(47) | Void
(47) | Void
(47) | Void

Figure 21: |

#### Pump Body Passages

(1) | Suction (intake)
(2) | Decrease
(2) | Decrease
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(4) | Converter Feed
(4) | Converter Feed
(4) | Converter Feed
(4) | Converter Feed
(5) | Release
(7) | To Cooler
(8) | Lube from Cooler
(11) | Torque Signal
(16) | Reverse Input
(16) | Reverse Input
(26) | C.C. Signal
(29) | 3-4 Clutch
(37) | Overrun Clutch
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(45) | Vent
(46) | Seal Drain
(47) | Void
(47) | Void