For 1990-2009 cars

Figure 1: |

#### Components

(1) | Converter Housing
(2) | Reverse Input Clutch
(3) | Input Clutch Housing
(4) | Overrun Clutch
(5) | Forward Clutch
(6) | Forward Sprag Clutch Assembly
(7) | 3-4 Clutch
(8) | Input Planetary Gear Set
(9) | Lo and Reverse Clutch
(10) | Lo Roller Clutch Assembly
(11) | Reaction Planetary Gear Set
(12) | Speed Sensor
(13) | Output Shaft
(14) | Case Extension
(15) | Main Section Case
(16) | Parking Pawl
(17) | Parking Lock Actuator Assembly
(18) | Control Valve Assembly
(19) | Manual Shaft
(20) | Inside Detent Lever
(21) | 2-4 Band Assembly
(22) | Pump Assembly
(23) | Stator Roller Clutch
(24) | Torque Converter Assembly
(25) | Turbine Shaft

Figure 2: |

#### Case and Associated Parts (1 of 2)

(1) | Torque Converter Assembly (Model Dependent)
(2) | Bolt, Pump to Case
(3) | O-Ring, Pump to Case Bolt
(4) | Pump Assembly, Oil
(5) | Seal, Oil (Pump to Case)
(6) | Gasket, Pump Cover to Case
(7) | Bushing, Case
(9) | Vent Assembly, Transmission
(10) | Connector, Oil Cooler Pipe (Model Dependent)
(11) | Plug, Case Servo
(12) | Spring, Servo Return
(13) | Pin, 2nd Apply Piston
(14) | Ring, Retainer (2nd Apply Piston)
(15) | Retainer, Servo Cushion Spring
(16) | Spring, Servo Cushion (Outer)
(17) | Piston, 2nd Apply
(18) | Ring, Oil Seal (2nd Apply Piston - Outer)
(19) | Ring, Oil Seal (2nd Apply Piston - Inner)
(20) | Housing, Servo Piston (Inner)
(21) | Seal, O-Ring
(22) | Spring, Servo Apply Pin
(23) | Washer, Servo Apply Pin
(24) | Ring, Retainer (Apply Pin)
(25) | Piston, 4th Apply
(26) | Ring, Oil Seal (4th Apply Piston - Outer)
(27) | Seal, O-Ring (2-4 Servo Cover)
(28) | Cover, 2-4 Servo
(29) | Ring, Servo Cover Retaining
(30) | Seal, Case Extension to Case
(31) | Extension, Case (Model Dependent)
(32) | Bolt, Case Extension to Case
(33) | Bushing, Case Extension
(34) | Seal Assembly, Case Extension Oil (Model Dependent)
(34) | Seal Assembly, Case Extension Oil (Model Dependent)
(35) | Bolt, Speed Sensor Retaining
(36) | Speed Sensor, Internal Transmission
(37) | Seal, O-Ring (ITSS to Case Extension)
(71) | Seal, Filter
(72) | Filter Assembly, Transmission Oil (Model Dependent)
(73) | Gasket, Transmission Oil Pan
(73) | Gasket, Transmission Oil Pan
(74) | Magnet, Chip Collector
(75) | Pan, Transmission Oil (Model Dependent)
(75) | Pan, Transmission Oil
(76) | Screw, Transmission Oil Pan
(76) | Screw, Transmission Oil Pan
(94) | Bolt, Converter Housing to Case
(95) | Connector, Oil Cooler Quick (Model Dependent)
(96) | Clip, Oil Cooler Quick Connect (Model Dependent)
(97) | Plug, Converter Housing Access Hole (Model Dependent)
(98) | Plate, Converter Bolt Inspection (Model Dependent)
(99) | Plug, Cup D4 Orifice
(100) | Stud, A/Trans. Case (Y-Car Only)
(101) | Plug Asm., A/Trans. Oil Pan
(102) | Housing, Converter (Model Dependent)
(102) | Housing, Converter (Model Dependent)
(103) | Case, Main Section (Model Dependent)
(103) | Case, Main Section
(105) | Spring, Servo Cushion (Inner) (Model Dependent)
(106) | Seal Assembly, Case Oil (Y-Car Only)

Figure 3: |

#### Case and Associated Parts (2 of 2)

(38) | Transmission Case Plug (Accumulator Bleed)
(39) | Pressure Plug
(40) | Third Accumulator (#7) Retainer and Ball Assembly
(41) | Band Anchor Pin
(42) | Retainer and Ball Assembly (Double Orifice) (#10)
(43) | Accumulator Piston Pin
(44) | 3-4 Accumulator Piston
(45) | Oil Seal Ring (3-4 Accumulator Piston)
(46) | 3-4 Accumulator Spring (Model Dependent)
(47) | Spacer Plate to Case Gasket
(48) | Valve Body Spacer Plate
(49) | Shift Solenoids Screen
(50) | Pressure Control Solenoid Screen
(52) | Spacer Plate to Valve Body Gasket
(53) | Spacer Plate Support Plate
(54) | 1-2 Accumulator Spring (Outer)
(55) | Oil Seal Ring (1-2 Accumulator)
(56) | 1-2 Accumulator Piston
(57) | 1-2 Accumulator Cover and Pin Assembly
(58) | Accumulator Cover Bolt
(59) | Accumulator Cover Bolt
(60) | Control Body Valve Assembly
(61) | Checkball (#2, 3, 4, 5, 6, 8, 12)
(62) | Valve Body Bolt
(63) | Manual Detent Spring Assembly
(64) | Manual Detent Spring Bolt
(65) | Wiring Harness Pass-through Connector O-Ring Seal
(66) | Wiring Harness Solenoid Assembly
(67) | O-Ring Seal (Solenoid)
(68) | Hex Washer Head Bolt (Solenoid)
(69) | Transmission Fluid Pressure Manual Valve Position Switch Assembly
(70) | Pressure Switch Assembly Bolt
(77) | Spacer Plate Support Bolt
(91) | Number 1 Checkball
(93) | Dipstick Stop Bracket (Model Dependent)
(103) | Main Section Case (Model Dependent)
(104) | 1-2 Accumulator Spring (Inner)

Figure 4: |

#### Oil Pump Assembly

(200) | Pump Body
(201) | Oil Seal Ring (Slide to Wear Plate)
(202) | O-Ring Seal (Slide Seal Back-Up)
(203) | Pump Slide
(204) | Pivot Pin Spring
(205) | Pivot Slide Pin
(206) | Pump Slide Spring (Outer)
(207) | Pump Slide Spring (Inner)
(208) | Pump Slide Seal Support
(209) | Pump Slide Seal
(210) | Pump Vane Ring
(210) | Pump Vane Ring
(211) | Rotor Guide
(212) | Oil Pump Rotor
(213) | Pump Vane
(214) | Stator Shaft
(215) | Pump Cover
(216) | Pressure Regulator Valve
(217) | Pressure Regulator Valve Spring
(218) | Pressure Regulator Isolator Spring
(219) | Reverse Boost Valve
(220) | Reverse Boost Valve Sleeve
(221) | Oil Pump Reverse Boost Valve Retaining Ring
(222) | Oil Pump Converter Clutch Valve Retaining Ring
(223) | Stop Valve
(224) | Converter Clutch Valve
(225) | Converter Clutch Valve Spring (Inner)
(226) | Converter Clutch Valve Spring (Outer)
(227) | Pressure Relief Bolt Rivet
(228) | Pressure Relief Ball
(229) | Pressure Relief Spring
(230) | Oil Seal Ring (Stator Shaft)
(231) | Oil Pump Cover Screen Seal
(232) | Oil Pump Cover Screen
(233) | Bolt M8 X 1.25 X 40 (Cover to Body)
(234) | Stator Shaft Bushing (Front)
(235) | Oil Pump Cover Plug (FWD Clutch Feed)
(236) | Oil Pump Cover Plug
(236) | Oil Pump Cover Plug
(236) | Oil Pump Cover Plug
(236) | Oil Pump Cover Plug
(236) | Oil Pump Cover Plug
(236) | Oil Pump Cover Plug
(237) | Check Valve Retainer and Ball Assembly
(237) | Check Valve Retainer and Ball Assembly
(238) | Converter Clutch Signal Orifice (Cup Plug)
(240) | Cup Orifice Plug
(241) | Stator Shaft Bushing (Rear)
(242) | Pump Body Bushing
(243) | Oil Seal Assembly
(244) | Front Helix Retainer

Figure 5: |

#### Control Valve Body Assembly (1 of 2)

(350) | Control Valve Body Assembly
(353) | Forward Accumulator Oil Seal
(354) | Forward Accumulator Piston
(355) | Forward Accumulator Pin
(356) | Forward Accumulator Spring
(357) | Forward Abuse Valve
(358) | Forward Abuse Valve Spring
(359) | Bore Plug
(360) | Coiled Spring Pin
(360) | Coiled Spring Pin
(361) | Low Overrun Valve
(362) | Low Overrun Valve Spring
(363) | Forward Accumulator Cover
(364) | Forward Accumulator Cover Bolt
(364a) | Pressure Control Solenoid Retainer Bolt
(365) | 1-2 Shift Valve Spring
(366) | 1-2 Shift Valve
(367a) | 1-2 Shift Solenoid Valve
(367b) | 2-3 Shift Solenoid Valve
(368) | 2-3 Shift Valve
(369) | 2-3 Shuttle Valve
(370) | 1-2 Accumulator Valve Spring
(371) | 1-2 Accumulator Valve
(372) | 1-2 Accumulator Valve Sleeve
(374) | Actuator Feed Limit Valve
(375) | Actuator Feed Limit Valve Spring
(376) | Bore Plug
(377) | Pressure Control Solenoid Valve
(378) | Pressure Control Solenoid Retainer
(395) | Bore Plug and Solenoid Retainer
(395) | Bore Plug and Solenoid Retainer
(395) | Bore Plug and Solenoid Retainer

Figure 6: |

#### Control Valve Body Assembly (2 of 2)

(340) | Manual Valve
(350) | Control Valve Body Assembly
(359) | Bore Plug
(360) | Coiled Spring Pin
(380) | Regulator Apply Valve
(381) | Bore Plug
(381) | Bore Plug
(381) | Bore Plug
(381) | Bore Plug
(382) | 4-3 Sequence Valve Spring
(383) | 4-3 Sequence Valve
(384) | 3-4 Relay Valve
(385) | 3-4 Shift Valve
(386) | 3-4 Shift Valve Spring
(387) | Reverse Abuse Valve
(388) | Reverse Abuse Valve Spring
(389) | 3-2 Downshift Valve
(390) | 3-2 Downshift Valve Spring
(391) | 3-2 Control Valve
(392) | 3-2 Control Valve Spring
(394) | 3-2 Control Solenoid Valve
(395) | Bore Plug and Solenoid Retainer
(395) | Bore Plug and Solenoid Retainer
(395) | Bore Plug and Solenoid Retainer
(395) | Bore Plug and Solenoid Retainer
(395) | Bore Plug and Solenoid Retainer
(395) | Bore Plug Retainer
(396) | TCC PWM Solenoid Valve
(397) | Regulator Apply Spring
(398) | Isolator Valve

Figure 7: |

#### Internal Parts (1 of 2)

(600) | 3-4 Clutch Boost (5) Spring Assembly
(601) | Thrust Washer (Pump to Drum)
(602) | 2-4 Band Assembly
(603) | Reverse Input Clutch Bushing (Front)
(605) | Reverse Input Clutch Housing and Drum Assembly
(606) | Reverse Input Clutch Bushing (Rear)
(607) | Reverse Input Clutch Piston Assembly
(608a) | Reverse Input Clutch Seal (Inner)
(608b) | Reverse Input Clutch Seal (Outer)
(609) | Reverse Input Clutch Spring Assembly
(610) | Reverse Input Clutch Spring Retainer Ring
(611) | Reverse Input Clutch Plate (Belleville)
(612a) | Reverse Input Clutch Turbulator Plate (Steel)
(612b) | Reverse Input Clutch Plate Assembly (Fiber)
(613) | Reverse Input Clutch Backing Plate (Selective)
(614) | Reverse Input Clutch Retaining Ring
(615) | Stator Shaft/Selective Washer Bearing Assembly
(616) | Thrust Washer (Selective)
(617) | Check Valve Retainer and Ball Assembly
(618) | O-Ring Seal - Location Model Dependent
(619) | Oil Seal Ring (Solid)
(620) | Retainer and Checkball Assembly
(620) | Retainer and Checkball Assembly
(621) | Input Housing and Shaft Assembly (Model Dependent)
(622) | O-Ring Input to Forward Clutch Housing Seal
(623) | 3rd and 4th Clutch Piston
(625) | 3rd and 4th Clutch Ring (Apply)
(626) | 3rd and 4th Clutch Spring Assembly
(627) | Forward Clutch Housing Retainer and Ball Assembly
(628) | Forward Clutch Housing
(630) | Forward Clutch Piston
(632) | Overrun Clutch Piston
(633) | Overrun Clutch Ball
(634) | Overrun Clutch Spring Assembly
(635) | Overrun Clutch Spring Retainer Snap Ring
(636) | Input Housing to Output Shaft Seal
(637) | Input Sun Gear Bearing Assembly
(638) | Overrun Clutch Hub Retaining Snap Ring
(639) | Overrun Clutch Hub
(640) | Forward Sprag Clutch Inner Race and Input Sun Gear Assembly
(642) | Forward Sprag Assembly
(643) | Sprag Assembly Retainer Ring
(643) | Sprag Assembly Retainer Ring
(644) | Forward Clutch Race (Outer)
(645a) | Overrun Clutch Plate (Steel)
(645b) | Overrun Clutch Plate Assembly (Fiber)
(646) | Forward Clutch Plate (Apply)
(648) | Forward Clutch Plate (Waved)
(649a) | Forward Clutch Plate (Steel)
(649b) | Forward Clutch Plate Assembly (Fiber)
(650) | Forward Clutch Backing Plate (Selective)
(651) | Forward Clutch Backing Plate Retainer Ring
(652) | 3rd and 4th Clutch Plate (Steel) (2.2L Engine Only)
(653) | 3rd and 4th Clutch Apply Plate (Stepped)
(653) | 3rd and 4th Clutch Apply Plate (Stepped)
(654a) | 3rd and 4th Clutch Plate Assembly (Fiber) (Quantity Model Dependent 5, 6 or 7 plates)
(654a) | 3rd and 4th Clutch Plate Assembly (Fiber) (Quantity Model Dependent 5, 6 or 7 plates)
(654b) | 3rd and 4th Clutch Plate (Steel) (Quantity Model Dependent)
(654b) | 3rd and 4th Clutch Plate (Steel) (Quantity Model Dependent)
(655) | 3rd and 4th Clutch Backing Plate (Selective) (Model Dependent)
(655) | 3rd and 4th Clutch Backing Plate (Selective) (Model Dependent)
(656) | 3rd and 4th Clutch Backing Plate Retainer Ring
(657) | Input Sun Gear Front Bushing
(659) | Input Sun Gear Rear Bushing
(688) | Cup Plug
(698) | Orificed Cup Plug

Figure 8: |

#### Internal Parts (2 of 2)

(661) | Output Shaft to Input Carrier Retainer
(662) | Input Carrier Assembly
(663) | Thrust Bearing Assembly (Input Carrier to Reaction Shaft)
(664) | Input Internal Gear
(665) | Reaction Carrier Shaft Front Bushing
(666) | Reaction Carrier Shaft
(667) | Reaction Carrier Shaft Rear Bushing
(668) | Reaction Shaft/Internal Gear Retainer Ring
(669) | Thrust Washer (Reaction Shaft Shell)
(670) | Reaction Sun Shell
(671) | Reaction Sun Gear Retainer Ring
(672) | Reaction Sun Bushing
(673) | Reaction Sun Gear
(674) | Thrust Washer (Race/Reaction Shell)
(675) | Low and Reverse Roller Clutch Race
(676) | Low and Reverse Support to Case Retainer Ring
(677) | Low and Reverse Roller Assembly Retainer Ring (Cam)
(677) | Low and Reverse Roller Assembly Retainer Ring (Cam)
(678) | Low and Reverse Roller Clutch Assembly
(679) | Low and Reverse Clutch Support Assembly
(680) | Low and Reverse Clutch Support Retainer Spring
(681) | Reaction Carrier Assembly
(682a) | Low and Reverse Clutch Plate (Waved)
(682b) | Spacer Low and Reverse Clutch Plate (Selective)
(682c) | Low and Reverse Clutch Plate Assembly (Fiber)
(682d) | Low and Reverse Clutch Turbulator Plate (Steel)
(683) | Thrust Bearing Assembly (Reaction Carrier/Support)
(684) | Internal Reaction Gear
(685) | Internal Reaction Gear Support
(686) | Reaction Gear/Support Retainer Ring
(687) | Output Shaft
(690) | Output Shaft Sleeve (Model Dependent)
(691) | Output Shaft Seal (Model Dependent)
(692) | Reaction Gear Support to Case Bearing
(693) | Low and Reverse Clutch Retainer Ring
(694) | Low and Reverse Clutch Spring Assembly
(695) | Low and Reverse Clutch Piston
(696a) | Low and Reverse Clutch Seal (Outer)
(696b) | Low and Reverse Clutch Seal (Center)
(696c) | Low and Reverse Clutch Seal (Inner)
(697) | Oil Deflector (High Output Models Only)
(699) | Internal Transmission Speed Sensor Rotor

Figure 9: |

#### Parking Lock and Manual Shift Shaft Assembly

(78) | Steel Cup Plug
(79) | Parking Brake Pawl Shaft
(80) | Parking Pawl Return Spring
(81) | Parking Brake Pawl
(82) | Manual Shaft Seal
(83) | Manual Shaft Retainer
(84) | Manual Shaft (Model Dependent)
(85) | Parking Lock Actuator Assembly
(86) | Parking Lock Bracket
(87) | Parking Lock Bracket (2) Bolt
(88) | Inside Detent Lever
(89) | Manual Valve Link
(90) | Hex Head Nut

Figure 10: |

#### Seals

(3) | Pump to Case Bolt O-Ring
(5) | Oil Seal (Pump to Case)
(18) | Oil Seal Ring (2nd Apply Piston-Outer)
(19) | Oil Seal Ring (2nd Apply Piston-Inner)
(21) | O-Ring Seal
(26) | Oil Seal Ring (4th Apply Piston-Outer)
(27) | O-Ring Seal (2-4 Servo Cover)
(30) | Case Extension to Case Seal
(34) | Case Extension Oil Seal Assembly
(37) | O-Ring Seal (ITSS to Case Extension)
(106) | Case Oil Seal Assembly (Y-Car Only)
(230) | Oil Seal Ring (Stator Shaft)
(243) | Oil Seal Assembly
(608a) | Reverse Input Clutch Seal (Inner)
(608b) | Reverse Input Clutch Seal (Outer)
(618) | O-Ring Seal (Turbine Shaft/Selective Washer)
(619) | Oil Seal Ring (Solid)
(622) | O-Ring Input to Forward Housing Seal
(623) | 3rd and 4th Clutch Piston
(630) | Forward Clutch Piston
(632) | Overrun Clutch Piston
(636) | Input Housing to Output Shaft Seal
(691) | Output Shaft (Model Dependent) Seal
(696a) | Low and Reverse Clutch (Outer) Seal
(696b) | Low and Reverse Clutch (Center) Seal
(696c) | Low and Reverse Clutch (Inner) Seal

Figure 11: |

#### Bearings and Bushings

(7) | Case Bushing
(33) | Case Extension Bushing
(234) | Stator Shaft Bushing (Front)
(241) | Stator Shaft Bushing (Rear)
(242) | Oil Pump Body Bushing
(601) | Thrust Washer (Pump to Drum)
(603) | Reverse Input Cl. Bushing (Front)
(606) | Reverse Input Clutch Bushing (Rear)
(615) | Stator Shaft/Selective Washer Bearing Assembly
(616) | Thrust Washer (Selective)
(637) | Input Sun Gear Bearing Assembly
(657) | Input Sun Gear Bushing (Front)
(659) | Input Sun Gear Bushing (Rear)
(663) | Thrust Bearing Assembly (Input Carrier to Reaction Shaft)
(665) | Reaction Carrier Shaft Bushing (Front)
(667) | Reaction Carrier Shaft Bushing (Rear)
(669) | Thrust Washer (Reaction Shaft/Shell)
(672) | Reaction Gear Bushing
(674) | Thrust Washer (Race/Reaction Shell)
(683) | Thrust Bearing Assembly (Reaction Carrier/Support)
(692) | Reaction Gear Support to Case Bearing

Figure 12: |

#### Torque Converter Housing Identification

(1) | Domestic Large Bell V-8 (Y-Car)
(2) | Domestic Gen lll Large Bell V-8 (300 mm)
(3) | Domestic Gen l/ll Large Bell V-8/V-6
(4) | Holden Small Bell V-6
(5) | Holden Gen lll Large Bell V-8
(6) | Domestic Small Bell V-6

Figure 13: |

#### Case Extension Identification

(1) | Case Extension - used on C-Truck, G-Van, M-Van, S-Truck
(2) | Case Extension - Some Models

Figure 14: |

#### Valve Trains

(340) | Manual Valve
(353) | Forward Accumulator Oil Seal
(354) | Forward Accumulator Piston
(355) | Forward Accumulator Pin
(356) | Forward Accumulator Spring
(357) | Forward Abuse Valve
(358) | Forward Abuse Valve Spring
(359) | Bore Plug
(359) | Bore Plug
(360) | Coiled Spring Pin
(360) | Coiled Spring Pin
(360) | Coiled Spring Pin
(361) | Low Overrun Valve
(362) | Low Overrun Valve Spring
(363) | Forward Accumulator Cover
(364) | Forward Accumulator Cover Bolt
(364) | Forward Accumulator Cover Bolt
(365) | 1-2 Shift Valve Spring
(366) | 1-2 Shift Valve
(367a) | 1-2 Shift Solenoid Valve
(367b) | 2-3 Shift Solenoid Valve
(368) | 2-3 Shift Valve
(369) | 2-3 Shuttle Valve
(370) | 1-2 Accumulator Valve Spring
(371) | 1-2 Accumulator Valve
(372) | 1-2 Accumulator Valve Sleeve
(374) | Actuator Feed Limit Valve
(375) | Actuator Feed Limit Valve Spring
(376) | Bore Plug
(377) | Pressure Control Solenoid Valve
(378) | Pressure Control Solenoid Retainer
(380) | Regulator Apply Valve
(381) | Bore Plug
(381) | Bore Plug
(381) | Bore Plug
(381) | Bore Plug
(382) | 4-3 Sequence Valve Spring
(383) | 4-3 Sequence Valve
(384) | 3-4 Relay Valve
(385) | 3-4 Shift Valve
(386) | 3-4 Shift Valve Spring
(387) | Reverse Abuse Valve
(388) | Reverse Abuse Valve Spring
(389) | 3-2 Downshift Valve
(390) | 3-2 Downshift Valve Spring
(391) | 3-2 Control Valve
(392) | 3-2 Control Valve Spring
(394) | 3-2 Control Solenoid Valve
(395) | Bore Plug and Solenoid Retainer
(395) | Bore Plug and Solenoid Retainer
(395) | Bore Plug and Solenoid Retainer
(395) | Bore Plug and Solenoid Retainer
(395) | Bore Plug and Solenoid Retainer
(395) | Bore Plug and Solenoid Retainer
(395) | Bore Plug and Solenoid Retainer
(395) | Bore Plug and Solenoid Retainer
(395) | Bore Plug and Solenoid Retainer
(396) | TCC PWM Solenoid Valve
(397) | Regulator Apply Spring
(398) | Isolator Valve

Figure 15: |

#### Pump Body Fluid Passages (Pump Cover Side)

(1) | Suction (intake)
(2) | Decrease
(2) | Decrease
(3) | Line
(3) | Line
(3) | Line
(4) | Converter Feed
(4) | Converter Feed
(4) | Converter Feed
(5) | Release
(7) | To Cooler
(8) | Lube from Cooler
(11) | Torque Signal
(16) | Reverse Input
(16) | Reverse Input
(29) | 3-4 Clutch
(37) | Overrun Clutch
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(45) | Vent
(46) | Seal Drain
(47) | Void
(47) | Void
(48) | Regulated Apply

Figure 16: |

#### Pump Cover Fluid Passages (Pump Body Side)

(1) | Suction (intake)
(1) | Suction (intake)
(2) | Decrease
(2) | Decrease
(2) | Decrease
(2) | Decrease
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(4) | Converter Feed
(4) | Converter Feed
(4) | Converter Feed
(4) | Converter Feed
(5) | Release
(5) | Release
(6) | Apply
(7) | To Cooler
(8) | Lube from Cooler
(8) | Lube from Cooler
(11) | Torque Signal
(16) | Reverse Input
(16) | Reverse Input
(16) | Reverse Input
(16) | Reverse Input
(18) | Forward Clutch Feed
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(37) | Overrun Clutch
(37) | Overrun Clutch
(37) | Overrun Clutch
(37) | Overrun Clutch
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(45) | Vent
(46) | Seal Drain
(47) | Void
(47) | Void
(47) | Void
(48) | Regulated Apply
(48) | Regulated Apply
(232) | Oil Pump Cover Screen
(237) | Check Valve Retainer and Ball Assembly
(237) | Check Valve Retainer and Ball Assembly
(238) | Converter Clutch Signal Orificed Cup Plug
(240) | Orificed Cup Plug

Figure 17: |

#### Pump Cover Fluid Passages (Case Side)

(1) | Suction (Intake)
(2) | Decrease
(2) | Decrease
(3) | Line
(3) | Line
(3) | Line
(5) | Release
(7) | To Cooler
(8) | Lube from Cooler
(8) | Lube from Cooler
(11) | Torque Signal
(16) | Reverse Input (Rev. Clutch
(16) | Reverse Input (Rev. Clutch
(16) | Reverse Input (Rev. Clutch
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(37) | Overrun Clutch
(37) | Overrun Clutch
(37) | Overrun Clutch
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(45) | Vent
(46) | Seal Drain
(47) | Void
(47) | Void
(48) | Regulated Apply
(232) | Oil Pump Cover Screen
(237) | Check Valve Retainer and Ball Assembly
(237) | Check Valve Retainer and Ball Assembly
(240) | Orificed Cup Plug
(240) | Orificed Cup Plug

Figure 18: |

#### Case Fluid Passages (Pump Cover Side)

(3) | Line
(3) | Line
(3) | Line
(7) | To Cooler
(7) | To Cooler
(8) | Lube from Cooler
(8) | Lube from Cooler
(10) | Oil Cooler Pipe Connector
(10) | Oil Cooler Pipe Connector
(11) | Torque Signal
(11) | Torque Signal
(16) | Reverse Input
(16) | Reverse Input
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(37) | Overrun Clutch
(37) | Overrun Clutch
(39) | Pressure Plug
(45) | Vent
(48) | Regulated Apply
(48) | Regulated Apply

Figure 19: |

#### Case Fluid Passages (Control Valve Body Side)

(#1) | Checkball (91)
(#7) | 3rd Accumulator Retainer and Ball Assembly (40)
(#10) | Checkball (42)
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(10) | Filtered Actuator Feed
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(13) | D4-3-2
(13) | D4-3-2
(14) | Lo/Reverse
(14) | Lo/Reverse
(14) | Lo/Reverse
(15) | Reverse
(16) | Reverse Input (Rev. Clutch
(16) | Reverse Input (Rev. Clutch
(16) | Reverse Input (Rev. Clutch
(16) | Reverse Input (Rev. Clutch
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(19) | Rear Lube
(20) | Accumulator
(21) | Orificed Accumulator
(22) | Signal A
(22) | Signal A
(22) | Signal A
(24) | 2nd
(24) | 2nd
(24) | 2nd
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(26) | C.C. Signal
(26) | C.C. Signal
(27) | 3-4 Signal
(27) | 3-4 Signal
(28) | 3rd Accumulator
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(30) | 4th Signal
(31) | Servo Feed
(32) | 4th
(32) | 4th
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(35) | Overrun
(35) | Overrun
(36) | Overrun Clutch Feed
(36) | Overrun Clutch Feed
(37) | Overrun Clutch
(37) | Overrun Clutch
(37) | Overrun Clutch
(38) | D2
(38) | D2
(38) | D2
(38) | D2
(39) | Orificed D2
(41) | Lo
(41) | Lo
(41) | Lo
(42) | Lo/1st
(42) | Lo/1st
(43) | Exhaust
(43) | Exhaust
(44) | Orificed Exhaust
(44) | Orificed Exhaust
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(48) | Regulated Apply
(48) | Regulated Apply

Figure 20: |

#### Spacer Plate to Case Gasket

(3) | Line
(3) | Line
(3) | Line
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(13) | D4-3-2
(13) | D4-3-2
(14) | Lo/Reverse
(14) | Lo/Reverse
(14) | Lo/Reverse
(15) | Reverse
(15) | Reverse
(16) | Reverse Input (Rev. Cl.)
(16) | Reverse Input (Rev. Cl.)
(16) | Reverse Input (Rev. Cl.)
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(20) | Accumulator
(20) | Accumulator
(20) | Accumulator
(20) | Accumulator
(21) | Orificed Accumulator
(21) | Orificed Accumulator
(22) | Signal A
(22) | Signal A
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(26) | C.C. Signal
(26) | C.C. Signal
(26) | C.C. Signal
(27) | 3-4 Signal
(27) | 3-4 Signal
(27) | 3-4 Signal
(28) | 3rd Accumulator
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(30) | 4th Signal
(30) | 4th Signal
(31) | Servo Feed
(31) | Servo Feed
(31) | Servo Feed
(32) | 4th
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(35) | Overrun
(35) | Overrun
(36) | Overrun Clutch Feed
(36) | Overrun Clutch Feed
(37) | Overrun Clutch
(38) | D2
(38) | D2
(38) | D2
(38) | D2
(39) | Orificed D2
(39) | Orificed D2
(41) | Lo
(41) | Lo
(41) | Lo
(41) | Lo
(42) | Lo/1st
(42) | Lo/1st
(43) | Exhaust
(43) | Exhaust
(44) | Orificed Exhaust
(44) | Orificed Exhaust
(47) | Void
(47) | Void
(48) | Regulated Apply
(48) | Regulated Apply

Figure 21: |

#### Spacer Plate Fluid Passages

(3) | Line
(3) | Line
(3) | Line
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9/10) | Actuator Feed Limit/Filtered Actuator Feed
(9/10) | Actuator Feed Limit/Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10/22) | Filtered Actuator Feed/Signal A
(10/23) | Filtered Actuator Feed/Signal B
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(13) | D4-3-2
(13) | D4-3-2
(14) | Lo/Reverse
(14) | Lo/Reverse
(14) | Lo/Reverse
(15) | Reverse
(15) | Reverse
(15/16) | Reverse/Reverse Input (Rev. Clutch
(15/16) | Reverse/Reverse Input (Rev. Clutch
(16) | Reverse Input (Rev. Clutch
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(17/18) | D4
(17/18) | D4
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(20) | Accumulator
(20) | Accumulator
(20) | Accumulator
(20/21) | Accumulator/Orificed Accumulator
(20/21) | Accumulator/Orificed Accumulator
(21) | Orificed Accumulator
(22) | Signal A
(22) | Signal A
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24/25) | 2nd/2nd Clutch
(24/25) | 2nd/2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(26) | C.C. Signal
(26) | C.C. Signal
(27) | 3-4 Signal
(27) | 3-4 Signal
(27/29) | 3-4 Signal
(27/29) | 3-4 Signal
(28) | 3rd Accumulator
(29/28) | 3-4 Clutch/3rd Accumulator
(29/28) | 3-4 Clutch/3rd Accumulator
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(30) | 4th Signal
(30) | 4th Signal
(31) | Servo Feed
(31) | Servo Feed
(31) | Servo Feed
(32) | 4th
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(35a) | Overrun
(35) | Overrun
(35/36) | Overrun/Overrun Clutch Feed
(35/36) | Overrun/Overrun Clutch Feed
(35/39) | Overrun/Orificed D2
(36) | Overrun Clutch Feed
(37) | Overrun Clutch
(38) | D2
(38) | D2
(38) | D2
(38) | D2
(38/39) | D2/Orificed D2
(41) | Lo
(41) | Lo
(41) | Lo
(41) | Lo
(42) | Lo/1st
(42) | Lo/1st
(43) | Exhaust
(43/44) | Exhaust/Orificed Exhaust
(43/44) | Exhaust/Orificed Exhaust
(44) | Orificed Exhaust
(47) | Void
(48) | Regulated Apply
(48) | Regulated Apply
(49) | Shift Solenoids Screen
(50) | Pressure Control Solenoid Screen

Figure 22: |

#### Spacer Plate to Control Valve Body Gasket

(3) | Line
(3) | Line
(3) | Line
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(12) | PR
(13) | D4-3-2
(13) | D4-3-2
(14) | Lo/Reverse
(14) | Lo/Reverse
(14) | Lo/Reverse
(15) | Reverse
(15) | Reverse
(15) | Reverse
(16) | Reverse Input (Rev. Cl.)
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(20) | Accumulator
(20) | Accumulator
(20) | Accumulator
(21) | Orificed Accumulator
(22) | Signal A
(22) | Signal A
(22) | Signal A
(23) | Signal B
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(26) | C.C. Signal
(26) | C.C. Signal
(27) | 3-4 Signal
(27) | 3-4 Signal
(28) | 3rd Accumulator
(28) | 3rd Accumulator
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(30) | 4th Signal
(30) | 4th Signal
(31) | Servo Feed
(31) | Servo Feed
(31) | Servo Feed
(32) | 4th
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(35) | Overrun
(35) | Overrun
(35/39) | Overrun/Orificed D2
(36) | Overrun Clutch Feed
(37) | Overrun Clutch
(38) | D2
(38) | D2
(38) | D2
(38) | D2
(38) | D2
(40) | 3-2 Signal
(40) | 3-2 Signal
(41) | Lo
(41) | Lo
(41) | Lo
(41) | Lo
(42) | Lo/1st
(42) | Lo/1st
(43) | Exhaust
(43) | Exhaust
(44) | Orificed Exhaust
(44) | Orificed Exhaust
(47) | Void
(48) | Regulated Apply
(48) | Regulated Apply

Figure 23: |

#### Control Valve Body Fluid Passages (Case Side)

(#2) | Checkball (61)
(#3) | Checkball (61)
(#4) | Checkball (61)
(#5) | Checkball (61)
(#6) | Checkball (61)
(#8) | Checkball (61)
(#12) | Checkball (61)
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(3) | Line
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(9) | Actuator Feed Limit
(10) | Filtered Actuator Feed
(10) | Filtered Actuator Feed
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(11) | Torque Signal
(12) | PR
(12) | PR
(12) | PR
(13) | D4-3-2
(13) | D4-3-2
(14) | Lo/Reverse
(14) | Lo/Reverse
(15) | Reverse
(15) | Reverse
(15) | Reverse
(16) | Reverse Input (Rev. Clutch
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(17) | D4
(18) | Forward Clutch Feed
(18) | Forward Clutch Feed
(20) | Accumulator
(20) | Accumulator
(22) | Signal A
(22) | Signal A
(23) | Signal B
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(24) | 2nd
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(26) | C.C. Signal
(26) | C.C. Signal
(27) | 3-4 Signal
(27) | 3-4 Signal
(28) | 3rd Accumulator
(28) | 3rd Accumulator
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(29) | 3-4 Clutch
(30) | 4th Signal
(30) | 4th Signal
(31) | Servo Feed
(31) | Servo Feed
(31) | Servo Feed
(32) | 4th
(33) | 3-4 Accumulator
(33) | 3-4 Accumulator
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(34) | D3
(35) | Overrun
(35) | Overrun
(36) | Overrun Clutch Feed
(37) | Overrun Clutch
(38) | D2
(38) | D2
(38) | D2
(40) | 3-2 Signal
(41) | Lo
(41) | Lo
(41) | Lo
(42) | Lo/1st
(42) | Lo/1st
(42) | Lo/1st
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(43) | Exhaust
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(47) | Void
(48) | Regulated Apply
(48) | Regulated Apply

Figure 24: |

#### 2-4 Servo Fluid Passages

(#7) | 3rd Accumulator Retainer and Ball Assembly (40)
(#7) | 3rd Accumulator Retainer and Ball Assembly (40)
(11) | Case Servo Orificed Plug
(11) | Case Servo Orificed Plug
(25) | 2nd Clutch
(25) | 2nd Clutch
(25) | 2nd Clutch
(28) | 3rd Accumulator
(28) | 3rd Accumulator
(28) | 3rd Accumulator
(32) | 4th
(32) | 4th
(32) | 4th
(32) | 4th
(43) | Exhaust
(43) | Exhaust
(44) | Orificed Exhaust
(44) | Orificed Exhaust

Figure 25: |

#### 1-2 Accumulator Cover Fluid Passages

(20) | Accumulator
(21) | Orificed Accumulator
(25) | 2nd Clutch
(25) | 2nd Clutch