For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Clutch Diode (V6 VIN K) | Sealed in harness, approximately 3 cm (1 in) from the injector 2 breakout | -- | --
A/C Clutch Diode (V8 VIN G) | Sealed in harness, approximately 17 cm (7 in) back from the A/C compressor clutch | -- | --
A/C Compressor Clutch (V6 VIN K) | In the front of the engine, on the lower right side | HVAC Component Views in HVAC | Engine Controls Connector End Views in Engine Controls
A/C Compressor Clutch (V8 VIN G) | In the front of the engine, on the lower right side | -- | Engine Controls Connector End Views in Engine Controls
A/C Compressor Relay | In the underhood electrical center 2 | HVAC Component Views in HVAC | --
A/C Refrigerant Pressure Sensor (V6 VIN K) | Above right front wheelhouse, attached to the refrigerant line | -- | Engine Controls Connector End Views in Engine Controls
A/C Refrigerant Pressure Sensor (V8 VIN G) | Above right front wheelhouse, attached to the refrigerant line | -- | Engine Controls Connector End Views in Engine Controls
Accelerator Control and Adjuster | In engine compartment, forward of the right front wheelhouse | -- | Antilock Brake System Connector End Views in Antilock Brake System
Accelerator Control and Cruse Control Servo Cable Adjuster Module (Traction Control Module) | Under the left side of dash, near the kick panel | -- | --
Air Pump Relay | In the underhood electrical center 2 | -- | --
Air Solenoid Relay | In the underhood electrical center 2 | -- | --
Amplifier | Mounted behind the right rear quarter inner trim panel | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
Ashtray Lamp (Auto Trans) | In the lighting tube from the PRNDL lamp | -- | --
Ashtray Lamp (Manual Trans) | Rearward of the shifter, in the ashtray | Harness Routing Views | --
Automatic Transmission | Behind the engine | Automatic Transmission Electronic Component Views in Automatic Transmission | Automatic Transmission Inline Harness Connector End View in Automatic Transmission
Auxiliary Power Socket | On the lower right side of the front of the console | Harness Routing Views | --
Backup Lamp, LH | Mounted in the taillamp assembly | Lighting Systems Component Views in Lighting Systems | Lighting Systems Component Views in Lighting Systems
Backup Lamp, RH | Mounted in the taillamp assembly | Lighting Systems Component Views in Lighting Systems | --
Backup Lamp Switch (M49) (V6 VIN K) | In the middle of the manual transmission, on the left side | Lighting Systems Component Views in Lighting Systems | --
Backup Lamp Switch (MM6) (V8 VIN G) | In the middle of the manual transmission, on the right side | Lighting Systems Component Views in Lighting Systems |
Battery | In the right front of the engine compartment | Power and Grounding Component Views | --
Blower Motor | Under the lower right side of the instrument panel, mounted in the HVAC module | Body Control System Component Views in Body Control System | --
Blower Motor Relay | Under the instrument panel, above the floor tunnel, attached to the inflatable restraint instrument panel module bracket | Theft Deterrent System Component Views in Theft Deterrent | --
Blower Resistor | In HVAC module, forward and left of temperature control cable attachment | -- | --
Body Control Module (BCM) | Under the right side of the instrument panel near the blower motor | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Brake Fluid Level Indicator Sensor | Part of the master cylinder | -- | --
Brake Malfunction Indicator Lamp Driver Module | Behind the center of the instrument panel near the HVAC control | HVAC Component Views in HVAC | Antilock Brake System Connector End Views in Antilock Brake System
Brake Pressure Modulator Valve (BPMV) | Mounted to the left front frame rail | Harness Routing Views | --
Brake Transmission Shift Interlock (BTSI) Diode | In instrument panel harness, main branch, approximately 6 cm from body control module (BCM) breakout | -- | --
Brake Transmission Shift Interlock (BTSI) Solenoid | In console, forward of shift control lever | Tilt Wheel/Column Component Views in Steering Wheel and Column-Tilt | Tilt Wheel/Column Connector End Views in Steering Wheel and Column-Tilt
Camshaft Position (CMP) Sensor (V6 VIN K) | Mounted in engine front cover | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Camshaft Position (CMP) Sensor (V8 VIN G) | Mounted in engine front cover | -- | Engine Controls Connector End Views in Engine Controls
Center High Mounted Stop Lamp (CHMSL) | In the rear center of the spoiler | -- | --
Cigar Lighter | Mounted on the front of the console | Harness Routing Views | --
Clutch Pedal Position (CPP) Switch | Mounted to the clutch pedal bracket | -- | Engine Electrical Connector End Views in Engine Electrical
Courtesy Lamp, Left Rear (Convertible) | Mounted in the left sail panel | -- | --
Courtesy Lamp, Rear Compartment (Convertible) | In the center of the rear compartment, near the rear compartment lid release actuator | Power Roof Systems Component Views in Roof | --
Courtesy Lamp, Right Rear (Convertible) | Mounted in the right sail panel | -- | --
Crankshaft Position Sensor (V6 VIN K) | Lower front of engine | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Crankshaft Position Sensor (V8 VIN G) | Lower front of engine | -- | Engine Controls Connector End Views in Engine Controls
Cruise Control/Clutch Anticipate (V6 VIN K Manual with K34) | Mounted in the clutch pedal bracket | Cruise Control Component Views in Cruise Control | --
Cruise Control (Clutch) Switch (V8 VIN G Manual with K34) | Mounted in the clutch pedal bracket | -- | --
Cruise Control Module | Mounted to the left frame rail, forward of the wheelhouse | Cruise Control Component Views in Cruise Control | Cruise Control Connector End Views in Cruise Control
Cruise Control Release Switch (Brake) (all with K34) | Mounted in the upper hole of the brake pedal bracket | Cruise Control Component Views in Cruise Control | --
Data Link Connector (DLC) | Under the instrument panel, right of the steering column | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Power and Grounding Connector End Views
Daytime Running Lamps (DRL) Ambient Light Sensor | Mounted in top of instrument panel, near defrost grill | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | --
Daytime Running Lamps (DRL) Module (Headlamp Auto Control Module) | Mounted behind the radio and the HVAC control, left of the instrument panel compartment | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Lighting Systems Connector End Views in Lighting Systems
Dome Lamp (Coupe) | On the roof, near the hatch | Harness Routing Views | --
Door Illumination Lamp | Mounted in left and right door trim panel, above armrest switches
Door Jamb Switch, LH | Near base of left A-pillar | Harness Routing Views | --
Door Jamb Switch, RH | Near base of right A-pillar | Harness Routing Views | --
Door Lock Switch | Mounted in the door armrest | Power Door Systems Component Views in Doors | --
Driver Power Seat Actuator Assembly (AG1 Power Seat) | Under driver seat | -- | --
Drivers Seat Adjuster Actuator-Forward/Back (AG1 Power Seat) | Under driver seat | Power Seat Component Views in Seats | --
Drivers Seat Adjuster Actuator Motor-Front Height Motor (AG1 Power Seat) | Under driver seat | Power Seat Component Views in Seats | --
Drivers Seat Adjuster Actuator-Rear Height Motor (AG1) | Under driver seat | Power Seat Component Views in Seats | --
Electronic Brake Control Module (EBCM) | Mounted with brake pressure modulator valve on the top of the left front frame rail | -- | Antilock Brake System Connector End Views in Antilock Brake System
Electronic Ignition Control Module (ICM) (V6 VIN K) | On the top front left side of the engine | -- | --
Electronic Ignition Control Module (ICM) Left (V8 VIN G) | On the top front left side of the engine | -- | --
Electronic Ignition Control Module (ICM) Right (V8 VIN G) | On the top front right side of the engine | -- | --
Electronic Traction Control Module | Under the left side of the instrument panel, near the kick panel | -- | Antilock Brake System Connector End Views in Antilock Brake System
Electronic Traction Control Switch (Chevrolet) | In the center of the instrument panel, above the HVAC control | -- | --
Electronic Traction Control Switch (Pontiac) | On the left side of the upper console | -- | --
Electronic Turn Signal Lamp Flasher (Export) | Below the center of the A/C duct, mounted to the SIR bracket | -- | --
Engine Coolant Fans | Behind the radiator |  | Cooling System Connector End Views in Engine Cooling
Engine Coolant Fan Relays | In the underhood electrical center 1 | -- | --
Engine Coolant Level Indicator Module (V8 VIN G) | Mounted on the upper right side of the radiator | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | --
Engine Coolant Temperature (ECT) Sensor (V6 VIN K) | Under throttle body, front side of engine | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Engine Coolant Temperature (ECT) Sensor (V8 VIN G) | Lower left side of engine, above generator | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Engine Oil Level Switch (V6 VIN K) | On the lower left side of the engine, in the oil pan | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Engine Oil Level Switch (V8 VIN G) | On the lower right side of the engine, in the oil pan | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Engine Oil Pressure Sensor (V6 VIN K) | On the top right side of the engine | -- | --
Engine Oil Pressure Sensor (V8 VIN G) | On the top rear of the engine, near the left cylinder head | Harness Routing Views | --
Evaporative Emission (EVAP) Canister Purge Solenoid Valve (V6 VIN K) | On the right side of the engine next to injector 2 | Engine Controls Component Views in Engine Controls | --
Evaporative Emission (EVAP) Canister Purge Solenoid Valve (V8 VIN G) | On the right center of the engine, mounted to the manifold | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Evaporative Emission (EVAP) Canister Vent Solenoid Valve (V6 VIN K) | On the top right side of the engine, part of the EVAP canister | -- | Engine Controls Connector End Views in Engine Controls
Evaporative Emission (EVAP) Canister Vent Solenoid Valve (V8 VIN G) | On the top right side of the engine, part of the EVAP canister | -- | Engine Controls Connector End Views in Engine Controls
Exhaust Gas Recirculation (EGR) Valve (V6 VIN K) | Front left side of engine, in front of ignition control module | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Exhaust Gas Recirculation (EGR) Valve (V8 VIN G) | Left rear of engine, mounted to intake manifold | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Fog Lamp, Left Front | On the lower left side of the front fascia | -- | --
Fog Lamp, Right Front | Lower right side of front fascia | -- | --
Fog Lamp Relay | In underhood electrical center 1 | -- | --
Fog Lamp Switch (Chevrolet) | In the center of the instrument panel, above the HVAC control | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Fog Lamp Switch (Pontiac) | On the left steering column, below the headlamp switch | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Folding Top Pump (with Motor) | Left side of the rear compartment, behind the carpeting | -- | --
Folding Top Relay | Behind the instrument panel, mounted to the right side of the inflatable restraint instrument panel module bracket | Theft Deterrent System Component Views in Theft Deterrent | --
Folding Top Switch | On the left side of the upper console | Power Roof Systems Connector End Views in Roof | --
Front Side Door Lock | Inside the rear of the door | Power Door Systems Component Views in Doors | --
Front Side Door Lock Actuator | Inside the rear of the door | Power Door Systems Component Views in Doors | --
Front Side Door Window Regulator Motor | Inside front door | Power Door Systems Component Views in Doors | --
Fuel Injectors (V6 VIN K) | Mounted on the intake manifold, part of the fuel rail | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Fuel Injectors (V8 VIN G) | Mounted on the intake manifold, part of the fuel rail | -- | Engine Controls Connector End Views in Engine Controls
Fuel Pump Relay | In the underhood electrical center 2 | -- | --
Fuel Tank Unit | Under the rear of the vehicle | -- | Engine Controls Connector End Views in Engine Controls
Fusible Links | Forward of the left front wheelhouse, behind the underhood electrical center 2 | -- | --
Generator (V6 VIN K) | On the front right side of the engine | Engine Controls Component Views in Engine Controls | Engine Electrical Connector End Views in Engine Electrical
Generator (V8 VIN G) | On the front left side of the engine | Engine Controls Component Views in Engine Controls | Engine Electrical Connector End Views in Engine Electrical
Hazard Lamp Flasher | Left of the steering column, mounted to the instrument panel carrier | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | --
Headlamp (Pontiac) | On the front of the vehicle | -- | --
Headlamp Dimmer Switch | Part of steering column, activated by multifunction lever | Harness Routing Views | --
Headlamp Door Motor | In the front of the vehicle, near each headlamp door | -- | --
Headlamp, High Beam (Chevrolet) | On the front of the vehicle | -- | --
Headlamp Leveling Switch (Export) | On the left side of the upper console | -- | --
Headlamp, Low Beam (Chevrolet) | On the front of the vehicle | Power and Grounding Component Views in Power and Grounding | --
Headlamp Opening Door Actuator Control Module | On the front left side of the engine compartment, beside the underhood electrical center 2 | Power and Grounding Component Views in Power and Grounding | Lighting Systems Connector End Views in Lighting Systems
Headlamp Switch | On the left side of the instrument panel | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Lighting Systems Connector End Views in Lighting Systems
Headlamp, High Beam (Chevrolet) | On the front of the vehicle | -- | --
Heated Oxygen Sensor Bank 1, Sensor 1 (V6 VIN K) | Mounted in the left exhaust manifold | -- | Engine Controls Connector End Views in Engine Controls
Heated Oxygen Sensor Bank 1, Sensor 1 (V8 VIN G) | Mounted in the left exhaust manifold | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Heated Oxygen Sensor Bank 1, Sensor 2 (V8 VIN G) | At the rear of the left catalytic converter | -- | Engine Controls Connector End Views in Engine Controls
Heated Oxygen Sensor Bank 1, Sensor 3 (V6 VIN K) | At the rear of the catalytic converter | -- | Engine Controls Connector End Views in Engine Controls
Heated Oxygen Sensor Bank 2, Sensor 1 (V6 VIN K) | Mounted in the right exhaust manifold | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Heated Oxygen Sensor Bank 2, Sensor 1 (V8 VIN G) | Mounted in the right exhaust manifold | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Heated Oxygen Sensor Bank 2, Sensor 2 (V8 VIN G) | At the rear of the right catalytic converter | -- | Engine Controls Connector End Views in Engine Controls
Horn | In the front right side of the vehicle, directly below headlamp | Power and Grounding Component Views in Power and Grounding | Horn Connector End Views in Horns
Horn Relay | In the underhood electrical center 1 | -- | --
Horn Switch | In steering wheel | -- | --
HVAC Control | In the center of the instrument panel, above the radio | HVAC Component Views in HVAC | --
HVAC Control Blower Switch | Part of HVAC control | -- | --
HVAC Control Lamp | Part of the HVAC control | -- | --
HVAC Control Selector Switch | Part of the HVAC control | HVAC Component Views in HVAC | HVAC Connector End Views in HVAC
Idle Air Control (IAC) Valve (V6 VIN K) | Right front of intake manifold | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Idle Air Control (IAC) Valve (V8 VIN G) | Right front on throttle body | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Ignition Key Lock Cylinder | Part of steering column | Harness Routing Views | --
Ignition Key Warning Switch | Part of steering column | -- | --
Ignition Switch | Part of the steering column | Harness Routing Views | --
Inflatable Restraint IP Module | Mounted behind right side of the instrument panel | SIR Component Views in SIR | SIR Connector End Views in SIR
Inflatable Restraint Sensing and Diagnostic Module (SDM) | On the floor tunnel, below the rear of the console | SIR Component Views in SIR | SIR Connector End Views in SIR
Inflatable Restraint Steering Wheel Module | Mounted on the steering wheel | -- | --
Inflatable Restraint Steering Wheel Module Coil | On the top of the steering column | SIR Component Views in SIR | --
Inside Rearview Mirror | Mounted to inside center of windshield | -- | --
Instrument Cluster | On the left side of the instrument panel | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Intake Air Temperature (IAT) Sensor (V6 VIN K) | Mounted on air duct, in front of intake manifold | -- | Engine Controls Connector End Views in Engine Controls
Intake Air Temperature (IAT) Sensor (V8 VIN G) | Mounted on air duct, in front of intake manifold | -- | Engine Controls Connector End Views in Engine Controls
IP Compartment Lamp | Inside the top center of the instrument panel compartment | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | --
IP Dimmer Switch | Left of the steering wheel, part of the headlamp switch | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Lighting Systems Connector End Views in Lighting Systems
IP Fuse Block | On the left end of the instrument panel carrier | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | --
Knock Sensor, LH (V6 VIN K) | In bottom left side of engine block | -- | --
Knock Sensor, LH (V8 VIN G) | In bottom left side of engine block | Harness Routing Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Knock Sensor, RH (V6 VIN K) | In bottom right side of engine block | -- | --
Knock Sensor, RH (V8 VIN G) | In bottom right side of engine block | -- | Engine Controls Connector End Views in Engine Controls
License Lamp | In the center of the rear fascia, above the license plate | Lighting Systems Component Views in Lighting Systems | --
Lumbar Inflator Switch, Driver | On the left side of the driver seat | -- | --
Lumbar Inflator Switch, Passenger | On the right side of the passenger seat | -- | --
Manifold Absolute Pressure (MAP) Sensor (V6 VIN K) | Mounted to right side of intake manifold | Engine Controls Component Views in Engine Controls | --
Manifold Absolute Pressure (MAP) Sensor (V8 VIN G) | Mounted to right side of intake manifold | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Manual Transmission (V6 VIN K) | Behind the engine | -- | --
Manual Transmission (V8 VIN G) | Behind the engine | -- | --
Mass Air Flow (MAF) Sensor (V6 VIN K) | Mounted on the air duct, in front of the intake manifold | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Mass Air Flow (MAF) Sensor (V8 VIN G) | Mounted on the air duct, in front of the intake manifold | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Multi Function Lever | On the left arm of the steering column | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | --
Outside Rearview Mirror | Mounted to the left and right front doors | Power Door Systems Component Views in Doors | --
Outside Rearview Mirror Switch | Mounted in the door armrest | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Park Brake Switch | In the console, at the base of the park brake lever | Tilt Wheel/Column Component Views in Steering Wheel and Column - Tilt | --
Park Neutral Position Switch | Under the console, on the base of the shift control lever | Tilt Wheel/Column Component Views in Steering Wheel and Column - Tilt | --
Park/Turn Lamp, Left Front | Exterior, left front | -- | --
Park/Turn Lamp, Right Front | Exterior, right front | Lighting Systems Component Views in Lighting Systems | --
Power Seat Cushion Air Control Module (AQ9) | Under the passenger seat | -- | --
Power Seat Inflator Switch, Driver (AQ9) | On the left side of the driver seat | -- | --
Power Seat Inflator Switch, Passenger (AQ9) | On the right side of the passenger seat | -- | --
Power Seat Switch (AG1) | On the left side of the driver seat | Power Seat Component Views in Seats | --
Powertrain Control Module (PCM) (V6 VIN K) | On the right side of the engine compartment, rear of the wheelhouse | Power and Grounding Component Views | Powertrain Control Module Connector End Views in Engine Controls
Powertrain Control Module (PCM) (V8 VIN G) | On the right side of the engine compartment, rear of the wheelhouse | Power and Grounding Component Views | Powertrain Control Module Connector End Views in Engine Controls
Power Window Control Module | Mounted to the center of the dash mat, above the floor tunnel | Harness Routing Views | --
PRNDL Illumination Lamp | Under the console, left of the shift control lever | Harness Routing Views | --
Pump Assembly (Seat Inflator Pump) | Under passenger seat | -- | --
Radio | In the center of the instrument panel, below the HVAC control | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Entertainment Connector End Views in Entertainment
Radio Power Antenna | Behind the right rear quarter inner trim panel | Entertainment Component Views in Entertainment | --
Rear Compartment Courtesy Lamp Switch | Part of rear compartment lid release actuator | -- | --
Rear Compartment Lid Ajar Indication Switch | Part of the rear compartment lid latch | Body Rear End Component Views in Body Rear End | --
Rear Compartment Lid Release Actuator | In the center of the end panel, in the cargo compartment | Body Rear End Component Views in Body Rear End | Body Rear End Connector End Views in Body Rear End
Rear Compartment Lid Release Relay | Under the left side of the instrument panel, near C200 | Body Rear End Component Views in Body Rear End | --
Rear Compartment Lid Release Switch | In the driver knee bolster, left of the steering column | -- | Body Rear End Connector End Views in Body Rear End
Rear Defogger Grid | Mounted on the rear windshield | Stationary Windows Component Views in Stationary Windows | --
Rear Defogger Switch | Part of the HVAC control | HVAC Component Views in HVAC | Stationary Windows Connector End Views in Stationary Windows
Rear Defogger Timer/Relay | Part of the HVAC control | HVAC Component Views in HVAC | --
Rear Fog Lamps (Export) | On the left and right side of the rear fascia | -- | --
Rear Fog Lamp Relay (Export) | Behind the instrument panel, mounted to the right side of the inflatable restraint instrument panel module bracket | Theft Deterrent System Component Views in Theft Deterrent | --
Rear Fog Lamp Switch (Export) | In the center of the instrument panel, above the HVAC control | -- | --
Rear Turn Lamp | On the left and right rear exterior of the vehicle | -- | --
Remote Compact Disc Player | In the left rear cargo compartment | Entertainment Component Views in Entertainment | Entertainment Connector End Views in Entertainment
Reverse Lockout Solenoid (V8 VIN G Manual) | On the rear left side of the transmission | -- | --
Seat Belt Switch | Part of the driver seat buckle assembly | Harness Routing Views | Audible Warnings Connector End Views
Seat Inflation Valve Solenoid (AQ9) | Under passenger seat | -- | --
Second Gear Start Switch (V6 VIN K) (Chevrolet) | In the center of the instrument panel, above the HVAC control | Lighting Systems Component Views in Lighting Systems | --
Second Gear Start Switch (V6 VIN K) (Pontiac) | On the left side of the upper console | Lighting Systems Component Views in Lighting Systems | --
Secondary Air Injection Bleed Valve Solenoid (V8 VIN G) | Mounted to the right front frame rail | -- | Engine Controls Connector End Views in Engine Controls
Secondary Air Injection Pump (V8 VIN G) | On the front left frame rail, in the engine compartment | -- | Engine Controls Connector End Views in Engine Controls
Security Indicator LED | On the top center of the instrument panel | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | --
Side Marker Lamp, Left Front | On the exterior, left front | Lighting Systems Component Views in Lighting | --
Side Marker Lamp, Left Rear | On the exterior, left rear | Lighting Systems Component Views in Lighting | --
Side Marker Lamp, Right Front | On the exterior, right front | Lighting Systems Component Views in Lighting | --
Side Marker Lamp, Right Rear | On the exterior, right rear | Lighting Systems Component Views in Lighting | --
Side Window Switch | Mounted in the door arm rest | Power Door Systems Component Views in Doors | --
Side Window Switch Illumination Lamp | Behind the door trim panel | Power Door Systems Component Views in Doors | --
Skip Shift Solenoid (V8 VIN G Manual) | On the center left side of the transmission | -- | Engine Controls Connector End Views in Engine Controls
Speaker Assembly, Front (with UZ7) (Chevrolet) | On the lower front door | Power Door Systems Component Views in Doors | --
Speaker, Front (UL0, UM6, UN0 with UQ0 or U62 (Chevrolet), and W51, W52, and W53 (Pontiac) | Lower front door | Power Door Systems Component Views in Doors | --
Speaker, Front Midrange (with W54, W55) (Pontiac) | Lower front door | Power Door Systems Component Views in Doors | --
Speaker, Front Midrange (with W59, W73) (Pontiac Convertible) | Lower front door | Power Door Systems Component Views in Doors | --
Speaker, Front Tweeter (with W54, W55) (Pontiac) | Lower front door | Power Door Systems Component Views in Doors | --
Speaker, Front Tweeter (with W59, W73) (Pontiac Convertible) | Lower front door | Power Door Systems Component Views in Doors | --
Speaker, Rear (UL0, UM6, UN0 with UQ0 or U62 (Chevrolet), and W51, W52, and W53) (Pontiac) | Mounted in sail panel | Entertainment Component Views in Entertainment | --
Speaker, Rear Coaxial (with W59, W73) (Pontiac Convertible) | Mounted in sail panel | Entertainment Component Views in Entertainment | --
Speaker, Rear Extended Range (with UZ7) (Chevrolet) | Mounted in rear quarter inner trim panel | Entertainment Component Views in Entertainment | --
Speaker, Rear Midrange (with W54, W55) (Pontiac) | Mounted in rear quarter inner trim panel | Entertainment Component Views in Entertainment | --
Speaker, Rear Subwoofer (with UZ7) (Chevrolet) | Mounted in sail panel | Entertainment Component Views in Entertainment | --
Speaker, Rear Tweeter (with W54, W55) (Pontiac) | Mounted in rear quarter inner trim panel | Entertainment Component Views in Entertainment | --
Star Connector | Under the left side of the instrument panel, near the DLC | -- | --
Starter Motor | On the bottom right side of the engine | Engine Controls Component Views in Engine Controls | --
Starter Motor (V6 VIN K) | On the bottom left side of the engine | Engine Controls Component Views in Engine Controls | --
Starter Relay | In the underhood electrical center 2 | -- | --
Starter Solenoid | On the bottom right side of the engine, above the starter motor | Engine Controls Component Views in Engine Controls | --
Steering Wheel | On the left side of the instrument panel | -- | --
Steering Wheel Controls | On the steering wheel | Entertainment Component Views in Entertainment | --
Stop Lamp Switch | Mounted on the brake pedal bracket | Cruise Control Component Views in Cruise Control | Antilock Brake System Connector End Views in Antilock Brake System
Stop Lamp/TCC Switch (Automatic) | Mounted on the brake pedal bracket | -- | Lighting Systems Connector End Views in Lighting Systems
Taillamp, LH | On the exterior, left rear of the vehicle | -- | --
Taillamp, RH | On the exterior, right rear of the vehicle | -- | --
Tail/Stop Lamp, LH (Chevrolet) | On the exterior, left rear of the vehicle | -- | --
Tail/Stop Lamp, RH (Chevrolet) | On the exterior, right rear of the vehicle | -- | --
Tail/Stop/Turn Lamp, LH Inboard (Pontiac) | On the exterior, left rear of the vehicle | -- | --
Tail/Stop/Turn Lamp, LH Outboard (Pontiac) | On the exterior, left rear of the vehicle | Lighting Systems Component Views in Lighting Systems | --
Tail/Stop/Turn Lamp, RH Inboard (Pontiac) | On the exterior, right rear of the vehicle | -- | --
Tail/Stop/Turn Lamp, RH Outboard (Pontiac) | On the exterior, right rear of the vehicle | Lighting Systems Component Views in Lighting Systems | --
Theft Deterrent Relay | Under the instrument panel, above the floor tunnel, attached to the inflatable restraint instrument panel module bracket | Theft Deterrent System Component Views in Theft Deterrent | --
Theft Deterrent Shock Sensor | Behind the right quarter inner trim panel, attached to the wheelhouse | Entertainment Component Views in Entertainment | Theft Deterrent System Connector End Views in Theft Deterrent
Throttle Position (TP) Sensor (V6 VIN K) | Mounted to the front of the throttle body | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Throttle Position (TP) Sensor (V8 VIN G) | Mounted to the front of the throttle body | -- | Engine Controls Connector End Views in Engine Controls
Traction Control Switch (Chevrolet) | In the center of the instrument panel, above the HVAC control | Lighting Systems Component Views in Lighting Systems | Antilock Brake System Connector End Views in Antilock Brakes
Traction Control Switch (Pontiac) | On the left side of the upper console | Lighting Systems Component Views in Lighting Systems | Antilock Brake System Connector End Views in Antilock Brakes
Turn/Hazard Switch Assembly | Part of steering column | -- | --
Turn Signal Lamp Flasher | Under the instrument panel, right of the steering column | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | --
Turn Signal Lamp Flasher (Export) | Under the instrument panel, right of the steering column | -- | --
Turn/Stop Lamp, LH (Chevrolet) | On the exterior, left rear of the vehicle | -- | --
Turn/Stop Lamp, RH (Chevrolet) | On the exterior, right rear of the vehicle | -- | --
Underhood Electrical Center 1 | On the Left front corner of the engine compartment | Power and Grounding Component Views | --
Underhood Electrical Center 2 | On the left front corner of the engine compartment | Power and Grounding Component Views | --
Vehicle Speed Sensor (Manual) (V6 VIN K) | Rear left side of transmission | Power and Grounding Component Views | Engine Controls Connector End Views in Engine Controls
Vehicle Speed Sensor (Manual) (V8 VIN G) | Rear left side of transmission | Power and Grounding Component Views | Engine Controls Connector End Views in Engine Controls
Vehicle Speed Sensor (Automatic) (V6 VIN K) | Rear right side of transmission | Power and Grounding Component Views | Engine Controls Connector End Views in Engine Controls
Vehicle Speed Sensor (Automatic) (V8 VIN G) | Rear right side of transmission | Power and Grounding Component Views | Engine Controls Connector End Views in Engine Controls
Wheel Speed Sensor, Left Front | Middle of left front steering knuckle | -- | Antilock Brake System Connector End Views in Antilock Brake System
Wheel Speed Sensor, Left Rear | Mounted to rear backing plate of wheel disc | Harness Routing Views | Antilock Brake System Connector End Views in Antilock Brake System
Wheel Speed Sensor, Rear (without NW9) | Top of rear differential | -- | Antilock Brake System Connector End Views in Antilock Brake System
Wheel Speed Sensor, Right Front | Middle of right front steering knuckle | -- | Antilock Brake System Connector End Views in Antilock Brake System
Wheel Speed Sensor, Right Rear | Mounted to rear backing plate of wheel disc | -- | Antilock Brake System Connector End Views in Antilock Brake System
Windshield Washer Pump | On the front of the vehicle, forward of the top radiator support | Wiper/Washer Component Views in Wipers/Washer System | --
Windshield Wiper Motor | On the rear of the left front wheelhouse, mounted to the dash panel below the left wiper mount | Wiper/Washer Component Views in Wipers/Washer System | Wiper/Washer Connector End Views in Wipers/Washer
Wiper Isolation Diode | Approximately 10 cm (4 in) from C215 breakout, in forward lamp harness | -- | --
Wipers/Washer Switch | In the left side of the steering column, actuated by the multi-function lever | -- | --
C100 (10 cavities) | Engine to forward lamp harness, in the engine compartment, above the right wheelhouse | Harness Routing Views | Inline Harness Connector End Views
C101 (10 cavities) | Engine to forward lamp harness, in the engine compartment, above the right wheelhouse | Harness Routing Views | Inline Harness Connector End Views
C102 (1 cavity) | Engine to forward lamp harness, in the engine compartment, above the right wheelhouse | Harness Routing Views | --
C105 (8 cavities) | Engine to forward lamp harness, in the engine compartment, above the right wheelhouse | Harness Routing Views | Inline Harness Connector End Views
C106 (7 cavities) | Engine to engine jumper harness | -- | --
C107 (7 cavities) | Engine to engine jumper harness | -- | --
C108 (3 cavities) | Engine to camshaft position sensor jumper harness | -- | Inline Harness Connector End Views
C120 (2 cavities) | Forward lamp to wheel speed sensor jumper harness, mounted to left frame rail | -- | Inline Harness Connector End Views
C 130 (2 cavities) | Forward lamp to wheel speed sensor jumper harness, mounted to right frame rail | -- | Inline Harness Connector End Views
C160 (5 cavities) (Pontiac) | Left headlamp to the forward lamp harness, behind the headlamp door bracket | Harness Routing Views | --
C165 (5 cavities) (Pontiac) | Right headlamp to the forward lamp harness, behind the headlamp door bracket | Harness Routing Views | --
C170 (6 cavities) Pontiac (Export) | Left leveling headlamp to forward lamp harness, mounted to body, under left headlamp door | -- | --
C175 (6 cavities) Pontiac (Export) | Right leveling headlamp to forward lamp harness, mounted to body, under right headlamp door | -- | --
C200A (17 cavities) | Forward lamp to instrument panel harness, behind the left kick panel and steering column | Harness Routing Views | Inline Harness Connector End Views
C200B (18 cavities) | Forward lamp to instrument panel harness, between the left kick panel and the steering column | Harness Routing Views | Inline Harness Connector End Views
C200C (13 cavities) | Cross car to instrument panel harness, between the left kick panel and the steering column | Harness Routing Views | Inline Harness Connector End Views
C200D (48 cavities) | Part of the instrument panel harness, between the left kick panel and the steering column | Harness Routing Views | Inline Harness Connector End Views
C205 (8 cavities) Pontiac (Export) | Forward lamp to instrument panel harness , between left kick panel and steering column | -- | --
C206 (4 cavities) Chevrolet (Export) | Forward lamp to instrument panel harness , between left kick panel and steering column | -- | --
C210 (8 cavities) | instrument panel to engine harness, under the right side of the instrument panel, behind the knee bolster | Harness Routing Views | Inline Harness Connector End Views
C211 (8 cavities) | Forward lamp to traction control module jumper harness, under the left side of the instrument panel, near the kick panel | Harness Routing Views | Inline Harness Connector End Views
C212 (10 cavities) | Forward lamp to traction control module jumper harness, under the left side of the instrument panel, near the kick panel | Harness Routing Views | Inline Harness Connector End Views
C215 (11 cavities) | Forward lamp to the steering column harness, near the base of the steering column | Harness Routing Views | --
C216 (11 cavities) | Instrument panel to steering column harness, attached to the base of the steering column | Harness Routing Views |
C217 (4 cavities) | Instrument panel to inflatable restraint steering wheel module coil harness, near the base of the steering column | Harness Routing Views | --
C218 (2 cavities) | SIR harness to inflatable restraint steering wheel module coil, at base of steering wheel column | Harness Routing Views | --
C219 (2 cavities) | SIR harness to inflatable restraint instrument panel module jumper harness, behind instrument panel compartment | Harness Routing Views | --
C220 (10 cavities) | Instrument panel to engine harness, under the right side of the instrument panel, behind the knee bolster | Harness Routing Views | Inline Harness Connector End Views
C230 (10 cavities) | Instrument panel to engine harness, under the right side of the instrument panel, behind the knee bolster | Harness Routing Views | Inline Harness Connector End Views
C240 (8 cavities) | Cross car to instrument panel harness, under the right side of the instrument panel, behind the knee bolster | Harness Routing Views | Inline Harness Connector End Views
C250 (2 cavities) | Forward lamp harness of the cruise control harness, near the brake/clutch pedal bracket | Harness Routing Views | --
C270 (2 cavities) | Instrument panel harness to cruise control harness, near the brake/clutch pedal bracket | Harness Routing Views | --
C300 (6 cavities) (AQ9) | Seat jumper to driver seat harness, under the driver seat assembly | Harness Routing Views | Inline Harness Connector End Views
C305 (6 cavities) (AQ9) | Seat jumper to passenger seat harness, under the passenger seat assembly | Harness Routing Views | Inline Harness Connector End Views
C310 (2 cavities) (w/AG1) | Instrument panel to driver seat harness, rear mounting bolt of the driver seat | Harness Routing Views | Inline Harness Connector End Views
C310 (2 cavities) (w/AQ9) | Instrument panel to seat jumper harness, between the rear mounting bolts of the driver seat | Harness Routing Views | --
C320 (1 cavity) Convertible | Convertible rear defogger jumper to instrument panel harness, under left interior trim molding, above left rear wheelhouse | Harness Routing Views | --
C330 (2 cavities) Coupe | Hatch to instrument panel harness, center of roof near dome lamp | Harness Routing Views | --
C400 (6 cavities) | Instrument panel to rear body harness, left rear cargo compartment, between rear end panel and carpet | Harness Routing Views | Inline Harness Connector End Views
C405A (7 cavities) | Fuel tank harness to the instrument panel harness pass through connector, forward of the rear axle | -- | Inline Harness Connector End Views
C405B (16 cavities) | Instrument panel harness pass through connector, forward of the rear axle | Harness Routing Views | Inline Harness Connector End Views
C405C (4 cavities) | Rear wheel speed sensor jumper to the instrument panel harness pass through connector, forward of the rear axle to the speed sensor (ABS) | Harness Routing Views | Inline Harness Connector End Views
C405D (4 cavities) | Fuel tank harness to the instrument panel harness pass through connector, forward of the rear axle | -- | Inline Harness Connector End Views
C410 (2 cavities) (Export) | Instrument panel to rear body harness in the left side of the rear compartment | -- | --
C420 (2 cavities) (Convertible) (Chevrolet) | Instrument panel to CHMSL jumper harness, left underside of the rear compartment lid | Harness Routing Views | --
C420 (2 cavities) (Convertible) (Pontiac) | Instrument panel to CHMSL jumper harness, center underside of the rear compartment lid | Harness Routing Views | --
C420 (2 cavities) (Coupe) | Hatch to CHMSL jumper harness, left side of the rear compartment lid, between the hatch frame and plastic panel | Harness Routing Views | --
C430 (2 cavities) | Rear body to rear fascia harness, between the rear fascia and the rear panel, on the left side | Harness Routing Views | --
G100 (V6 VIN K) | On the lower right side of the engine, above the A/C compressor | Harness Routing Views | --
G100 (V8 VIN G) | On the lower right side of the engine, above the starter solenoid | Harness Routing Views | --
G101 | In the engine compartment, attached to the front of the left wheelhouse | Harness Routing Views | --
G102 | In the engine compartment, attached to the front of the right wheelhouse | Harness Routing Views | --
G105 | Attached to the top right side of the radiator support | Harness Routing Views | --
G106 | Attached to the top left side of the radiator support | Harness Routing Views | --
G109 | Attached to the left front frame rail, forward of the brake pressure modulator valve bracket | Harness Routing Views | --
G110 (V6 VIN K) | In the front of the engine, bolted to the pulley above the A/C clutch connector | Harness Routing Views | --
G110 (V8 VIN G) | Attached to the rear of the left cylinder head | Harness Routing Views | --
G111 (V6 VIN K) | Attached to the left engine mount | Harness Routing Views | --
G111 (V8 VIN G) | Attached to the lower left side of the engine, behind the generator | Harness Routing Views | --
G112 | Attached to the rear of the left cylinder head | Harness Routing Views | --
G200 | Near the left A-pillar, bolted to the instrument panel mounting stud behind the kick panel | Harness Routing Views | --
G201 | Near the right A-pillar, bolted to the instrument panel mounting stud behind the kick panel | Harness Routing Views | --
G202 | Attached to the floor pan, under the center console, to the rear of the inflatable restraint sensing and diagnostic module (SDM) | Harness Routing Views | --
G305 | Bolted to the left rocker panel at the floor pan bar 3 | Harness Routing Views | --
G310 | Bolted to the roof, left of the dome lamp | Harness Routing Views | --
G320 | Bolted to the roof, to the left of the dome lamp | -- | --
G400 | Bolted to the rear compartment lid release actuator bracket in the rear compartment | Harness Routing Views | --
P100 | Left side in the dash panel, engine to the passenger compartment | Harness Routing Views | --
P110 | Right side in the dash panel, engine to the passenger compartment | -- | --
P300 | In the rear center of the roof, near the dome lamp | Harness Routing Views | --
P400 | In the rear of the cargo compartment, left of the rear compartment lid release actuator | Harness Routing Views | --
P410 | In the center underside of the rear compartment lid | Harness Routing Views | --
P500 | Between the driver door and A-pillar | Harness Routing Views | --
P600 | Between the passenger door and A-pillar | Harness Routing Views | --
S100 (V8 VIN G) (Manual Transmission) | Engine harness, approximately 5 cm (2 in) from the vehicle speed sensor breakout | -- | --
S100 (V8 VIN G) (Automatic Transmission) | Engine harness, approximately 12 cm (5 in) from the automatic transmission breakout | -- | --
S101 (V6 VIN K) | Engine harness, main branch, approximately 11 cm (4 in) from the vehicle speed sensor breakout | -- | --
S102 (V6 VIN K) | In the engine harness, approximately 11 cm (4 in) from G211 breakout | -- | --
S102 (V8 VIN G) | In the engine harness, main branch, approximately 7 cm (3 in) from the engine oil pressure sensor breakout | -- | --
S104 (V6 VIN K) | In the engine harness, approximately 15 cm (6 in) from the powertrain control module (PCM) breakout | -- | --
S104 (V8 VIN G) | Engine harness, approximately 14 cm (6 in) from the powertrain control module (PCM) breakout | -- | --
S105 (V8 VIN G) | Engine harness at A/C refrigerant pressure sensor breakout | -- | --
S106 (V8 VIN G) | In the engine harness, main branch approximately 4 cm (2 in) from the powertrain control module (PCM) breakout | -- | --
S107 (V6 VIN K) | In the engine harness, main branch, approximately 21 cm (8 in) from the powertrain control module (PCM) breakout | -- | --
S107 (V8 VIN G) | In the engine harness, main branch, approximately 7 cm (3 in) from the powertrain control module (PCM) breakout | -- | --
S108 (V6 VIN K) | In the engine harness, main branch, approximately 7 cm (3 in) from the vehicle speed sensor breakout | -- | --
S108 (V8 VIN G) (Automatic Transmission) | In the engine harness, main branch, approximately 5 cm (2 in) from the automatic transmission breakout | -- | --
S108 (V8 VIN G) (Manual Transmission) | In the engine harness, main branch, approximately 12 cm (5 in) from the vehicle speed sensor breakout | -- | --
S109 (V8 VIN G) | In the engine harness, approximately 8 cm (3 in) from the fuel injector 4 breakout | -- | --
S110 (V6 VIN K) | In the engine harness, approximately 4 cm (2 in) from the powertrain control module (PCM) breakout | -- | --
S110 (V8 VIN G) | In the engine harness, main branch, approximately 19 cm (7 in) from the powertrain control module (PCM) breakout | -- | --
S112 | In the forward lamp harness, approximately 9 cm (4 in) from the right lamps breakout | -- | --
S113 | In the forward lamp harness approximately 7 cm (3 in) from the engine coolant fans/cruise control | -- | --
S114 (V6 VIN K) | Engine harness, approximately 3 cm (1 in) from generator breakout | -- | --
S114 (V8 VIN G) | Engine harness, approximately 17 cm (7 in) back from A/C compressor clutch connector | -- | --
S115 (V6 VIN K) | In the engine harness at the generator breakout | -- | --
S115 (V8 VIN G) | In the engine harness, approximately 20 cm (8 in) back from the A/C compressor clutch connector | -- | --
S116 (V8 VIN G) | Engine harness, approximately 9 cm (4 in) from manifold absolute pressure (MAP) sensor breakout | -- | --
S118 (V8 VIN G) | Engine harness, approximately 15 cm (6 in) from manifold absolute pressure (MAP) sensor breakout | -- | --
S119 (V8 VIN G) (Automatic Transmission) | Engine harness, main branch, approximately 8 cm (3 in) from automatic transmission breakout | -- | --
S119 (V8 VIN G) (Manual Transmission) | Engine harness, main branch, approximately 9 cm (4 in) from vehicle speed sensor breakout | -- | --
S120 (V8 VIN G) | Engine harness, main branch, 8 cm (3 in) from powertrain control module (PCM) breakout | -- | --
S121 (V6 VIN K) | Engine harness, main branch, 8 cm (3 in) from powertrain control module (PCM) breakout | -- | --
S122 | Engine jumper harness | -- | --
S123 | Engine jumper harness | -- | --
S124 | Engine jumper harness | -- | --
S125 | Engine jumper harness | -- | --
S126 | Engine jumper harness | -- | --
S127 | Engine jumper harness | -- | --
S150 | Forward lamp harness, approximately 16 cm (6 in) from windshield washer pump breakout | -- | --
S151 | Forward lamp harness, approximately 28 cm (4 in) from C200 | -- | --
S152 | Forward lamp harness, approximately 7 cm (3 in) from C120 (left front wheel speed sensor) breakout | -- | --
S153 | Forward lamp harness, approximately 13 cm (5 in) from C120 (left front wheel speed sensor) breakout | -- | --
S154 | Forward lamp harness, approximately 13 cm (5 in) from C120 (left front wheel speed sensor) breakout | -- | --
S155 | Forward lamp harness, approximately 27 cm (11 in) from engine coolant fans/cruise control module breakout | -- | --
S156 (Export) | Forward lamp harness, approximately 7 cm (3 in) from G106 breakout | -- | --
S157 (Export) | Forward lamp harness, approximately 8 cm (3 in) from G105 breakout | -- | --
S159 | Forward lamp harness, approximately 8 cm (3 in) into secondary air injection bleed valve solenoid breakout | -- | --
S160 | Forward lamp harness, approximately 4 cm (2 in) from the engine coolant fans/cruise control module breakout | -- | --
S161 | Forward lamp harness, main branch, approximately 13 cm (5 in) from G106 breakout | -- | --
S164 | In the forward lamp harness, approximately 13 cm (5 in) from the main branch into the UH electrical center 2 breakout | -- | --
S165 | In the forward lamp harness, approximately 7 cm (3 in) from the main branch into the UH electrical center 2 breakout | -- | --
S166 | Forward lamp harness, approximately 14 cm (6 in) from G105 breakout | -- | --
S167 | Forward lamp harness, approximately 7 cm (3 in) from electronic brake control module (EBCM) breakout | -- | --
S168 | In the forward lamp harness, approximately 8 cm (3 in) from the main branch into the UH electrical center 1 breakout | -- | --
S169 | In the forward lamp harness, approximately 6 cm (2 in) from the main branch into the UH electrical center 1 breakout | -- | --
S170 | In the forward lamp harness, approximately 13 cm (5 in) from G106 breakout | -- | --
S171 | In the forward lamp harness, approximately 10 cm (4 in) from G102 breakout | -- | --
S172 (Export) | Forward lamp harness, approximately 28 cm (11 in) from G105 | -- | --
S177 | In the forward lamp harness, approximately 4 cm (2 in) from the main branch into the UH electrical center 1 breakout | -- | --
S179 | In the forward lamp harness, approximately 25 cm (10 in) from the UH electrical center 1 breakout | -- | --
S181 | In the forward lamp harness, approximately 20 cm (8 in) from the UH electrical center 1 breakout | -- | --
S182 | In the forward lamp harness, approximately 15 cm (6 in) from the UH electrical center 1 breakout | -- | --
S183 | In the forward lamp harness, approximately 10 cm (4 in) from the UH electrical center 1 breakout | -- | --
S184 | In the forward lamp harness, approximately 5 cm (2 in) from the UH electrical center 1 breakout | -- | --
S185 | In the forward lamp harness, at the UH electrical center 1 breakout | -- | --
S202 | Forward lamp harness, approximately 28 cm (11 ) from C200 | -- | --
S203 | In the forward lamp harness, main branch, approximately 4 cm from C211/C212 breakout, toward C200 | -- | --
S204 | Forward lamp harness, main branch, at C211/C212 breakout | -- | --
S205 | Forward lamp harness, main branch, approximately 4 cm (2 in) from C211/C212 breakout, toward P100 | -- | --
S206 | Instrument panel, at rear compartment lid release relay breakout | -- | --
S207 | In the instrument panel harness, main branch, approximately 4 cm (2 in) from the data link connector (DLC) breakout | -- | --
S208 | In the cross car harness, main branch, approximately 26 cm (10 in) from the power window control module breakout | -- | --
S209 | Forward lamp harness, main branch, approximately 11 cm (5 in) from C211/C212 breakout, toward P100 | -- | --
S210 | Forward lamp harness, main branch, approximately 8 cm (3 in) from C211/C212 breakout toward P100 | -- | --
S211 | In the instrument panel harness, main branch, approximately 7 cm (3 in) from the rear compartment lid release relay breakout | -- | --
S214 (Chevrolet) | instrument panel harness, approximately 8 cm (3 in) into instrument cluster breakout | -- | --
S215 | In the instrument panel harness, main branch, approximately 11 cm (4 in) from the antenna cable breakout | -- | --
S216 | In the instrument panel harness, main branch, approximately 10 cm (4 in) from the instrument cluster breakout | -- | --
S217 | In the instrument panel harness, main branch, approximately 18 cm (7 in) from the body control module (BCM) breakout | -- | --
S218 | In the instrument panel harness, approximately 4 cm (2 in) from the instrument cluster breakout | -- | --
S219 | instrument panel harness, main branch, approximately 13 cm (5 in) from rear compartment lid release relay breakout | -- | --
S220 | In the cross car harness, main branch, approximately 9 cm from C200C breakout | -- | --
S222 | instrument panel harness, approximately 6 cm from G202 breakout, in the inflatable restraint sensing and diagnostic module (SDM) branch | -- | --
S224 | In the instrument panel harness, main branch, approximately 17 cm (7 in) from the instrument cluster breakout | -- | --
S225 | Instrument panel harness, approximately 6 cm (2 in) from blower motor breakout | -- | --
S226 | Instrument panel harness, approximately 7 cm (3 in) into headlamp switch breakout | -- | --
S227 | Instrument panel harness, approximately 14 cm (6 in) into headlamp switch breakout | -- | --
S228 | Instrument panel harness, main branch, approximately 20 cm (8 in) from rear compartment lid release relay breakout | -- | --
S232 | In the instrument panel harness, approximately 7 cm (3 in) from the park brake switch breakout | -- | --
S234 (Automatic) | Instrument panel harness, main branch, approximately 5 cm (2 in) from body control module (BCM) breakout | -- | --
S237 (Automatic) | Instrument panel harness, main branch, approximately 6 cm (2 in) from body control module (BCM) breakout | -- | --
S239 (Automatic) | instrument panel harness, main branch, approximately 1 cm (0.5 in) from body control module (BCM) breakout | -- | --
S240 | In the instrument panel harness, main branch, approximately 17 cm (7 in) from the antenna cable breakout | -- | --
S241 | In the instrument panel harness, main branch, approximately 4 cm (2 in) from the antenna cable breakout | -- | --
S242 | In the instrument panel harness, main branch, approximately 4 cm (2 in) from data link connector (DLC) breakout | -- | --
S243 | Instrument panel harness, approximately 9 cm (4 in) from G200 breakout | -- | --
S244 (Convertible) | Instrument panel harness, approximately 46 cm (18 in) from C405 | -- | --
S244 (Coupe) | Instrument panel harness, approximately 40 cm (16 in) back from C405 | -- | --
S245 | Instrument panel harness, approximately 22 cm (9 in) from G200 breakout | -- | --
S246 | In the instrument panel harness, approximately 3 cm (1.2 in) from the antenna cable breakout | -- | --
S247 | Instrument panel harness, approximately 16 cm (6 in) from G200 breakout | -- | --
S248 | In the instrument panel harness, approximately 2 cm (1 in) from the radio connectors breakout | -- | --
S250 (Chevrolet) (Export) | In the instrument panel harness, approximately 29 cm (11 in) from the G200 breakout | -- | --
S251 (Chevrolet) (Export) | instrument panel harness, at instrument panel fuse block breakout | -- | --
S252 (Convertible) | In the instrument panel harness, main branch, approximately 48 cm (19 in) from G200 breakout | -- | --
S252 (Coupe) | In the instrument panel harness, main branch, approximately 33 cm (13 in) from G305 breakout | -- | --
S253 (Convertible) | In the instrument panel harness, main branch, approximately 4 cm (2 in) from the instrument cluster breakout | -- | --
S254 | In the instrument panel harness, approximately 7 cm (3 in) from C200 breakout | -- | --
S255 | In the instrument panel harness, approximately 7 cm (3 in) into the instrument panel fuse block breakout | -- | --
S260 | Cross car harness, main branch, approximately 22 cm (9 in) from the C200C breakout | -- | --
S261 (Pontiac) | Cross car harness, approximately 6 cm (3 in) from body control module (BCM) breakout | -- | --
S263 | Cross car harness, approximately 16 cm (6 in) from the C200C breakout | -- | --
S267 | Cross car harness, main branch, approximately 24 cm (9 in) from inside rearview mirror breakout | -- | --
S268 | Cross car harness, main branch, approximately 18 cm (7 in) from inside rearview mirror breakout | -- | --
S275 | Forward lamp harness, approximately 30 cm (12 in) back from ignition switch connector | -- | --
S276 | Forward lamp harness, approximately 25 cm (10 in) back from ignition switch connector | -- | --
S278 | Forward lamp harness, approximately 7 cm (3 in) into C215 breakout | -- | --
S284 | In the instrument panel harness, approximately 11 cm (4.3 in) fromt he G202 breakout | -- | --
S285 | In the instrument panel harness, approximately 16 cm (6.3 in) from the G202 module | -- | --
S300 (Pontiac Coupe) | Instrument panel harness, main branch, approximately 4 cm (2 in) from theft deterrent shock sensor breakout | -- | --
S301 (Pontiac Coupe) | Instrument panel harness, main branch, approximately 7 cm (3 in) from theft deterrent shock sensor breakout | -- | --
S302 (Pontiac Coupe) | Instrument panel harness, main branch, approximately 13 cm (5 in) from remote compact disc player/left rear speaker breakout | -- | --
S303 (Pontiac) | Instrument panel harness, main branch, approximately 18 cm (7 in) from C220 breakout | -- | --
S303 (Pontiac Convertible) | Instrument panel harness, main branch, approximately 11 cm (4 in) from body control module (BCM) breakout | -- | --
S304 (Pontiac) | Instrument panel harness, main branch, approximately 18 cm (7 in) from body control module (BCM) breakout | -- | --
S304 (Pontiac Convertible) | Instrument panel harness, main branch, approximately 18 cm (7 in) from body control module (BCM) breakout | -- | --
S305 (Pontiac Coupe) | Instrument panel harness, main branch, approximately 7 cm (3 in) from remote compact disc player/left rear speaker breakout | -- | --
S306 (Pontiac) | Instrument panel harness, main branch, approximately 14 cm (6 in) from G201 breakout | -- | --
S307 (Pontiac) | Instrument panel harness, main branch, approximately 7 cm (3 in) from G201 breakout | -- | --
S315 (Coupe) | Instrument panel harness, approximately 19 cm (7 in) back from C330 | -- | --
S317 (Convertible) | Instrument panel harness, main branch, approximately 40 cm (16 in) (from left rear courtesy lamp breakout | -- | --
S320 (AQ9) | In the seat jumper harness, main branch, approximately 7 cm (3 in) from C310 breakout | -- | --
S321 (AQ9) | In the seat jumper harness, main branch, approximately 13 cm (5 in) from C310 breakout | -- | --
S330 (AQ9) | In the driver seat harness, main branch, approximately 5 cm (2 in) from the power seat switch breakout | -- | --
S331 (AQ9) | In the passenger seat harness, approximately 30 cm (12 in) from C305 breakout | -- | --
S333 (Convertible) | In the instrument panel harness, approximately 11 cm (4 in) (4.3 in) from the body control module (BCM) breakout | -- | --
S333 (Coupe) | In the instrument panel harness, main branch, approximately 23 cm (9 in) from the remote compact disc player/left rear speaker breakout | -- | --
S400 (Chevrolet) | Rear body harness, main branch, approximately 20 cm (8 in) from P400 breakout toward right taillamp | -- | --
S400 (Pontiac) | Rear body harness, main branch, approximately 13 cm (5 in) from P400 breakout toward right taillamp | -- | --
S401 (Pontiac) | Rear body harness, between P400 and C400 in breakout, approximately 16 cm (6 in) from P400 | -- | --
S402 (Pontiac) | Rear body harness, between P400 and C400 in breakout, approximately 13 cm (5 in) from P400 | -- | --
S403 (Chevrolet) | Rear body harness, between P400 and C400 in breakout, 11 cm (4 in) from P400 | -- | --
S404 | Rear body harness, main branch, approximately 20 cm (8 in) from the P400 breakout | -- | --
S405 (Chevrolet) | Rear body harness, between P400 and C400 in breakout, approximately 17 cm (7 in) from P400 | -- | --
S405 (Pontiac) | Rear body harness, between P400 and C400 in breakout, approximately 9 cm (4 in from P400 | -- | --
S406 | In the rear body harness, approximately 10 cm (4 in) from the rear compartment lid release actuator | -- | --
S408 (Chevrolet) (Export) | Rear body harness, main branch, approximately 20 cm (8 in) from P400 breakout | -- | --
S410 | In the rear body harness, main branch, approximately 27 cm (11 in) from P400 breakout, toward the right taillamp | -- | --
S415 (Export) | In the cross car harness, approximately 13 cm (5.1 in) from the license lamp breakout | -- | --
S420 | In the hatch harness, main branch, approximately 7 cm (3 in) from P300 breakout | -- | --
S430 | Rear fascia harness, main branch, approximately 12 cm (5 in) from the license lamp breakout | -- | --
S430 (Export) | In the rear fascia harness, approximately 8 cm (3 in) from the main branch, in license lamp breakout | -- | --
S435 (Pontiac) (Export) | Rear fascia harness, main branch, approximately 20 cm (8 in) from license lamp breakout | -- | --
S440 | Rear fascia harness, main branch, approximately 5 cm (2 in) from license lamp breakout | -- | --
S440 (Export) | Rear fascia harness, main branch, approximately 7 cm (3 in from license lamp breakout | -- | --
S450 | CHMSL jumper harness, approximately 24 cm (9 in) from the bulbs | -- | --
S460 | CHMSL jumper harness, approximately 30 cm (12 in) from the bulbs | -- | --
S470 | In the instrument panel harness, approximately 24 cm (9 in) from the rear compartment lid release actuator | -- | --
S501 | Cross car harness, approximately 4 cm (2 in) from left outside rearview mirror breakout | -- | --
S504 | Cross car harness, approximately 11 cm (4 in) from left outside rearview mirror breakout | -- | --
S610 (Chevrolet) | Cross car harness, approximately 7 cm (3 in) from left outside rearview mirror breakout | -- | --