For 1990-2009 cars

# CORE INFORMATION TAG REMANUFACTURED GENERATOR

#### 1986 GENERATOR APPLICATIONS:

Firebird 2.5L Model #1105662 - 1105612 Grand Am 2.5L Model #1105669 - 1105670 Grand Am 3.OL Model #1105671 - 1105672

#### 1987 GENERATOR APPLICATIONS:

6000 2.5L Model #1101142 6000 2.8L Model #1101135 - 1101136 - 1101246 Firebird 2.8L Model #1101139 - 1101140 Firebird 5.OL (CARB) Model #1101137 - 1101138 Firebird 5.OL (PFI) Model #1101141 Firebird 5.7L (PFI) Model #1001141 2000 2.OL Model #1101144 Bonneville 3.8L Model #1101250 Grand Am 2.OL Model #1101144 - 1101145 Grand Am 2.5L Model #1101123 - 1101124 Grand Am 3.OL Model #1101125 - 1101126 Fiero 2.5L Model #1101148

A remanufactured unit is used to replace the new CS-130 generators. Both a remanufactured unit and service parts are available for CS-144.

A core information tag comes with the remanufactured assembly. This tag is to be completed and returned with the defective generator.

It is very important that this tag be filled out completely. With complete information, Delco Remy will be able to quickly identify and correct any problem areas on these new products.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.