For 1990-2009 cars

# SCRATCH/DAMAGED VINYL WINDOWS REPAIR KITS AND PROCEDURES

ALL CONVERTIBLE TOPS WITH CLEAR PLASTIC BACK WINDOWS

Customer comments of scratches or damage to clear plastic rear windows on convertible tops can be repaired with a special compound and buffing operation to remove the damage. The repair kit, Part Number JG-5A, contains an instruction sheet, an abrasive compound, anti-static cream and two buffing cloths for the anti-static material. Each kit contains enough material for 10 to 20 repairs.

The recommended repair kit Micro Surface Products (#JG-5A - Price $15.39) 1217 West Third Street is available from Micro Box 818 Surface Products for orders Wilton, Iowa 52778 over $125.00. #319-732-3240

Individual kits or orders less than $125.00 can be Micro Mesh Specialties placed through Micro Mesh 3714 West 211th Place Specialties and will include Matteson, IL 60443 approximately a $5.00 shipping #312-748-0644 and handling charge per order.

Larger orders can be placed through the Wilton, Iowa location. Suggested Repair Time for this operation is .5 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.